| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Functions | Variables
vmClock.ino File Reference

Go to the source code of this file.

## Functions
static void | setup ()
| Initialize Linduino. More...
static void | loop ()

## Variables
char | demo_name [] = "DC934"
| Demo Board Name stored in QuikEval EEPROM. More...
const uint8_t | address_map [3] = {LTC2607_DAC_A, LTC2607_DAC_B, LTC2607_ALL_DACS}
| Look-up table for DAC_A, DAC_B, or both command byte option. More...
static int8_t | demo_board_connected
| Set to 1 if the board is connected. More...
static uint32_t | startMinutes = 10*60 + 24
static float | MY_LSB = 7.65841584E-5
static float | MY_OFF = 0.0012425743

## Function Documentation

## ◆ loop()

static void loop | ( | void |  | ) |
| static

Definition at line 90 of file vmClock.ino.

## ◆ setup()

static void setup | ( | void |  | ) |
| static

Initialize Linduino.

Definition at line 76 of file vmClock.ino.

## Variable Documentation

## ◆ address_map

const uint8_t address_map[3] = {LTC2607_DAC_A, LTC2607_DAC_B, LTC2607_ALL_DACS}

Look-up table for DAC_A, DAC_B, or both command byte option.

Definition at line 66 of file vmClock.ino.

## ◆ demo_board_connected

int8_t demo_board_connected
| static

Set to 1 if the board is connected.

Definition at line 68 of file vmClock.ino.

## ◆ demo_name

char demo_name[] = "DC934"

Demo Board Name stored in QuikEval EEPROM.

Definition at line 64 of file vmClock.ino.

## ◆ MY_LSB

float MY_LSB = 7.65841584E-5
| static

Definition at line 72 of file vmClock.ino.

## ◆ MY_OFF

float MY_OFF = 0.0012425743
| static

Definition at line 73 of file vmClock.ino.

## ◆ startMinutes

uint32_t startMinutes = 10*60 + 24
| static

Definition at line 70 of file vmClock.ino.