| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Functions
LTC2496.cpp File Reference
Analog-to-Digital Converters (ADC) » LTC2496: 16-Bit 8-/16-Channel Delta Sigma ADC with Easy Drive Input Current Cancellation

Library for LTC2496 LTC2496: 16-Bit 8-/16-Channel Delta Sigma ADC with Easy Drive Input Current Cancellation. More...

## Detailed Description

Library for LTC2496 LTC2496: 16-Bit 8-/16-Channel Delta Sigma ADC with Easy Drive Input Current Cancellation.

Definition in file LTC2496.cpp.

Go to the source code of this file.

## Functions
int8_t | LTC2496_EOC_timeout (uint8_t cs, uint16_t miso_timeout)
| Checks for EOC with a specified timeout. More...
void | LTC2496_read (uint8_t cs, uint8_t adc_command, int32_t *adc_code)
| Read LTC2496 result, program configuration for next conversion. More...
float | LTC2496_code_to_voltage (int32_t adc_code, float vref)
| Calculates the LTC2496 input voltage. More...

## Function Documentation

## ◆ LTC2496_code_to_voltage()

float LTC2496_code_to_voltage | ( | int32_t | adc_code,
|  | float | vref
| ) |  |

Calculates the LTC2496 input voltage.

Returns
  Calculated voltage

Parameters

  adc_code | Raw ADC code
  vref | the reference voltage to the ADC

Definition at line 93 of file LTC2496.cpp.

## ◆ LTC2496_EOC_timeout()

int8_t LTC2496_EOC_timeout | ( | uint8_t | cs,
|  | uint16_t | miso_timeout
| ) |  |

Checks for EOC with a specified timeout.

Returns
  Returns 0=successful, 1=unsuccessful (exceeded timeout)

Parameters

  cs | Chip Select pin
  miso_timeout | Timeout (in millisends)

Definition at line 79 of file LTC2496.cpp.

## ◆ LTC2496_read()

void LTC2496_read | ( | uint8_t | cs,
|  | uint8_t | adc_command,
|  | int32_t * | adc_code
| ) |  |

Read LTC2496 result, program configuration for next conversion.

Returns
  void

Parameters

  cs | Chip Select pin
  adc_command | Command byte
  adc_code | Returns raw 32-bit code read from ADC

Definition at line 86 of file LTC2496.cpp.