| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - i -

- i : DC2430A.ino , DC590B.ino , DC590B_enhanced.ino
- I2C_8ADDR : LT_I2C.h , LT_I2C_Wire.h
- i2c_acread() : LT3965.cpp , LT3965.h
- i2c_acwrite() : LT3965.cpp , LT3965.h
- i2c_address : DC1558_DC1808.ino , DC1976A.ino , DC2423A.ino , Serial_EEPROM_Test.ino , LTM9100.h
- I2C_ADDRESS : LTC2373.h
- i2c_address : DC1444A.ino , DC1337A.ino , DC1716A.ino , DC1012A_B.ino , DC1012AA.ino
- i2c_auxiliary_mode : DC590_subset.ino , DC2430A.ino , DC590B.ino , DC590B_enhanced.ino
- i2c_bcread() : LT3965.cpp , LT3965.h
- I2C_Board0_EEPROM_ADDR0 : MasterAddressConstants.h
- I2C_Board0_LTC2485_Iout_LH_ADDR0 : MasterAddressConstants.h
- I2C_Board0_LTC2485_Iout_LH_Global : MasterAddressConstants.h
- I2C_Board0_LTC2485_Vout_LF_ADDR0 : MasterAddressConstants.h
- I2C_Board0_LTC2485_Vout_LF_Global : MasterAddressConstants.h
- I2C_Board0_LTC2655_LLL_ADDR0 : MasterAddressConstants.h
- I2C_Board0_LTC2655_LLL_Global : MasterAddressConstants.h
- I2C_Board1_EEPROM_ADDR0 : MasterAddressConstants.h
- I2C_Board1_LTC2485_Iout_LH_ADDR0 : MasterAddressConstants.h
- I2C_Board1_LTC2485_Iout_LH_Global : MasterAddressConstants.h
- I2C_Board1_LTC2485_Vout_LF_ADDR0 : MasterAddressConstants.h
- I2C_Board1_LTC2485_Vout_LF_Global : MasterAddressConstants.h
- I2C_Board1_LTC2655_LLL_ADDR0 : MasterAddressConstants.h
- I2C_Board1_LTC2655_LLL_Global : MasterAddressConstants.h
- I2C_Board2_EEPROM_ADDR0 : MasterAddressConstants.h
- I2C_Board2_LTC2485_Iout_LH_ADDR0 : MasterAddressConstants.h
- I2C_Board2_LTC2485_Iout_LH_Global : MasterAddressConstants.h
- I2C_Board2_LTC2485_Vout_LF_ADDR0 : MasterAddressConstants.h
- I2C_Board2_LTC2485_Vout_LF_Global : MasterAddressConstants.h
- I2C_Board2_LTC2655_LLL_ADDR0 : MasterAddressConstants.h
- I2C_Board2_LTC2655_LLL_Global : MasterAddressConstants.h
- I2C_Board3_EEPROM_ADDR0 : MasterAddressConstants.h
- I2C_Board3_LTC2485_Iout_LH_ADDR0 : MasterAddressConstants.h
- I2C_Board3_LTC2485_Iout_LH_Global : MasterAddressConstants.h
- I2C_Board3_LTC2485_Vout_LF_ADDR0 : MasterAddressConstants.h
- I2C_Board3_LTC2485_Vout_LF_Global : MasterAddressConstants.h
- I2C_Board3_LTC2655_LLL_ADDR0 : MasterAddressConstants.h
- I2C_Board3_LTC2655_LLL_Global : MasterAddressConstants.h
- I2C_Board4_EEPROM_ADDR0 : MasterAddressConstants.h
- I2C_Board4_LTC2485_Iout_LH_ADDR0 : MasterAddressConstants.h
- I2C_Board4_LTC2485_Iout_LH_Global : MasterAddressConstants.h
- I2C_Board4_LTC2485_Vout_LF_ADDR0 : MasterAddressConstants.h
- I2C_Board4_LTC2485_Vout_LF_Global : MasterAddressConstants.h
- I2C_Board4_LTC2655_LLL_ADDR0 : MasterAddressConstants.h
- I2C_Board4_LTC2655_LLL_Global : MasterAddressConstants.h
- I2C_Board5_EEPROM_ADDR0 : MasterAddressConstants.h
- I2C_Board5_LTC2485_Iout_LH_ADDR0 : MasterAddressConstants.h
- I2C_Board5_LTC2485_Iout_LH_Global : MasterAddressConstants.h
- I2C_Board5_LTC2485_Vout_LF_ADDR0 : MasterAddressConstants.h
- I2C_Board5_LTC2485_Vout_LF_Global : MasterAddressConstants.h
- I2C_Board5_LTC2655_LLL_ADDR0 : MasterAddressConstants.h
- I2C_Board5_LTC2655_LLL_Global : MasterAddressConstants.h
- I2C_Board6_EEPROM_ADDR0 : MasterAddressConstants.h
- I2C_Board6_LTC2485_Iout_LH_ADDR0 : MasterAddressConstants.h
- I2C_Board6_LTC2485_Iout_LH_Global : MasterAddressConstants.h
- I2C_Board6_LTC2485_Vout_LF_ADDR0 : MasterAddressConstants.h
- I2C_Board6_LTC2485_Vout_LF_Global : MasterAddressConstants.h
- I2C_Board6_LTC2655_LLL_ADDR0 : MasterAddressConstants.h
- I2C_Board6_LTC2655_LLL_Global : MasterAddressConstants.h
- I2C_Board7_EEPROM_ADDR0 : MasterAddressConstants.h
- I2C_Board7_LTC2485_Iout_LH_ADDR0 : MasterAddressConstants.h
- I2C_Board7_LTC2485_Iout_LH_Global : MasterAddressConstants.h
- I2C_Board7_LTC2485_Vout_LF_ADDR0 : MasterAddressConstants.h
- I2C_Board7_LTC2485_Vout_LF_Global : MasterAddressConstants.h
- I2C_Board7_LTC2655_LLL_ADDR0 : MasterAddressConstants.h
- I2C_Board7_LTC2655_LLL_Global : MasterAddressConstants.h
- I2C_COMMAND : LTC2373.h
- i2c_desc : platform_drivers.h
- i2c_enable() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- I2C_FT6206_ADDR0 : EasySMU_Run.ino
- i2c_init() : platform_drivers.cpp , platform_drivers.h
- i2c_init_param : platform_drivers.h
- i2c_mode : DC590_subset.ino , DC2430A.ino , DC590B.ino , DC590B_enhanced.ino
- i2c_params : CN-0413.ino , EVAL-AD5933.ino , EVAL-AD5686R.ino , EVAL-AD5696R.ino , EVAL-ADT7420.ino
- i2c_poll() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h
- i2c_read() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h , platform_drivers.cpp , platform_drivers.h
- I2C_READ_BIT : LT_I2C.h , LT_I2C_Wire.h
- i2c_read_block_data() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_read_byte() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_read_byte_data() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_read_word_data() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_remove() : platform_drivers.cpp , platform_drivers.h
- i2c_repeated_start() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h
- i2c_scwritelong() : LT3965.cpp , LT3965.h
- i2c_scwriteshort() : LT3965.cpp , LT3965.h
- i2c_scwriteshort_scread() : LT3965.cpp , LT3965.h
- i2c_start() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h
- i2c_stop() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h
- i2c_two_byte_command_read_block() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_type : platform_drivers.h
- i2c_write() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h , platform_drivers.cpp , platform_drivers.h
- I2C_WRITE_BIT : LT_I2C.h , LT_I2C_Wire.h
- i2c_write_block_data() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_write_block_data_no_command() : DC2222AB.ino , DC2222AC.ino
- i2c_write_byte() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_write_byte_data() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_write_word_data() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2cbus : sandbox.ino
- IC_LTC6813 : LTC681x.h
- ICP_RTLI_Root : main_record_processor.h
- icpFile : nvm.cpp
- id : rail_logger.ino
- id_string : DC590B_enhanced.ino , DC2430A.ino , DC590B.ino
- id_string_size : Serial_EEPROM_Test.ino
- ignore_records : main_record_processor.cpp
- IIN_OC_WARN_LIMIT : LT_PMBus.h
- ILI9341_BLACK : Adafruit_ILI9341.h
- ILI9341_BLUE : Adafruit_ILI9341.h
- ILI9341_CASET : Adafruit_ILI9341.h
- ILI9341_CYAN : Adafruit_ILI9341.h
- ILI9341_DARKCYAN : Adafruit_ILI9341.h
- ILI9341_DARKGREEN : Adafruit_ILI9341.h
- ILI9341_DARKGREY : Adafruit_ILI9341.h
- ILI9341_DFUNCTR : Adafruit_ILI9341.h
- ILI9341_DISPOFF : Adafruit_ILI9341.h
- ILI9341_DISPON : Adafruit_ILI9341.h
- ILI9341_FRMCTR1 : Adafruit_ILI9341.h
- ILI9341_FRMCTR2 : Adafruit_ILI9341.h
- ILI9341_FRMCTR3 : Adafruit_ILI9341.h
- ILI9341_GAMMASET : Adafruit_ILI9341.h
- ILI9341_GMCTRN1 : Adafruit_ILI9341.h
- ILI9341_GMCTRP1 : Adafruit_ILI9341.h
- ILI9341_GREEN : Adafruit_ILI9341.h
- ILI9341_GREENYELLOW : Adafruit_ILI9341.h
- ILI9341_INVCTR : Adafruit_ILI9341.h
- ILI9341_INVOFF : Adafruit_ILI9341.h
- ILI9341_INVON : Adafruit_ILI9341.h
- ILI9341_LIGHTGREY : Adafruit_ILI9341.h
- ILI9341_MADCTL : Adafruit_ILI9341.h
- ILI9341_MAGENTA : Adafruit_ILI9341.h
- ILI9341_MAROON : Adafruit_ILI9341.h
- ILI9341_NAVY : Adafruit_ILI9341.h
- ILI9341_NOP : Adafruit_ILI9341.h
- ILI9341_NORON : Adafruit_ILI9341.h
- ILI9341_OLIVE : Adafruit_ILI9341.h
- ILI9341_ORANGE : Adafruit_ILI9341.h
- ILI9341_PASET : Adafruit_ILI9341.h
- ILI9341_PINK : Adafruit_ILI9341.h
- ILI9341_PIXFMT : Adafruit_ILI9341.h
- ILI9341_PTLAR : Adafruit_ILI9341.h
- ILI9341_PTLON : Adafruit_ILI9341.h
- ILI9341_PURPLE : Adafruit_ILI9341.h
- ILI9341_PWCTR1 : Adafruit_ILI9341.h
- ILI9341_PWCTR2 : Adafruit_ILI9341.h
- ILI9341_PWCTR3 : Adafruit_ILI9341.h
- ILI9341_PWCTR4 : Adafruit_ILI9341.h
- ILI9341_PWCTR5 : Adafruit_ILI9341.h
- ILI9341_RAMRD : Adafruit_ILI9341.h
- ILI9341_RAMWR : Adafruit_ILI9341.h
- ILI9341_RDDID : Adafruit_ILI9341.h
- ILI9341_RDDST : Adafruit_ILI9341.h
- ILI9341_RDID1 : Adafruit_ILI9341.h
- ILI9341_RDID2 : Adafruit_ILI9341.h
- ILI9341_RDID3 : Adafruit_ILI9341.h
- ILI9341_RDID4 : Adafruit_ILI9341.h
- ILI9341_RDIMGFMT : Adafruit_ILI9341.h
- ILI9341_RDMADCTL : Adafruit_ILI9341.h
- ILI9341_RDMODE : Adafruit_ILI9341.h
- ILI9341_RDPIXFMT : Adafruit_ILI9341.h
- ILI9341_RDSELFDIAG : Adafruit_ILI9341.h
- ILI9341_RED : Adafruit_ILI9341.h
- ILI9341_SLPIN : Adafruit_ILI9341.h
- ILI9341_SLPOUT : Adafruit_ILI9341.h
- ILI9341_SWRESET : Adafruit_ILI9341.h
- ILI9341_TFTHEIGHT : Adafruit_ILI9341.h
- ILI9341_TFTWIDTH : Adafruit_ILI9341.h
- ILI9341_VMCTR1 : Adafruit_ILI9341.h
- ILI9341_VMCTR2 : Adafruit_ILI9341.h
- ILI9341_WHITE : Adafruit_ILI9341.h
- ILI9341_YELLOW : Adafruit_ILI9341.h
- imon_gain : LTC2492_Panel_Meter.ino
- INC_BUTTON : LTC2492_Thermocouple_Meter.ino
- increment_counter() : retention.ino
- increment_page() : DC1978.ino
- index : device_logger.ino
- init64() : LTC6945.cpp , LTC6947.cpp , LTC6948.cpp , LTC6950.cpp , LTC6946.h , LTC6950.h , LTC6948.h , LTC6947.h , LTC6945.h , LTC6946.cpp
- init_16_bit_PWM() : Margining.ino , DC2197.ino
- init_cfg() : DC1651A.ino , DC1942.ino , DC1894.ino , DC1652A.ino
- init_dac() : Precision_Voltage_Source.ino
- init_gain_pins() : DC1410AB.ino , DC1410AA.ino
- init_params : EVAL-AD5933.ino , EVAL-AD5686R.ino , EVAL-AD5696R.ino , EVAL-AD7124-8.ino , EVAL-ADT7420.ino , CN-0413.ino
- initialise_i2c_data() : DC2222_interrupt_driven_read.ino , DC2222AC.ino , DC2222AB.ino
- initialize() : LTC2492_original.h
- input : DC2218A.ino , Linduino.h
- inputByte_0 : DC2218A.ino
- inputByte_1 : DC2218A.ino
- inputByte_2 : DC2218A.ino
- inputByte_3 : DC2218A.ino
- inputByte_4 : DC2218A.ino
- INSYSTEM_CHIP_AFTER_VERIFY : record_type_definitions.h
- INSYSTEM_CHIP_BEFORE_PROGRAM : record_type_definitions.h
- INSYSTEM_CHIP_BEFORE_VERIFY : record_type_definitions.h
- INT_CAL_PARAMS_BASE : DC1678A.ino , DC1529A.ino , DC1703A.ino , DC1534A.ino , DC1397A.ino , DC1333A.ino
- INT_CAL_VALID_BASE : DC1529A.ino , DC1534A.ino , DC1397A.ino , DC1678A.ino , DC1703A.ino , DC1333A.ino
- int_data : Serial_EEPROM_Test.ino
- integral : LT1054_voltage_mode_buck.ino , LT1054_voltage_mode_buck_DC_ctrl.ino
- INTEGRATOR_CONTROL : DC2692A.ino , DC2025A.ino , DC2196A.ino
- internalCLK : DC2156.ino
- interruptPin : DC2222_interrupt_driven_read.ino
- interval : DC2218A.ino
- IOpanel : EasySMU_Run.ino
- IOUT_OC_FAULT_LIMIT : LT_PMBus.h
- IOUT_OC_WARN_LIMIT : LT_PMBus.h
- is_ltc2977() : retention.ino
- is_ltc2978() : retention.ino
- is_ltc297x() : retention.ino
- is_number_in_array() : support_functions_LTC2983.cpp , support_functions_LTC2984.cpp , support_functions_LTC2983.h , support_functions_LTC2986.cpp , support_functions_LTC2984.h , support_functions_LTC2986.h
- isBitSet() : DC1812AA.ino , DC1812A-B.ino , DC1496BB.ino
- ISOSPI_DIR : DC2515.ino
- ISR() : DC2839A.ino
- ISR_flag : DC2839A.ino
- ISR_prompt_flag : DC2839A.ino
- ith : DC2155A.ino
- ith_dec : DC2155A.ino
- ith_decimal2hex() : DC2155A.ino
- ith_hex2decimal() : DC2155A.ino
- ITH_MAX : DC2155A.ino
- ith_nearest_legal_value() : DC2155A.ino
- ith_vals : DC2155A.ino
- ith_vals_hex : DC2155A.ino