| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

### - a -

- AC_ADDR_0 : LT3965.h
- ACTIVE_ANALOG_CUSTOM_ADDRESS_LSB : configuration_constants_LTC2986.h
- ACTIVE_ANALOG_CUSTOM_LENGTH_1_LSB : configuration_constants_LTC2986.h
- ACTIVE_ANALOG_CUSTOM_VALUES_LSB : configuration_constants_LTC2986.h
- ACTIVE_ANALOG_DIFFERENTIAL : configuration_constants_LTC2986.h
- ACTIVE_ANALOG_DIFFERENTIAL_LSB : configuration_constants_LTC2986.h
- ACTIVE_ANALOG_SINGLE_ENDED : configuration_constants_LTC2986.h
- ADAFRUIT_TFT_TOUCHSHIELD_1947 : EasySMU_IOpanel.h
- ADC_HARD_FAILURE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- ADC_MFR_TELEMETRY_STATUS : fast_telemetry.ino
- ADC_OPT_DISABLED : LTC681x.h
- ADC_OPT_ENABLED : LTC681x.h
- ADC_RANGE_ERROR : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- address1 : LT3965.h
- address2 : LT3965.h
- ADDRESS_DAC_ALL : LTC2752.h , LTC2758.h
- ADDRESS_DACA : LTC2752.h , LTC2758.h
- ADDRESS_DACB : LTC2752.h , LTC2758.h
- ADDRx : LTC6952.h , LTC6953.h , LTC6954.h , LTC6945.h , LTC6946.h , LTC6947.h , LTC6948.h , LTC6950.h , LTC6951.h
- AFTER_DONE : record_type_definitions.h
- ALERTPIN : LT3965.h
- AREF : LTC6115.h
- AUTOMATIC_MODE_DISPLAY_DELAY : DC1496BB.ino , DC1812A-B.ino , DC1812AA.ino
- AUX : LTC6812.h , LTC6810.h , LTC6811.h , LTC6813.h , LTC681x.h
- AUX_CH_ALL : LTC68042.h , LTC68041.h , LTC681x.h
- AUX_CH_GPIO1 : LTC681x.h , LTC68041.h , LTC68042.h
- AUX_CH_GPIO2 : LTC681x.h , LTC68041.h , LTC68042.h
- AUX_CH_GPIO3 : LTC68041.h , LTC68042.h , LTC681x.h
- AUX_CH_GPIO4 : LTC68042.h , LTC681x.h , LTC68041.h
- AUX_CH_GPIO5 : LTC681x.h , LTC68042.h , LTC68041.h
- AUX_CH_VREF2 : LTC681x.h , LTC68041.h , LTC68042.h
- AVERAGE : SeeedTouchScreen.cpp
- AVERAGETIME : SeeedTouchScreen.cpp