| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Data Fields
LT_union_int32_4bytes Union Reference

This union splits one int32_t (32-bit signed integer) or uint32_t (32-bit unsigned integer) four uint8_t's (8-bit unsigned integers) and vice versa. More...

## Detailed Description

This union splits one int32_t (32-bit signed integer) or uint32_t (32-bit unsigned integer) four uint8_t's (8-bit unsigned integers) and vice versa.

Definition at line 108 of file Linduino.h.

## Data Fields
int32_t | LT_int32
| 32-bit signed integer to be converted to four bytes More...
uint32_t | LT_uint32
| 32-bit unsigned integer to be converted to four bytes More...
uint8_t | LT_byte [4]
| 4 bytes (unsigned 8-bit integers) to be converted to a 32-bit signed or unsigned integer More...

## Field Documentation

## ◆ LT_byte

uint8_t LT_union_int32_4bytes::LT_byte[4]

4 bytes (unsigned 8-bit integers) to be converted to a 32-bit signed or unsigned integer

Definition at line 112 of file Linduino.h.

## ◆ LT_int32

int32_t LT_union_int32_4bytes::LT_int32

32-bit signed integer to be converted to four bytes

Definition at line 110 of file Linduino.h.

## ◆ LT_uint32

uint32_t LT_union_int32_4bytes::LT_uint32

32-bit unsigned integer to be converted to four bytes

Definition at line 111 of file Linduino.h.

The documentation for this union was generated from the following file:

- Linduino.h