| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

LT_PMBusDeviceLTC3886.cpp
Go to the documentation of this file.
1 #include "LT_PMBusDeviceLTC3886.h"
2
3 uint32_t LT_PMBusDeviceLTC3886::cap_ = HAS_VOUT
4 | HAS_VIN
5 | HAS_IOUT
6 | HAS_IIN
7 | HAS_POUT
8 | HAS_PIN
9 | HAS_TEMP
10 | HAS_DC
11 | HAS_STATUS_WORD
12 | HAS_STATUS_EXT
13 ;
HAS_VIN
#define HAS_VIN
Definition: LT_PMBusDevice.h:59
HAS_TEMP
#define HAS_TEMP
Definition: LT_PMBusDevice.h:64
HAS_POUT
#define HAS_POUT
Definition: LT_PMBusDevice.h:62
HAS_DC
#define HAS_DC
Definition: LT_PMBusDevice.h:65
LT_PMBusDeviceLTC3886.h
LTC PSM Device.
HAS_IOUT
#define HAS_IOUT
Definition: LT_PMBusDevice.h:60
HAS_PIN
#define HAS_PIN
Definition: LT_PMBusDevice.h:63
HAS_IIN
#define HAS_IIN
Definition: LT_PMBusDevice.h:61
HAS_STATUS_WORD
#define HAS_STATUS_WORD
Definition: LT_PMBusDevice.h:66
LT_PMBusDeviceLTC3886::cap_
static uint32_t cap_
Definition: LT_PMBusDeviceLTC3886.h:59
HAS_VOUT
#define HAS_VOUT
Definition: LT_PMBusDevice.h:58
HAS_STATUS_EXT
#define HAS_STATUS_EXT
Definition: LT_PMBusDevice.h:67