| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

### - e -

- EEPROM_CAL_KEY : QuikEval_EEPROM.h , QuikEval_EEPROM_Wire.h
- EEPROM_CAL_KEY_EXT : DC1333A.ino , DC1529A.ino , DC1678A.ino , DC1534A.ino , DC1703A.ino , DC1397A.ino
- EEPROM_CAL_KEY_INT : DC1534A.ino , DC1333A.ino , DC1678A.ino , DC1703A.ino , DC1397A.ino , DC1529A.ino
- EEPROM_CAL_STATUS_ADDRESS : QuikEval_EEPROM_Wire.h , QuikEval_EEPROM.h
- EEPROM_DATA_SIZE : QuikEval_EEPROM.h , QuikEval_EEPROM_Wire.h , Serial_EEPROM_Test.ino
- EEPROM_FACTORY_CAL_INFO_ADDRESS : EasySMU.h
- EEPROM_FACTORY_CAL_STATUS_ADDRESS : EasySMU.h
- EEPROM_I2C_ADDRESS : QuikEval_EEPROM.h , QuikEval_EEPROM_Wire.h
- EEPROM_KEY : configuration_constants_LTC2984.h
- EEPROM_PAGE_SIZE : QuikEval_EEPROM.h , QuikEval_EEPROM_Wire.h , Serial_EEPROM_Test.ino
- EEPROM_RESULT_CODE_ADDRESS : configuration_constants_LTC2984.h
- EEPROM_START_ADDRESS : configuration_constants_LTC2984.h
- EEPROM_STATUS_REGISTER : configuration_constants_LTC2984.h
- EEPROM_TIMEOUT : QuikEval_EEPROM_Wire.h , QuikEval_EEPROM.h
- ENABLE_KELVIN_2_WIRE_RTD_MODE : configuration_constants_LTC2986.h
- ENABLE_KELVIN_3_WIRE_RTD_MODE : configuration_constants_LTC2986.h
- ENABLE_KELVIN_DIFFERENTIAL_THERMISTOR_MODE : configuration_constants_LTC2986.h
- ENABLED : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- EXT_CAL_PARAMS_BASE : DC1333A.ino , DC1678A.ino , DC1534A.ino , DC1397A.ino , DC1703A.ino , DC1529A.ino
- EXT_CAL_VALID_BASE : DC1529A.ino , DC1703A.ino , DC1397A.ino , DC1678A.ino , DC1333A.ino , DC1534A.ino
- EXT_REF_V_BASE : DC1678A.ino , DC1333A.ino , DC1534A.ino , DC1529A.ino , DC1703A.ino , DC1397A.ino