| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - r -

- R50 : LTC2492_original.h
- R55 : LTC2492_original.h
- R60 : LTC2492_original.h
- R_ONLY : LTC6945.h , LTC6950.h , LTC6951.h , LTC6946.h , LTC6952.h , LTC6953.h , LTC6947.h , LTC6954.h , LTC6948.h
- rail : DC1989A.ino , rail_logger.ino
- rails : rail_logger.ino
- range : DC1096B.ino
- range_low_high : DC682A.ino
- range_selected : DC572A.ino
- RAW_EEPROM : LT_2974FaultLog.cpp , LT_2975FaultLog.cpp , LT_2977FaultLog.cpp , LT_3880FaultLog.cpp , LT_3882FaultLog.cpp , LT_3883FaultLog.cpp , LT_3887FaultLog.cpp
- RE485b : DC2364A.ino
- read16() : spitftbitmap.ino
- read32() : spitftbitmap.ino
- read_68() : LTC681x.cpp , LTC681x.h
- read_bytes() : retention.ino , DC2218A.ino
- read_calibration() : LTC2492_original.h , LTC2492_Thermocouple_Meter.ino
- READ_CH_BASE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- read_char() : UserInterface.cpp , UserInterface.h
- read_command_seq : DC1410AB.ino , DC1410AA.ino
- READ_CONFIG : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- read_count : Serial_EEPROM_Test.ino
- read_data() : UserInterface.cpp , UserInterface.h
- read_data_ISR() : DC2222_interrupt_driven_read.ino
- READ_DUTY_CYCLE : LT_PMBus.h
- read_float() : UserInterface.cpp , UserInterface.h
- READ_FROM_EEPROM : configuration_constants_LTC2984.h
- READ_FROM_RAM : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- read_gain_seq : DC1410AB.ino , DC1410AA.ino
- read_hex() : DC2430A.ino , DC590B.ino , DC590B_enhanced.ino , DC590_subset.ino , DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- READ_IIN : LT_PMBus.h
- read_input_current() : DC2978A.ino
- read_input_voltage() : DC2978A.ino
- read_int() : UserInterface.cpp , UserInterface.h
- READ_IOUT : LT_PMBus.h
- READ_ITEMP : LT_PMBus.h , retention.ino
- READ_ITEMP_2977_8 : retention.ino
- read_LTC2442() : LTC2442_Datalogger.ino
- read_LTC2449() : LTC2449_Datalogger.ino
- read_LTC2492() : LTC2492_original.h , LTC2492_Thermocouple_Meter.ino
- READ_OTEMP : LT_PMBus.h
- read_output_current() : DC2978A.ino
- read_output_voltage() : DC2978A.ino
- READ_PIN : LT_PMBus.h
- READ_POUT : LT_PMBus.h
- read_quikeval_id_string() : QuikEval_EEPROM.cpp , QuikEval_EEPROM.h , QuikEval_EEPROM_Wire.cpp , QuikEval_EEPROM_Wire.h
- read_reg_map() : DC1976A.ino
- read_register() : DC1674A.ino
- read_status() : DC2978A.ino
- read_string() : UserInterface.cpp , UserInterface.h
- read_switches() : Precision_Voltage_Source.ino , Synth.ino
- READ_TIMEOUT : DC2430A.ino , DC590B.ino , DC590B_enhanced.ino
- READ_VIN : LT_PMBus.h
- read_voltage_or_resistance_results() : support_functions_LTC2983.cpp , support_functions_LTC2983.h , support_functions_LTC2984.cpp , support_functions_LTC2984.h , support_functions_LTC2986.cpp , support_functions_LTC2986.h
- READ_VOUT : LT_PMBus.h
- readback : DC2741_production_test.ino
- readI : DC2839A.ino
- readItemp() : retention.ino
- readItemp2977_8() : retention.ino
- ReadLine() : EasySMU_Run.ino
- readpot() : DC2218A.ino
- readThenVerifyNvmData() : nvm_data_helpers.cpp , nvm_data_helpers.h
- readV : DC2839A.ino
- REb_val : DC2364A.ino
- record_data : nvm_data_helpers.cpp
- record_data_hold : nvm_data_helpers.cpp
- RECORD_TYPE_DELAY_MS : record_type_definitions.h
- RECORD_TYPE_DEVICE_ADDRESS : record_type_definitions.h
- RECORD_TYPE_END_OF_RECORDS : record_type_definitions.h
- RECORD_TYPE_EVENT : record_type_definitions.h
- RECORD_TYPE_MODIFY_BYTE_NOPEC : record_type_definitions.h
- RECORD_TYPE_MODIFY_WORD_NOPEC : record_type_definitions.h
- RECORD_TYPE_NVM_DATA : record_type_definitions.h
- RECORD_TYPE_PACKING_CODE : record_type_definitions.h
- RECORD_TYPE_PMBUS_MODIFY_BYTE : record_type_definitions.h
- RECORD_TYPE_PMBUS_MODIFY_WORD : record_type_definitions.h
- RECORD_TYPE_PMBUS_POLL_UNTIL_ACK_NOPEC : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_AND_VERIFY_EE_DATA : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_BLOCK_EXPECT : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_BLOCK_EXPECT_NOPEC : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_BYTE_EXPECT : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_BYTE_EXPECT_MASK_NOPEC : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_BYTE_EXPECT_NOPEC : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_BYTE_LOOP_MASK : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_BYTE_LOOP_MASK_NOPEC : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_WORD_EXPECT : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_WORD_EXPECT_MASK_NOPEC : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_WORD_EXPECT_NOPEC : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_WORD_LOOP_MASK : record_type_definitions.h
- RECORD_TYPE_PMBUS_READ_WORD_LOOP_MASK_NOPEC : record_type_definitions.h
- RECORD_TYPE_PMBUS_SEND_BYTE : record_type_definitions.h
- RECORD_TYPE_PMBUS_SEND_BYTE_NOPEC : record_type_definitions.h
- RECORD_TYPE_PMBUS_WRITE_BLOCK : record_type_definitions.h
- RECORD_TYPE_PMBUS_WRITE_BLOCK_NOPEC : record_type_definitions.h
- RECORD_TYPE_PMBUS_WRITE_BYTE : record_type_definitions.h
- RECORD_TYPE_PMBUS_WRITE_BYTE_NOPEC : record_type_definitions.h
- RECORD_TYPE_PMBUS_WRITE_EE_DATA : record_type_definitions.h
- RECORD_TYPE_PMBUS_WRITE_WORD : record_type_definitions.h
- RECORD_TYPE_PMBUS_WRITE_WORD_NOPEC : record_type_definitions.h
- RECORD_TYPE_VARIABLE_META_DATA : record_type_definitions.h
- recording_buffer : DC2430A.ino , DC590B.ino , DC590B_enhanced.ino
- recording_index : DC2430A.ino , DC590B.ino , DC590B_enhanced.ino
- recording_mode : DC2430A.ino , DC590B.ino , DC590B_enhanced.ino
- RECORDING_SIZE : DC2430A.ino , DC590B.ino , DC590B_enhanced.ino
- RecordOn : onoffbutton.ino , onoffbutton_breakout.ino
- recordProcessor___0x01___processWriteByteOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x02___processWriteWordOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x04___processReadByteExpectOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x05___processReadWordExpectOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x09___bufferNVMData() : main_record_processor.cpp
- recordProcessor___0x0A___processReadByteLoopMaskOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x0B___processReadWordLoopMaskOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x0C___processPollReadByteUntilAckNoPEC() : main_record_processor.cpp
- recordProcessor___0x0D___processDelayMs() : main_record_processor.cpp
- recordProcessor___0x0E___processSendByteOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x0F___processWriteByteNoPEC() : main_record_processor.cpp
- recordProcessor___0x10___processWriteWordNoPEC() : main_record_processor.cpp
- recordProcessor___0x12___processReadByteExpectNoPEC() : main_record_processor.cpp
- recordProcessor___0x13___processReadWordExpectNoPEC() : main_record_processor.cpp
- recordProcessor___0x15___processReadByteLoopMaskNoPEC() : main_record_processor.cpp
- recordProcessor___0x16___processReadWordLoopMaskNoPEC() : main_record_processor.cpp
- recordProcessor___0x17___processSendByteNoPEC() : main_record_processor.cpp
- recordProcessor___0x18___processEvent() : main_record_processor.cpp
- recordProcessor___0x19___processReadByteExpectMaskNoPEC() : main_record_processor.cpp
- recordProcessor___0x1A___processReadWordExpectMaskNoPEC() : main_record_processor.cpp
- recordProcessor___0x1B___processVariableMetaData() : main_record_processor.cpp
- recordProcessor___0x1C___modifyWordNoPEC() : main_record_processor.cpp
- recordProcessor___0x1D___modifyByteNoPEC() : main_record_processor.cpp
- recordProcessor___0x1E___writeNvmData() : main_record_processor.cpp
- recordProcessor___0x1F___read_then_verifyNvmData() : main_record_processor.cpp
- recordProcessor___0x20___modifyByteOptionalPEC() : main_record_processor.cpp
- recordProcessor___0x21___modifyWordOptionalPEC() : main_record_processor.cpp
- redBtn() : onoffbutton.ino , onoffbutton_breakout.ino
- REDBUTTON_H : onoffbutton.ino , onoffbutton_breakout.ino
- REDBUTTON_W : onoffbutton.ino , onoffbutton_breakout.ino
- REDBUTTON_X : onoffbutton.ino , onoffbutton_breakout.ino
- REDBUTTON_Y : onoffbutton.ino , onoffbutton_breakout.ino
- REDLED : LT3965.h
- REF_EXTERNAL : DC935A.ino , DC1466.ino , DC1534A.ino , DC1333A.ino , DC1678A.ino , DC1703A.ino , DC1397A.ino , DC1529A.ino , DC2692A.ino , DC2376A.ino , DC2196A.ino , DC2025A.ino
- REF_INTERNAL : DC935A.ino , DC1466.ino , DC1534A.ino , DC1333A.ino , DC1678A.ino , DC1703A.ino , DC1397A.ino , DC1529A.ino , DC2692A.ino , DC2376A.ino , DC2196A.ino , DC2025A.ino
- ref_out : DC1649A.ino , DC1705C.ino , DC1846A.ino , DC1959A.ino , DC1795A.ino , DC1954A.ino
- reference_mode : DC935A.ino , DC1466.ino , DC1534A.ino , DC1333A.ino , DC1678A.ino , DC1703A.ino , DC1397A.ino , DC1529A.ino
- reference_voltage : DC1397A.ino , DC1529A.ino , _24xx_iso_spi_delay.ino , _24xx_iso_spi_poll.ino , DC746A.ino , DC1011AB.ino , DC1703A.ino , DC579A.ino , DC809A.ino , DC935A.ino , DC1466.ino , DC1534A.ino , DC1333A.ino , DC1096B.ino , DC1678A.ino
- REFON : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- REFRESH_INTERVAL : DC2343A.ino
- refresh_time_last : DC2343A.ino
- REG : Synth.ino
- REG_1 : LTC681x.h
- REG_2 : LTC681x.h
- REG_3 : LTC681x.h
- REG_4 : LTC681x.h
- REG_5 : LTC681x.h
- REG_6 : LTC681x.h
- REG_ALL : LTC681x.h
- reg_phase : DC1558_DC1808.ino , DC1976A.ino
- reg_read_list : LTM9100.cpp , LTM9100.h , DC1558_DC1808.ino
- reg_test() : DC1880A.ino
- reg_write_list : LTM9100.cpp , DC1558_DC1808.ino , LTM9100.h
- register_value : LTC5556.cpp
- regNr : EVAL-AD7124-8.ino
- REJECTION50 : DC939A.ino
- REJECTION50_60 : DC939A.ino
- REJECTION60 : DC939A.ino
- REJECTION__50_60_HZ : configuration_constants_LTC2983.h , configuration_constants_LTC2986.h , configuration_constants_LTC2984.h
- REJECTION__50_HZ : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- REJECTION__60_HZ : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- rejection_mode : DC1009AA.ino , DC1011AA.ino , DC1410AA.ino , DC1012AA.ino , LTC2492_Panel_Meter.ino
- RESERVED2 : retention.ino
- reset() : DC2978A.ino
- reset_all_devices() : program.ino
- reset_parse_hex() : hex_file_parser.h , hex_file_parser.cpp
- resistive_ratio : DC998A.ino
- resistor : DC1496BB.ino , DC1812AA.ino , DC1812A-B.ino , DC1697A.ino , DC2156.ino , DC1208A.ino , DC998A.ino , DC2024A.ino , DC2561.ino
- restore() : retention.ino
- restore_alert_settings() : DC1496BB.ino , DC1812AA.ino , DC1812A-B.ino , DC2156.ino , DC1697A.ino
- restore_calibration() : DC1397A.ino , DC806A.ino , DC571A.ino , DC742A.ino , DC1491A.ino , DC939A.ino , DC1466.ino , DC1333A.ino , DC1678A.ino , DC1703A.ino , DC1529A.ino , Audio_Spectrum_Analyzer.ino , DC1534A.ino
- restore_dac_from_eeprom() : DC2692A.ino , DC2196A.ino , DC2025A.ino , DC2376A.ino
- restore_nvm() : program.ino
- restore_settings() : Synth.ino
- RESTORE_USER_ALL : retention.ino , LT_PMBus.h
- ret : EVAL-AD7124-8.ino
- return_values : DC2313A.ino
- reverse_isospi_direction() : DC2515.ino
- RIGHT : Precision_Voltage_Source.ino , Synth.ino
- RO : DC2364A.ino
- rotate() : LT_2974FaultLog.cpp
- RS : LTC2492_Thermocouple_Meter.ino , Precision_Voltage_Source.ino , Synth.ino
- RTD_CUSTOM_ADDRESS_LSB : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- RTD_CUSTOM_LENGTH_1_LSB : configuration_constants_LTC2986.h , configuration_constants_LTC2984.h , configuration_constants_LTC2983.h
- RTD_CUSTOM_VALUES_LSB : configuration_constants_LTC2983.h , configuration_constants_LTC2986.h , configuration_constants_LTC2984.h
- RTD_EXCITATION_CURRENT__100UA : configuration_constants_LTC2986.h , configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_EXCITATION_CURRENT__10UA : configuration_constants_LTC2984.h , configuration_constants_LTC2983.h , configuration_constants_LTC2986.h
- RTD_EXCITATION_CURRENT__1MA : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- RTD_EXCITATION_CURRENT__250UA : configuration_constants_LTC2983.h , configuration_constants_LTC2986.h , configuration_constants_LTC2984.h
- RTD_EXCITATION_CURRENT__25UA : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- RTD_EXCITATION_CURRENT__500UA : configuration_constants_LTC2986.h , configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_EXCITATION_CURRENT__50UA : configuration_constants_LTC2984.h , configuration_constants_LTC2983.h , configuration_constants_LTC2986.h
- RTD_EXCITATION_CURRENT__5UA : configuration_constants_LTC2986.h , configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_EXCITATION_CURRENT__EXTERNAL : configuration_constants_LTC2986.h
- RTD_EXCITATION_CURRENT__INVALID : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_EXCITATION_CURRENT_LSB : configuration_constants_LTC2986.h , configuration_constants_LTC2984.h , configuration_constants_LTC2983.h
- RTD_EXCITATION_MODE__NO_ROTATION_NO_SHARING : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- RTD_EXCITATION_MODE__NO_ROTATION_SHARING : configuration_constants_LTC2983.h , configuration_constants_LTC2986.h , configuration_constants_LTC2984.h
- RTD_EXCITATION_MODE__ROTATION_SHARING : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- RTD_EXCITATION_MODE_LSB : configuration_constants_LTC2986.h , configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_NUM_WIRES__2_WIRE : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- RTD_NUM_WIRES__3_WIRE : configuration_constants_LTC2983.h , configuration_constants_LTC2986.h , configuration_constants_LTC2984.h
- RTD_NUM_WIRES__4_WIRE : configuration_constants_LTC2983.h , configuration_constants_LTC2986.h , configuration_constants_LTC2984.h
- RTD_NUM_WIRES__4_WIRE_KELVIN_RSENSE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- RTD_NUM_WIRES_LSB : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- RTD_RSENSE_CHANNEL__1 : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- RTD_RSENSE_CHANNEL__10 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- RTD_RSENSE_CHANNEL__11 : configuration_constants_LTC2984.h , configuration_constants_LTC2983.h
- RTD_RSENSE_CHANNEL__12 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_RSENSE_CHANNEL__13 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_RSENSE_CHANNEL__14 : configuration_constants_LTC2984.h , configuration_constants_LTC2983.h
- RTD_RSENSE_CHANNEL__15 : configuration_constants_LTC2984.h , configuration_constants_LTC2983.h
- RTD_RSENSE_CHANNEL__16 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_RSENSE_CHANNEL__17 : configuration_constants_LTC2984.h , configuration_constants_LTC2983.h
- RTD_RSENSE_CHANNEL__18 : configuration_constants_LTC2984.h , configuration_constants_LTC2983.h
- RTD_RSENSE_CHANNEL__19 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_RSENSE_CHANNEL__2 : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- RTD_RSENSE_CHANNEL__20 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_RSENSE_CHANNEL__3 : configuration_constants_LTC2986.h , configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_RSENSE_CHANNEL__4 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- RTD_RSENSE_CHANNEL__5 : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- RTD_RSENSE_CHANNEL__6 : configuration_constants_LTC2986.h , configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_RSENSE_CHANNEL__7 : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- RTD_RSENSE_CHANNEL__8 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- RTD_RSENSE_CHANNEL__9 : configuration_constants_LTC2984.h , configuration_constants_LTC2983.h , configuration_constants_LTC2986.h
- RTD_RSENSE_CHANNEL__NONE : configuration_constants_LTC2986.h , configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_RSENSE_CHANNEL_LSB : configuration_constants_LTC2983.h , configuration_constants_LTC2986.h , configuration_constants_LTC2984.h
- RTD_STANDARD__AMERICAN : configuration_constants_LTC2984.h , configuration_constants_LTC2983.h , configuration_constants_LTC2986.h
- RTD_STANDARD__EUROPEAN : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- RTD_STANDARD__ITS_90 : configuration_constants_LTC2986.h , configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- RTD_STANDARD__JAPANESE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- RTD_STANDARD_LSB : configuration_constants_LTC2986.h , configuration_constants_LTC2984.h , configuration_constants_LTC2983.h
- run_command() : DC1651A.ino , DC2350AB.ino , DC1942.ino , DC1894.ino , DC2515.ino , DC1652A.ino , DC2350AA.ino , DC2259.ino
- rw : DC2091A.ino
- rx_cfg : DC1894.ino , DC1652A.ino , DC1942.ino , DC1651A.ino
- RXPLATE : SeeedTouchScreen.cpp