| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
ARM_SHIPMODE
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

ARM_SHIPMODE Bit Field. More...

## Macros
#define | LTC4155_ARM_SHIPMODE_SUBADDR LTC4155_REG7_SUBADDR
| ARM_SHIPMODE More...
#define | LTC4155_ARM_SHIPMODE_SIZE 8
#define | LTC4155_ARM_SHIPMODE_OFFSET 0
#define | LTC4155_ARM_SHIPMODE_MASK 0xFF
#define | LTC4155_ARM_SHIPMODE (LTC4155_ARM_SHIPMODE_OFFSET << 12 | (LTC4155_ARM_SHIPMODE_SIZE - 1) << 8 | LTC4155_ARM_SHIPMODE_SUBADDR)
#define | LTC4155_ARM_SHIPMODE_PRESET_ARM 0x01

## Detailed Description

ARM_SHIPMODE Bit Field.

Write any data to this address to enable ship-and-store shutdown mode

- Register: REG7
- CommandCode: 0x07
- Size: 8
- Offset: 0
- MSB: 7
- MASK: 0xFF
- Access: W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_ARM_SHIPMODE

#define LTC4155_ARM_SHIPMODE (LTC4155_ARM_SHIPMODE_OFFSET << 12 | (LTC4155_ARM_SHIPMODE_SIZE - 1) << 8 | LTC4155_ARM_SHIPMODE_SUBADDR)

Definition at line 1036 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ARM_SHIPMODE_MASK

#define LTC4155_ARM_SHIPMODE_MASK 0xFF

Definition at line 1035 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ARM_SHIPMODE_OFFSET

#define LTC4155_ARM_SHIPMODE_OFFSET 0

Definition at line 1034 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ARM_SHIPMODE_PRESET_ARM

#define LTC4155_ARM_SHIPMODE_PRESET_ARM 0x01

Definition at line 1037 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ARM_SHIPMODE_SIZE

#define LTC4155_ARM_SHIPMODE_SIZE 8

Definition at line 1033 of file LTC4155_reg_defs.h.

## ◆ LTC4155_ARM_SHIPMODE_SUBADDR

#define LTC4155_ARM_SHIPMODE_SUBADDR LTC4155_REG7_SUBADDR

ARM_SHIPMODE

Definition at line 1032 of file LTC4155_reg_defs.h.