| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - p -

- packingCode : t_RECORD_PACKING_CODE
- page() : LT_PMBus
- pages : tRailDef
- peak : LT_2974FaultLog::Peak16Words , LT_2974FaultLog::Peak5_11Words , LT_2975FaultLog::Peak16Words , LT_2975FaultLog::Peak5_11Words , LT_2977FaultLog::Peak16Words , LT_2977FaultLog::Peak5_11Words , LT_2978FaultLog::Peak16Words , LT_2978FaultLog::Peak5_11Words
- peaks : LT_2974FaultLog::FaultLogPreambleLtc2974 , LT_2975FaultLog::FaultLogPreambleLtc2975 , LT_2977FaultLog::FaultLogPreambleLtc2977 , LT_2978FaultLog::FaultLogPreambleLtc2978 , LT_3880FaultLog::FaultLogPreambleLtc3880 , LT_3882FaultLog::FaultLogPreambleLtc3882 , LT_3883FaultLog::FaultLogPreambleLtc3883 , LT_3887FaultLog::FaultLogPreambleLtc3887
- pec_count : pec_counter
- pec_enabled_ : LT_SMBus
- pec_match : ax , cv , st
- pecAdd() : LT_SMBus
- pecClear() : LT_SMBus
- pecEnabled() : LT_SMBus
- pecGet() : LT_SMBus
- pin_data : LT_2975FaultLog::FaultLogReadLoopLtc2975
- pin_peaks : LT_2975FaultLog::FaultLogPeaksLtc2975
- pmbus() : LT_PMBusDevice
- pmbus_ : LT_FaultLog , LT_PMBusDetect , LT_PMBusDevice , LT_PMBusSpeedTest
- Point() : Point
- poly_ : LT_SMBus
- port_configuration : LTC4155_chip_cfg_t
- position_fault : LT_3880FaultLog::FaultLogPreambleLtc3880 , LT_3882FaultLog::FaultLogPreambleLtc3882 , LT_3883FaultLog::FaultLogPreambleLtc3883 , LT_3887FaultLog::FaultLogPreambleLtc3887
- position_last : LT_2974FaultLog::FaultLogPreambleLtc2974 , LT_2975FaultLog::FaultLogPreambleLtc2975 , LT_2977FaultLog::FaultLogPreambleLtc2977 , LT_2978FaultLog::FaultLogPreambleLtc2978
- pout_data0 : LT_2974FaultLog::FaultLogReadLoopLtc2974 , LT_2975FaultLog::FaultLogReadLoopLtc2975
- pout_data1 : LT_2974FaultLog::FaultLogReadLoopLtc2974 , LT_2975FaultLog::FaultLogReadLoopLtc2975
- pout_data2 : LT_2974FaultLog::FaultLogReadLoopLtc2974 , LT_2975FaultLog::FaultLogReadLoopLtc2975
- pout_data3 : LT_2974FaultLog::FaultLogReadLoopLtc2974 , LT_2975FaultLog::FaultLogReadLoopLtc2975
- preamble : LT_2974FaultLog::FaultLogLtc2974 , LT_2975FaultLog::FaultLogLtc2975 , LT_2977FaultLog::FaultLogLtc2977 , LT_2978FaultLog::FaultLogLtc2978 , LT_3880FaultLog::FaultLogLtc3880 , LT_3882FaultLog::FaultLogLtc3882 , LT_3883FaultLog::FaultLogLtc3883 , LT_3887FaultLog::FaultLogLtc3887
- present_ : EasySMU
- press() : Adafruit_GFX_Button
- print() : LT_2974FaultLog , LT_2975FaultLog , LT_2977FaultLog , LT_2978FaultLog , LT_3880FaultLog , LT_3882FaultLog , LT_3883FaultLog , LT_3887FaultLog , LT_FaultLog
- PrintFactoryCalibrationInfo() : EasySMU
- probe() : LT_SMBus , LT_SMBusBase
- probeSpeed() : LT_PMBusDevice
- probeUnique() : LT_SMBus , LT_SMBusBase
- product_name : demo_board_type
- programWithData() : NVM
- pushColor() : Adafruit_ILI9341
- pwm : cell_asic
- pwmb : cell_asic