| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Functions | Macros
I2C_Address_Scan.ino File Reference

Go to the source code of this file.

## Functions
static void | print_title ()
static void | setup ()
static void | loop ()

## Macros
#define | SW_I2C_FREQUENCY 400

## Function Documentation

## ◆ loop()

static void loop | ( | void |  | ) |
| static

Definition at line 82 of file I2C_Address_Scan.ino.

## ◆ print_title()

static void print_title | ( | void |  | ) |
| static

Definition at line 58 of file I2C_Address_Scan.ino.

## ◆ setup()

static void setup | ( | void |  | ) |
| static

Definition at line 73 of file I2C_Address_Scan.ino.

## Macro Definition Documentation

## ◆ SW_I2C_FREQUENCY

#define SW_I2C_FREQUENCY 400

Definition at line 49 of file I2C_Address_Scan.ino.