| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
REG3
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

REG3 Register. More...

## Macros
#define | LTC4155_REG3_SUBADDR 0x03
#define | LTC4155_REG3 (0 << 12 | (16 - 1) << 8 | LTC4155_REG3_SUBADDR)

## Detailed Description

REG3 Register.

7:5 | 4 | 3 | 2:1 | 0
--- | --- | --- | --- | ---
CHARGER_STATUS | ID_PIN_DETECT | OTG_ENABLED | NTCSTAT | LOWBAT

- CommandCode: 0x03
- Contains Bit Fields:
  - CHARGER_STATUS : Battery charger status.
  - ID_PIN_DETECT : On-the-Go boost ID pin detection status.
  - OTG_ENABLED : On-the-Go boost converter enable status.
  - NTCSTAT : Thermistor reading status.
  - LOWBAT : Battery below ~2.8V or charger disabled.

## Macro Definition Documentation

## ◆ LTC4155_REG3

#define LTC4155_REG3 (0 << 12 | (16 - 1) << 8 | LTC4155_REG3_SUBADDR)

Definition at line 432 of file LTC4155_reg_defs.h.

## ◆ LTC4155_REG3_SUBADDR

#define LTC4155_REG3_SUBADDR 0x03

Definition at line 431 of file LTC4155_reg_defs.h.