| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - d -

- D4 : LTC2492_Thermocouple_Meter.ino , Precision_Voltage_Source.ino , Synth.ino
- D5 : LTC2492_Thermocouple_Meter.ino , Precision_Voltage_Source.ino , Synth.ino
- D6 : Precision_Voltage_Source.ino , Synth.ino , LTC2492_Thermocouple_Meter.ino
- D7 : LTC2492_Thermocouple_Meter.ino , Precision_Voltage_Source.ino , Synth.ino
- DAC_A : DC2197.ino , Margining.ino
- DAC_B : Margining.ino , DC2197.ino
- DAC_C : DC2197.ino
- DAC_D : DC2197.ino
- DAC_SELECTED : DC1684AB.ino , DC1684AA.ino
- dac_selection : EVAL-AD5686R.ino , EVAL-AD5696R.ino
- DACA_RANGE_HIGH : DC1684AB.ino , DC1684AA.ino
- DACA_RANGE_LOW : DC1684AB.ino , DC1684AA.ino
- DACB_RANGE_HIGH : DC1684AB.ino , DC1684AA.ino
- DACB_RANGE_LOW : DC1684AB.ino , DC1684AA.ino
- data : DC2094A.ino , DC1674A.ino , DC572A.ino
- DATA_H : data.h
- data_point_counter : DC2343A.ino
- DATALOG_DISABLED : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- DATALOG_ENABLED : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- dazzle() : DC2218A.ino
- DC1605_DAC_ADDRESS : DC1605B.ino
- dc1605_dac_address : DC1605B.ino
- dc1605_write_dac_voltage() : DC1605B.ino
- dc1605b_is_address_0x5n() : DC1605B.ino
- dc1605b_print_address_warning() : DC1605B.ino
- dc1613_addresses : program.ino
- DC1633_DAC_ADDRESS : DC1633B.ino
- dc1633_dac_address : DC1633B.ino
- dc1633_write_dac_voltage() : DC1633B.ino
- dc2248_board_connected : DC2248A.ino
- DC2430_Bin : DC2430A.ino
- dc2430_en_Pin : DC2248A.ino , DC2609A.ino , DC2610A.ino
- DC2430_parallelsync_example() : DC2430A.ino
- dc2430_site_A0_APin : DC2248A.ino , DC2609A.ino , DC2610A.ino
- dc2430_site_A1_APin : DC2609A.ino , DC2610A.ino , DC2248A.ino
- dc2430_site_A2_APin : DC2248A.ino , DC2609A.ino , DC2610A.ino
- dc2430_site_DA0_Pin : DC2248A.ino , DC2609A.ino , DC2610A.ino
- dc2430_site_DA1_Pin : DC2248A.ino , DC2609A.ino , DC2610A.ino
- dc2430_site_DA2_Pin : DC2248A.ino , DC2609A.ino , DC2610A.ino
- dc2430_site_select() : DC2248A.ino , DC2609A.ino , DC2610A.ino
- DC2430_test_manualmode() : DC2430A.ino
- DC2430_test_supply() : DC2430A.ino
- DC2430_test_swmode() : DC2430A.ino
- DC2430_test_SYNC() : DC2430A.ino
- DC2430_testmode_ctr : DC2430A.ino
- DC2430_testprog() : DC2430A.ino
- DC2609_board_connected : DC2609A.ino
- DC2610_board_connected : DC2610A.ino
- dc590Busy : DC590_subset.ino , DC2574A_KIT.ino
- DCCBIT_0 : DC2515.ino
- DCCBITS : DC2515.ino
- DCCBITS_A : DC2259.ino , DC2350AA.ino , DC2350AB.ino
- DCCBITS_B : DC2350AA.ino , DC2350AB.ino
- DCP_DISABLED : LTC68041.h , LTC68042.h , LTC681x.h
- DCP_ENABLED : LTC68041.h , LTC68042.h , LTC681x.h
- DCTOBITS : DC2515.ino , DC2259.ino , DC2350AA.ino , DC2350AB.ino
- DE : CN0416_capitalizer.ino , CN0416_echo_node.ino
- DE485_F232 : DC2364A.ino
- DE485_F232_val : DC2364A.ino
- DEBUG_FLASH : nvm.cpp
- DEBUG_PARSE_DATA : hex_file_parser.cpp
- DEBUG_PRINT : main_record_processor.cpp
- DEBUG_PROCESSING : main_record_processor.cpp
- DEBUG_SILENT : main_record_processor.cpp
- DEC_BUTTON : LTC2492_Thermocouple_Meter.ino
- decode_DF_value() : DC2222AB.ino , DC2222AC.ino
- decode_values() : DC2094A.ino
- DELAY : Adafruit_ILI9341.cpp
- delay_EOC : _24xx_iso_spi_delay.ino
- delay_m() : bms_hardware.cpp , bms_hardware.h
- delay_ms : DC1558_DC1808.ino , DC1976A.ino
- delay_u() : bms_hardware.h , bms_hardware.cpp
- DelayAndCheckSerialData() : DC590_subset.ino
- DelayAndProcessInputs() : DC2574A_KIT.ino
- DelayAndUserInput() : EasySMU_Run.ino
- demo_board : QuikEval_EEPROM.cpp , QuikEval_EEPROM.h , QuikEval_EEPROM_Wire.cpp , QuikEval_EEPROM_Wire.h
- demo_board_connected : _24xx_iso_spi_delay.ino , _24xx_iso_spi_poll.ino , LTC2492_Panel_Meter.ino , DC572A.ino , DC806A.ino , DC1444A.ino , DC2094A.ino , DC746A.ino , DC571A.ino , DC570A.ino , DC1410AB.ino , DC742A.ino , DC1490.ino , DC1491A.ino , DC798B.ino , DC941A.ino , DC939A.ino , DC1009AA.ino , DC1011AB.ino , DC1012A_B.ino , DC1011AA.ino , DC1410AA.ino , DC1012AA.ino , DC579A.ino , DC809A.ino , DC935A.ino , Synth.ino , DC934A.ino , DC1466.ino , DC1534A.ino , DC2610A.ino , DC1333A.ino , DC1678A.ino , DC1703A.ino , DC1397A.ino , DC1529A.ino , DC2692A.ino , DC2376A.ino , DC2217A.ino , DC2196A.ino , DC2025A.ino , DC1684AB.ino , DC1976A.ino , DC1684AA.ino , DC1880A.ino , DC1496BB.ino , DC1812AA.ino , DC1812A-B.ino , DC1697A.ino , DC2156.ino , DC2334A.ino , DC1338.ino , DC1785A.ino , DC2561.ino , DC1558_DC1808.ino , DC1208A.ino , DC998A.ino , DC2024A.ino , DC1649A.ino , DC1705C.ino , DC1846A.ino , DC1959A.ino , DC1795A.ino , DC2248A.ino , DC2609A.ino , DC1954A.ino , DC2430A.ino , Precision_Voltage_Source.ino , vmClock.ino
- demo_board_connected_man : DC2430A.ino
- demo_board_option() : DC1976A.ino
- demo_board_test() : LTC2668_backpage_app.ino
- demo_name : DC1880A.ino , DC1976A.ino , Synth.ino , vmClock.ino , LTC24XX_general_test.ino
- demo_name_1 : DC1558_DC1808.ino
- demo_name_2 : DC1558_DC1808.ino
- DequeueChar() : DC590_subset.ino
- descr : DC2741_production_test.ino
- detect_colons() : hex_file_parser.cpp , hex_file_parser.h
- detector : DC1989A.ino , device_logger.ino , rail_logger.ino
- device : EVAL-AD5933.ino , CN-0413.ino , EVAL-AD5686R.ino , EVAL-AD5696R.ino , EVAL-ADT7420.ino , device_logger.ino , rail_logger.ino
- devices : device_logger.ino , rail_logger.ino
- DI : DC2364A.ino
- di_toggle : DC2364A.ino
- DI_val : DC2364A.ino
- DIFF_CONFIG_ARRAY : LTC24XX_general_test.ino , LTC2449_Datalogger.ino
- DIODE_AVERAGING_OFF : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- DIODE_AVERAGING_ON : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- DIODE_AVERAGING_ON_LSB : configuration_constants_LTC2983.h , configuration_constants_LTC2986.h , configuration_constants_LTC2984.h
- DIODE_CURRENT__10UA_40UA_80UA : configuration_constants_LTC2986.h , configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- DIODE_CURRENT__20UA_80UA_160UA : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- DIODE_CURRENT__40UA_160UA_320UA : configuration_constants_LTC2983.h , configuration_constants_LTC2986.h , configuration_constants_LTC2984.h
- DIODE_CURRENT__80UA_320UA_640UA : configuration_constants_LTC2986.h , configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- DIODE_CURRENT_LSB : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- DIODE_DIFFERENTIAL : configuration_constants_LTC2983.h , configuration_constants_LTC2986.h , configuration_constants_LTC2984.h
- DIODE_DIFFERENTIAL_LSB : configuration_constants_LTC2984.h , configuration_constants_LTC2983.h , configuration_constants_LTC2986.h
- DIODE_IDEALITY_FACTOR_LSB : configuration_constants_LTC2983.h , configuration_constants_LTC2986.h , configuration_constants_LTC2984.h
- DIODE_NUM_READINGS__2 : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- DIODE_NUM_READINGS__3 : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- DIODE_NUM_READINGS_LSB : configuration_constants_LTC2984.h , configuration_constants_LTC2983.h , configuration_constants_LTC2986.h
- DIODE_SINGLE_ENDED : configuration_constants_LTC2986.h , configuration_constants_LTC2983.h , configuration_constants_LTC2984.h
- DIRECT_ADC_CUSTOM__NO : configuration_constants_LTC2986.h
- DIRECT_ADC_CUSTOM__YES : configuration_constants_LTC2986.h
- DIRECT_ADC_CUSTOM_ADDRESS_LSB : configuration_constants_LTC2986.h
- DIRECT_ADC_CUSTOM_LENGTH_1_LSB : configuration_constants_LTC2986.h
- DIRECT_ADC_CUSTOM_LSB : configuration_constants_LTC2986.h
- DIRECT_ADC_CUSTOM_VALUES_LSB : configuration_constants_LTC2986.h
- DIRECT_ADC_DIFFERENTIAL : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- DIRECT_ADC_DIFFERENTIAL_LSB : configuration_constants_LTC2983.h , configuration_constants_LTC2986.h , configuration_constants_LTC2984.h
- DIRECT_ADC_SINGLE_ENDED : configuration_constants_LTC2984.h , configuration_constants_LTC2986.h , configuration_constants_LTC2983.h
- DIS_RED : DC2515.ino
- disable_calibration() : QuikEval_EEPROM_Wire.cpp , QuikEval_EEPROM_Wire.h , QuikEval_EEPROM.h , QuikEval_EEPROM.cpp
- DISABLE_MINUS_999 : configuration_constants_LTC2986.h
- DISABLED : DC2350AA.ino , DC2350AB.ino , DC2515.ino , DC2259.ino
- discharged_capacity : DC2343A.ino
- discover_DC1684AB() : DC1684AA.ino , DC1684AB.ino
- discover_DC2094() : DC2094A.ino
- discover_DC786A() : DC786A.ino
- discover_DC985A() : DC985A.ino
- discover_demo_board() : QuikEval_EEPROM_Wire.h , QuikEval_EEPROM.cpp , QuikEval_EEPROM.h , QuikEval_EEPROM_Wire.cpp
- discover_demo_board_local() : LTC6951.h , LTC6952.cpp , LTC6953.cpp , LTC6953.h , LTC6951.cpp , DC2430A.ino , LTC6952.h
- discover_demo_boards() : DC1558_DC1808.ino
- display() : LTC2492_original.h
- display_code : DC2071AA.ino
- display_decimal() : Precision_Voltage_Source.ino
- display_fault() : DC2692A.ino
- display_graph() : Audio_Spectrum_Analyzer.ino
- display_hex() : Precision_Voltage_Source.ino
- display_menu() : Audio_Spectrum_Analyzer.ino
- div64() : LTC6946.cpp , LTC6948.h , LTC6950.h , LTC6947.h , LTC6948.cpp , LTC6946.h , LTC6950.cpp , LTC6945.h , LTC6945.cpp , LTC6947.cpp
- dodisplay : rail_logger.ino
- doprint : device_logger.ino , rail_logger.ino
- DOWN : Synth.ino , Precision_Voltage_Source.ino , LT3965.h
- DPI : fontconvert.c
- drawFrame() : onoffbutton_breakout.ino , onoffbutton.ino
- DTMEN : DC2350AA.ino , DC2350AB.ino
- DUTsync() : DC2609A.ino , DC2248A.ino , DC2610A.ino
- DxMSB : LTC6947.h , LTC6946.h , LTC6954.h , LTC6950.h , LTC6948.h , LTC6952.h , LTC6951.h , LTC6945.h , LTC6953.h