| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - s -

- sctrl : cell_asic
- sctrlb : cell_asic
- searchForLCD() : LCDKeypad
- sendByte() : LT_SMBus , LT_SMBusBase , LT_SMBusGroup
- sequenceOff() : LT_PMBus , LT_PMBusRail
- sequenceOffGlobal() : LT_PMBus
- sequenceOn() : LT_PMBus , LT_PMBusRail
- sequenceOnGlobal() : LT_PMBus
- serialNumber : t_RECORD_META_OEM_SERIAL_NUMBER
- setAddrWindow() : Adafruit_ILI9341
- SetCalibration() : EasySMU
- SetCalibrationSinglePoint() : EasySMU
- setCmlStatusMask() : LT_PMBus
- setCursor() : Adafruit_GFX
- setFont() : Adafruit_GFX
- setIinOcWarnLimit() : LT_PMBus
- setInputStatusMask() : LT_PMBus
- setIoutOcFaultLimit() : LT_PMBus
- setIoutOcFaultLimitWithPage() : LT_PMBus
- setIoutOcFaultLimitWithPagePlus() : LT_PMBus
- setIoutOcWarnLimit() : LT_PMBus
- setIoutOcWarnLimitWithPage() : LT_PMBus
- setIoutOcWarnLimitWithPagePlus() : LT_PMBus
- setIoutStatusMask() : LT_PMBus
- setMfrStatusMask() : LT_PMBus
- setMfrWatchdog() : LT_PMBus
- setMfrWatchdogFirst() : LT_PMBus
- setOtFaultLimit() : LT_PMBus
- setOtFaultLimitWithPage() : LT_PMBus
- setOtFaultLimitWithPagePlus() : LT_PMBus
- setOtWarnLimit() : LT_PMBus
- setOtWarnLimitWithPage() : LT_PMBus
- setOtWarnLimitWithPagePlus() : LT_PMBus
- setPage() : LT_PMBus , LT_PMBusDevice
- setPageWithPolling() : LT_PMBus
- setRailAddress() : LT_PMBus
- setRotation() : Adafruit_GFX , Adafruit_ILI9341
- setSpareData0() : LT_PMBus
- setSpeed() : LT_PMBusDevice , LT_PMBusDeviceManager
- setTemp1Gain() : LT_PMBus
- setTemp1Offset() : LT_PMBus
- setTemperatureStatusMask() : LT_PMBus
- setTextColor() : Adafruit_GFX
- setTextSize() : Adafruit_GFX
- setTextWrap() : Adafruit_GFX
- setToffDelay() : LT_PMBus
- setToffFall() : LT_PMBus
- setToffMaxWarnLimit() : LT_PMBus
- setTonDelay() : LT_PMBus
- setTonMaxFaultLimit() : LT_PMBus
- setTonRise() : LT_PMBus
- setUserData03() : LT_PMBus
- setUserData04() : LT_PMBus
- setUtFaultLimit() : LT_PMBus
- setUtFaultLimitWithPage() : LT_PMBus
- setUtFaultLimitWithPagePlus() : LT_PMBus
- setUtWarnLimit() : LT_PMBus
- setUtWarnLimitWithPage() : LT_PMBus
- setUtWarnLimitWithPagePlus() : LT_PMBus
- setVinOvFaultLimit() : LT_PMBus
- setVinOvWarningLimit() : LT_PMBus
- setVinOvWarnLimit() : LT_PMBus
- setVinUvFaultLimit() : LT_PMBus
- setVinUvWarnLimit() : LT_PMBus
- setVout() : LT_PMBus , LT_PMBusDevice , LT_PMBusRail
- setVoutMarginHigh() : LT_PMBus
- setVoutMarginHighWithPage() : LT_PMBus
- setVoutMarginHighWithPagePlus() : LT_PMBus
- setVoutMarginLow() : LT_PMBus
- setVoutMarginLowWithPage() : LT_PMBus
- setVoutMarginLowWithPagePlus() : LT_PMBus
- setVoutMax() : LT_PMBus
- setVoutMaxWithPage() : LT_PMBus
- setVoutMaxWithPagePlus() : LT_PMBus
- setVoutMin() : LT_PMBus
- setVoutMinWithPage() : LT_PMBus
- setVoutMinWithPagePlus() : LT_PMBus
- setVoutOvFaultLimit() : LT_PMBus
- setVoutOvFaultLimitWithPage() : LT_PMBus
- setVoutOvFaultLimitWithPagePlus() : LT_PMBus
- setVoutOvWarnLimit() : LT_PMBus
- setVoutOvWarnLimitWithPage() : LT_PMBus
- setVoutOvWarnLimitWithPagePlus() : LT_PMBus
- setVoutStatusMask() : LT_PMBus
- setVoutUvFaultLimit() : LT_PMBus
- setVoutUvFaultLimitWithPage() : LT_PMBus
- setVoutUvFaultLimitWithPagePlus() : LT_PMBus
- setVoutUvWarnLimit() : LT_PMBus
- setVoutUvWarnLimitWithPage() : LT_PMBus
- setVoutUvWarnLimitWithPagePlus() : LT_PMBus
- setVoutWithPage() : LT_PMBus
- setVoutWithPagePlus() : LT_PMBus
- setVoutWithSupervision() : LT_PMBus
- setVoutWithSupervisionWithPage() : LT_PMBus
- setVoutWithSupervisionWithPagePlus() : LT_PMBus
- shared_time : LT_2974FaultLog::FaultLogPreambleLtc2974 , LT_2975FaultLog::FaultLogPreambleLtc2975 , LT_2977FaultLog::FaultLogPreambleLtc2977 , LT_2978FaultLog::FaultLogPreambleLtc2978 , LT_3880FaultLog::FaultLogPreambleLtc3880 , LT_3882FaultLog::FaultLogPreambleLtc3882 , LT_3883FaultLog::FaultLogPreambleLtc3883 , LT_3887FaultLog::FaultLogPreambleLtc3887
- shared_time_byte0 : LT_FaultLog::FaultLogTimeStamp
- shared_time_byte1 : LT_FaultLog::FaultLogTimeStamp
- shared_time_byte2 : LT_FaultLog::FaultLogTimeStamp
- shared_time_byte3 : LT_FaultLog::FaultLogTimeStamp
- shared_time_byte4 : LT_FaultLog::FaultLogTimeStamp
- shared_time_byte5 : LT_FaultLog::FaultLogTimeStamp
- sid : cell_asic
- slave_address : i2c_desc , i2c_init_param
- slin11_t : LT_PMBusMath
- smbus() : LT_PMBus , LT_PMBusDevice
- smbus_ : LT_SMBusARA
- SMUselected_ : EasySMU_IOpanel
- soft_span_range : eeprom_data_union::data_struct_type
- spiread() : Adafruit_ILI9341
- spiwrite() : Adafruit_ILI9341
- start_button_pressed_ : EasySMU_IOpanel
- startGroupProtocol() : LT_I2CBus , LT_PMBus
- stat : cell_asic
- stat_channels : register_cfg
- stat_codes : st
- stat_pec : pec_counter
- status_iout : LT_2974FaultLog::ChanStatus , LT_2974FaultLog::IoutData , LT_2975FaultLog::ChanStatus , LT_2975FaultLog::IoutData
- status_mfr : LT_2974FaultLog::VoutData , LT_2975FaultLog::VoutData , LT_2977FaultLog::ChanStatus , LT_2977FaultLog::VoutData , LT_2978FaultLog::VoutData
- status_mfr_specific : LT_2974FaultLog::ChanStatus , LT_2975FaultLog::ChanStatus
- status_mfr_specificP0 : LT_3880FaultLog::FaultLogReadLoopLtc3880 , LT_3882FaultLog::FaultLogReadLoopLtc3882 , LT_3883FaultLog::FaultLogReadLoopLtc3883 , LT_3887FaultLog::FaultLogReadLoopLtc3887
- status_mfr_specificP1 : LT_3880FaultLog::FaultLogReadLoopLtc3880 , LT_3882FaultLog::FaultLogReadLoopLtc3882 , LT_3887FaultLog::FaultLogReadLoopLtc3887
- status_temp : LT_2974FaultLog::TempData , LT_2975FaultLog::TempData , LT_2977FaultLog::TempData , LT_2977FaultLog::TempStatus , LT_2978FaultLog::TempData
- status_vin : LT_2974FaultLog::VinData , LT_2974FaultLog::VinStatus , LT_2975FaultLog::VinData , LT_2975FaultLog::VinStatus , LT_2977FaultLog::VinData , LT_2977FaultLog::VinStatus , LT_2978FaultLog::VinData , LT_2978FaultLog::VinStatus
- status_vout : LT_2974FaultLog::ChanStatus , LT_2974FaultLog::VoutData , LT_2975FaultLog::ChanStatus , LT_2975FaultLog::VoutData , LT_2977FaultLog::ChanStatus , LT_2977FaultLog::VoutData , LT_2978FaultLog::VoutData
- status_vout_p0 : LT_3880FaultLog::FaultLogReadLoopLtc3880 , LT_3882FaultLog::FaultLogReadLoopLtc3882 , LT_3883FaultLog::FaultLogReadLoopLtc3883 , LT_3887FaultLog::FaultLogReadLoopLtc3887
- status_vout_p1 : LT_3880FaultLog::FaultLogReadLoopLtc3880 , LT_3882FaultLog::FaultLogReadLoopLtc3882 , LT_3887FaultLog::FaultLogReadLoopLtc3887
- status_word_p0 : LT_3880FaultLog::FaultLogReadLoopLtc3880 , LT_3882FaultLog::FaultLogReadLoopLtc3882 , LT_3883FaultLog::FaultLogReadLoopLtc3883 , LT_3887FaultLog::FaultLogReadLoopLtc3887
- status_word_p1 : LT_3880FaultLog::FaultLogReadLoopLtc3880 , LT_3882FaultLog::FaultLogReadLoopLtc3882 , LT_3887FaultLog::FaultLogReadLoopLtc3887
- storeToNvm() : LT_PMBus
- storeToNvmAll() : LT_PMBus
- storeToNvmGlobal() : LT_PMBus
- system_open_wire : cell_asic