| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - v -

- VALID : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- valid_register() : LTM9100.cpp , LTM9100.h , DC1558_DC1808.ino
- values : DC2218A.ino
- var1 : DoxygenExample.h , DoxygenExample.ino
- var2 : DoxygenExample.h , DoxygenExample.ino
- vbat : DC2343A.ino
- vdiv_gain : LTC2492_Panel_Meter.ino
- verbose : LT1054_voltage_mode_buck.ino , LT1054_voltage_mode_buck_DC_ctrl.ino
- verification_in_progress : main_record_processor.cpp
- verify_nvm() : program.ino
- verifyRecordsOnDemand() : main_record_processor.cpp , main_record_processor.h
- VIN : LTC2492_original.h
- vin_cal : LTC2492_Thermocouple_Meter.ino
- VIN_OV_FAULT_LIMIT : LT_PMBus.h
- VIN_OV_WARN_LIMIT : LT_PMBus.h
- VIN_UV_FAULT_LIMIT : LT_PMBus.h
- VIN_UV_WARN_LIMIT : LT_PMBus.h
- voltage : DC2289AA.ino
- VOLTAGE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- voltage_fullscale : DC2024A.ino
- voltage_to_code() : EVAL-AD5696R.ino , EVAL-AD5686R.ino
- volts : Precision_Voltage_Source.ino
- vout : LT1054_voltage_mode_buck_DC_ctrl.ino , LT1054_voltage_mode_buck.ino
- VOUT_CH_BASE : configuration_constants_LTC2983.h , configuration_constants_LTC2984.h , configuration_constants_LTC2986.h
- VOUT_COMMAND : LT_PMBus.h
- VOUT_MARGIN_HIGH : LT_PMBus.h
- VOUT_MARGIN_LOW : LT_PMBus.h
- VOUT_MAX : LT_PMBus.h
- VOUT_MODE : LT_PMBus.h
- VOUT_OV_FAULT_LIMIT : LT_PMBus.h
- VOUT_OV_FAULT_RESPONSE : LT_PMBus.h
- VOUT_OV_WARN_LIMIT : LT_PMBus.h
- VOUT_UV_FAULT_LIMIT : LT_PMBus.h
- VOUT_UV_FAULT_RESPONSE : LT_PMBus.h
- VOUT_UV_WARN_LIMIT : LT_PMBus.h
- VREF : DC2222_interrupt_driven_read.ino , DC2222AB.ino
- vref : LTC2492_Thermocouple_Meter.ino
- VREF : LTC2348.h , DC2222AC.ino
- VREF1 : DC1096B.ino
- VREF2 : DC1096B.ino