| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
LOCKOUT_ID_PIN
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

LOCKOUT_ID_PIN Bit Field. More...

## Macros
#define | LTC4155_LOCKOUT_ID_PIN_SUBADDR LTC4155_REG0_SUBADDR
| LOCKOUT_ID_PIN More...
#define | LTC4155_LOCKOUT_ID_PIN_SIZE 1
#define | LTC4155_LOCKOUT_ID_PIN_OFFSET 5
#define | LTC4155_LOCKOUT_ID_PIN_MASK 0x20
#define | LTC4155_LOCKOUT_ID_PIN (LTC4155_LOCKOUT_ID_PIN_OFFSET << 12 | (LTC4155_LOCKOUT_ID_PIN_SIZE - 1) << 8 | LTC4155_LOCKOUT_ID_PIN_SUBADDR)

## Detailed Description

LOCKOUT_ID_PIN Bit Field.

Disables autonomous USB OTG operation when the ID pin is grounded by an appropriate USB cable.

- Register: REG0
- CommandCode: 0x00
- Size: 1
- Offset: 5
- MSB: 5
- MASK: 0x20
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_LOCKOUT_ID_PIN

#define LTC4155_LOCKOUT_ID_PIN (LTC4155_LOCKOUT_ID_PIN_OFFSET << 12 | (LTC4155_LOCKOUT_ID_PIN_SIZE - 1) << 8 | LTC4155_LOCKOUT_ID_PIN_SUBADDR)

Definition at line 159 of file LTC4155_reg_defs.h.

## ◆ LTC4155_LOCKOUT_ID_PIN_MASK

#define LTC4155_LOCKOUT_ID_PIN_MASK 0x20

Definition at line 158 of file LTC4155_reg_defs.h.

## ◆ LTC4155_LOCKOUT_ID_PIN_OFFSET

#define LTC4155_LOCKOUT_ID_PIN_OFFSET 5

Definition at line 157 of file LTC4155_reg_defs.h.

## ◆ LTC4155_LOCKOUT_ID_PIN_SIZE

#define LTC4155_LOCKOUT_ID_PIN_SIZE 1

Definition at line 156 of file LTC4155_reg_defs.h.

## ◆ LTC4155_LOCKOUT_ID_PIN_SUBADDR

#define LTC4155_LOCKOUT_ID_PIN_SUBADDR LTC4155_REG0_SUBADDR

LOCKOUT_ID_PIN

Definition at line 155 of file LTC4155_reg_defs.h.