| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
OVP_ACTIVE
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

OVP_ACTIVE Bit Field. More...

## Macros
#define | LTC4155_OVP_ACTIVE_SUBADDR LTC4155_REG4_SUBADDR
| OVP_ACTIVE More...
#define | LTC4155_OVP_ACTIVE_SIZE 1
#define | LTC4155_OVP_ACTIVE_OFFSET 2
#define | LTC4155_OVP_ACTIVE_MASK 0x04
#define | LTC4155_OVP_ACTIVE (LTC4155_OVP_ACTIVE_OFFSET << 12 | (LTC4155_OVP_ACTIVE_SIZE - 1) << 8 | LTC4155_OVP_ACTIVE_SUBADDR)

## Detailed Description

OVP_ACTIVE Bit Field.

Overvoltage protection fault.

- Register: REG4
- CommandCode: 0x04
- Size: 1
- Offset: 2
- MSB: 2
- MASK: 0x04
- Access: R
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_OVP_ACTIVE

#define LTC4155_OVP_ACTIVE (LTC4155_OVP_ACTIVE_OFFSET << 12 | (LTC4155_OVP_ACTIVE_SIZE - 1) << 8 | LTC4155_OVP_ACTIVE_SUBADDR)

Definition at line 700 of file LTC4155_reg_defs.h.

## ◆ LTC4155_OVP_ACTIVE_MASK

#define LTC4155_OVP_ACTIVE_MASK 0x04

Definition at line 699 of file LTC4155_reg_defs.h.

## ◆ LTC4155_OVP_ACTIVE_OFFSET

#define LTC4155_OVP_ACTIVE_OFFSET 2

Definition at line 698 of file LTC4155_reg_defs.h.

## ◆ LTC4155_OVP_ACTIVE_SIZE

#define LTC4155_OVP_ACTIVE_SIZE 1

Definition at line 697 of file LTC4155_reg_defs.h.

## ◆ LTC4155_OVP_ACTIVE_SUBADDR

#define LTC4155_OVP_ACTIVE_SUBADDR LTC4155_REG4_SUBADDR

OVP_ACTIVE

Definition at line 696 of file LTC4155_reg_defs.h.