| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Functions | Macros | Variables
DC2741_production_test.ino File Reference

Go to the source code of this file.

## Functions
static void | print_title ()
static void | setup ()
static void | loop ()

## Macros
#define | SW_I2C_FREQUENCY 400

## Variables
char * | descr [] = {"SCK - MISO", "MOSI - MISO", "CS - MISO", "IO2 - AD0", "IO3~ - AD1", "IO4 - AD2", "IO5 - AD3"}
const uint8_t | stimulus [7] = {13, 11, QUIKEVAL_CS, 2, 3, 4, 5}
const uint8_t | readback [7] = {12, 12, 12 , 0, 1, 2, 3}

## Function Documentation

## ◆ loop()

static void loop | ( | void |  | ) |
| static

Definition at line 116 of file DC2741_production_test.ino.

## ◆ print_title()

static void print_title | ( | void |  | ) |
| static

Definition at line 82 of file DC2741_production_test.ino.

## ◆ setup()

static void setup | ( | void |  | ) |
| static

Definition at line 94 of file DC2741_production_test.ino.

## Macro Definition Documentation

## ◆ SW_I2C_FREQUENCY

#define SW_I2C_FREQUENCY 400

Definition at line 59 of file DC2741_production_test.ino.

## Variable Documentation

## ◆ descr

char* descr[] = {"SCK - MISO", "MOSI - MISO", "CS - MISO", "IO2 - AD0", "IO3~ - AD1", "IO4 - AD2", "IO5 - AD3"}

Definition at line 70 of file DC2741_production_test.ino.

## ◆ readback

const uint8_t readback[7] = {12, 12, 12 , 0, 1, 2, 3}

Definition at line 80 of file DC2741_production_test.ino.

## ◆ stimulus

const uint8_t stimulus[7] = {13, 11, QUIKEVAL_CS, 2, 3, 4, 5}

Definition at line 79 of file DC2741_production_test.ino.