| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

### - i -

- i2c_acread() : LT3965.cpp , LT3965.h
- i2c_acwrite() : LT3965.h , LT3965.cpp
- i2c_bcread() : LT3965.cpp , LT3965.h
- i2c_enable() : LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h , LT_I2C.cpp
- i2c_init() : platform_drivers.cpp , platform_drivers.h
- i2c_poll() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h
- i2c_read() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h , platform_drivers.cpp , platform_drivers.h
- i2c_read_block_data() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_read_byte() : LT_I2C_Wire.h , LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp
- i2c_read_byte_data() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_read_word_data() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_remove() : platform_drivers.cpp , platform_drivers.h
- i2c_repeated_start() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h
- i2c_scwritelong() : LT3965.cpp , LT3965.h
- i2c_scwriteshort() : LT3965.cpp , LT3965.h
- i2c_scwriteshort_scread() : LT3965.cpp , LT3965.h
- i2c_start() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h
- i2c_stop() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h
- i2c_two_byte_command_read_block() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_write() : LT_I2C_Wire.h , platform_drivers.cpp , platform_drivers.h , LT_I2C.cpp , LT_I2C.h
- i2c_write_block_data() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.cpp , LT_I2C_Wire.h
- i2c_write_block_data_no_command() : DC2222AC.ino , DC2222AB.ino
- i2c_write_byte() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h , LT_I2C_Wire.cpp
- i2c_write_byte_data() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h , LT_I2C_Wire.cpp
- i2c_write_word_data() : LT_I2C.cpp , LT_I2C.h , LT_I2C_Wire.h , LT_I2C_Wire.cpp
- increment_counter() : retention.ino
- increment_page() : DC1978.ino
- init64() : LTC6948.h , LTC6946.cpp , LTC6948.cpp , LTC6945.h , LTC6946.h , LTC6945.cpp , LTC6947.h , LTC6950.h , LTC6950.cpp , LTC6947.cpp
- init_16_bit_PWM() : Margining.ino , DC2197.ino
- init_cfg() : DC1652A.ino , DC1942.ino , DC1894.ino , DC1651A.ino
- init_dac() : Precision_Voltage_Source.ino
- init_gain_pins() : DC1410AB.ino , DC1410AA.ino
- initialise_i2c_data() : DC2222AB.ino , DC2222_interrupt_driven_read.ino , DC2222AC.ino
- initialize() : LTC2492_original.h
- is_ltc2977() : retention.ino
- is_ltc2978() : retention.ino
- is_ltc297x() : retention.ino
- is_number_in_array() : support_functions_LTC2983.h , support_functions_LTC2984.h , support_functions_LTC2983.cpp , support_functions_LTC2986.h , support_functions_LTC2984.cpp , support_functions_LTC2986.cpp
- isBitSet() : DC1496BB.ino , DC1812A-B.ino , DC1812AA.ino
- ISR() : DC2839A.ino
- ith_decimal2hex() : DC2155A.ino
- ith_hex2decimal() : DC2155A.ino
- ith_nearest_legal_value() : DC2155A.ino