| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Public Member Functions
Adafruit_FT6206 Class Reference

## Detailed Description

Definition at line 61 of file Adafruit_FT6206.h.

## Public Member Functions
| Adafruit_FT6206 (void)
| Instantiates a new FT6206 class. More...
boolean | begin (uint8_t thresh=FT6206_DEFAULT_THRESSHOLD)
| Setups the HW. More...
void | writeRegister8 (uint8_t reg, uint8_t val)
uint8_t | readRegister8 (uint8_t reg)
void | readData (uint16_t *x, uint16_t *y)
void | autoCalibrate (void)
boolean | touched (void)
TS_Point | getPoint (void)

## Member Function Documentation

## ◆ autoCalibrate()

void Adafruit_FT6206::autoCalibrate | ( | void |  | ) |

Definition at line 74 of file Adafruit_FT6206.cpp.

## ◆ begin()

boolean Adafruit_FT6206::begin | ( | uint8_t | thresh = `FT6206_DEFAULT_THRESSHOLD` | ) |

Setups the HW.

Definition at line 48 of file Adafruit_FT6206.cpp.

## ◆ getPoint()

TS_Point Adafruit_FT6206::getPoint | ( | void |  | ) |

Definition at line 184 of file Adafruit_FT6206.cpp.

## ◆ readData()

void Adafruit_FT6206::readData | ( | uint16_t * | x,
|  | uint16_t * | y
| ) |  |

Definition at line 112 of file Adafruit_FT6206.cpp.

## ◆ readRegister8()

uint8_t Adafruit_FT6206::readRegister8 | ( | uint8_t | reg | ) |

Definition at line 193 of file Adafruit_FT6206.cpp.

## ◆ touched()

boolean Adafruit_FT6206::touched | ( | void |  | ) |

Definition at line 102 of file Adafruit_FT6206.cpp.

## ◆ writeRegister8()

void Adafruit_FT6206::writeRegister8 | ( | uint8_t | reg,
|  | uint8_t | val
| ) |  |

Definition at line 211 of file Adafruit_FT6206.cpp.

## Constructor & Destructor Documentation

## ◆ Adafruit_FT6206()

Adafruit_FT6206::Adafruit_FT6206 | ( | void |  | ) |

Instantiates a new FT6206 class.

Definition at line 38 of file Adafruit_FT6206.cpp.

The documentation for this class was generated from the following files:

- Adafruit_FT6206.h
- Adafruit_FT6206.cpp