| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
EN_BAT_CONDITIONER
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

EN_BAT_CONDITIONER Bit Field. More...

## Macros
#define | LTC4155_EN_BAT_CONDITIONER_SUBADDR LTC4155_REG0_SUBADDR
| EN_BAT_CONDITIONER More...
#define | LTC4155_EN_BAT_CONDITIONER_SIZE 1
#define | LTC4155_EN_BAT_CONDITIONER_OFFSET 6
#define | LTC4155_EN_BAT_CONDITIONER_MASK 0x40
#define | LTC4155_EN_BAT_CONDITIONER (LTC4155_EN_BAT_CONDITIONER_OFFSET << 12 | (LTC4155_EN_BAT_CONDITIONER_SIZE - 1) << 8 | LTC4155_EN_BAT_CONDITIONER_SUBADDR)

## Detailed Description

EN_BAT_CONDITIONER Bit Field.

Enables autonomous Overtemperature Battery Conditioner Load when the thermistor temperature exceeds 60°C.

- Register: REG0
- CommandCode: 0x00
- Size: 1
- Offset: 6
- MSB: 6
- MASK: 0x40
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_EN_BAT_CONDITIONER

#define LTC4155_EN_BAT_CONDITIONER (LTC4155_EN_BAT_CONDITIONER_OFFSET << 12 | (LTC4155_EN_BAT_CONDITIONER_SIZE - 1) << 8 | LTC4155_EN_BAT_CONDITIONER_SUBADDR)

Definition at line 138 of file LTC4155_reg_defs.h.

## ◆ LTC4155_EN_BAT_CONDITIONER_MASK

#define LTC4155_EN_BAT_CONDITIONER_MASK 0x40

Definition at line 137 of file LTC4155_reg_defs.h.

## ◆ LTC4155_EN_BAT_CONDITIONER_OFFSET

#define LTC4155_EN_BAT_CONDITIONER_OFFSET 6

Definition at line 136 of file LTC4155_reg_defs.h.

## ◆ LTC4155_EN_BAT_CONDITIONER_SIZE

#define LTC4155_EN_BAT_CONDITIONER_SIZE 1

Definition at line 135 of file LTC4155_reg_defs.h.

## ◆ LTC4155_EN_BAT_CONDITIONER_SUBADDR

#define LTC4155_EN_BAT_CONDITIONER_SUBADDR LTC4155_REG0_SUBADDR

EN_BAT_CONDITIONER

Definition at line 134 of file LTC4155_reg_defs.h.