| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Data Structures | Macros | Enumerations
LT_PMBus.h File Reference
PMBus and SMBus Support Libraries » LT_PMBus: PMBus commands

LTC PMBus Support. More...

## Detailed Description

LTC PMBus Support.

    This PMBus code does not cover the entire PMBus command set. The intention
    is to cover the common commands. It was written for LTC PMBus devices,
    and may not perform properly with other PMBus devices.

Copyright 2018(c) Analog Devices, Inc.

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

- Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.
- Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.
- Neither the name of Analog Devices, Inc. nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.
- The use of this software may or may not infringe the patent rights of one or more patent holders. This license does not release you from the requirement that you obtain separate licenses from these patent holders to use this software.
- Use of the software either in source or binary form, must be run on or directly connected to an Analog Devices Inc. component.

THIS SOFTWARE IS PROVIDED BY ANALOG DEVICES "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, NON-INFRINGEMENT, MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL ANALOG DEVICES BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, INTELLECTUAL PROPERTY RIGHTS, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Library Header File for LT_PMBus

Definition in file LT_PMBus.h.

Go to the source code of this file.

## Data Structures
class | LT_PMBus
| PMBus communication. More...

## Macros
#define | SUCCESS 1
#define | FAILURE 0
#define | PAGE 0x00
#define | OPERATION 0x01
#define | ON_OFF_CONFIG 0x02
#define | CLEAR_FAULTS 0x03
#define | PAGE_PLUS_WRITE 0x05
#define | PAGE_PLUS_READ 0x06
#define | WRITE_PROTECT 0x10
#define | STORE_USER_ALL 0x15
#define | RESTORE_USER_ALL 0x16
#define | MFR_COMPARE_USER_ALL 0xF0
#define | SMBALERT_MASK 0x1B
#define | VOUT_MODE 0x20
#define | VOUT_COMMAND 0x21
#define | VOUT_MAX 0x24
#define | VOUT_MARGIN_HIGH 0x25
#define | VOUT_MARGIN_LOW 0x26
#define | VOUT_OV_FAULT_LIMIT 0x40
#define | VOUT_OV_FAULT_RESPONSE 0x41
#define | VOUT_OV_WARN_LIMIT 0x42
#define | VOUT_UV_WARN_LIMIT 0x43
#define | VOUT_UV_FAULT_LIMIT 0x44
#define | VOUT_UV_FAULT_RESPONSE 0x45
#define | IOUT_OC_FAULT_LIMIT 0x46
#define | IOUT_OC_WARN_LIMIT 0x4A
#define | OT_FAULT_LIMIT 0x4F
#define | OT_WARN_LIMIT 0x51
#define | UT_FAULT_LIMIT 0x53
#define | UT_WARN_LIMIT 0x52
#define | VIN_OV_FAULT_LIMIT 0x55
#define | VIN_OV_WARN_LIMIT 0x57
#define | VIN_UV_WARN_LIMIT 0x58
#define | VIN_UV_FAULT_LIMIT 0x59
#define | TON_DELAY 0x60
#define | TON_RISE 0x61
#define | TON_MAX_FAULT_LIMIT 0x62
#define | TON_MAX_FAULT_RESPONSE 0x63
#define | TOFF_DELAY 0x64
#define | TOFF_FALL 0x65
#define | TOFF_MAX_WARN_LIMIT 0x66
#define | IIN_OC_WARN_LIMIT 0x5D
#define | STATUS_BYTE 0x78
#define | STATUS_WORD 0x79
#define | STATUS_VOUT 0x7A
#define | STATUS_IOUT 0x7B
#define | STATUS_INPUT 0x7C
#define | STATUS_TEMP 0X7D
#define | STATUS_CML 0x7E
#define | STATUS_MFR_SPECIFIC 0x80
#define | READ_VIN 0x88
#define | READ_IIN 0x89
#define | READ_VOUT 0x8B
#define | READ_IOUT 0x8C
#define | READ_OTEMP 0x8D
#define | READ_ITEMP 0x8E
#define | READ_DUTY_CYCLE 0x94
#define | READ_POUT 0x96
#define | READ_PIN 0x97
#define | MFR_MODEL 0x9A
#define | USER_DATA_03 0xB3
#define | USER_DATA_04 0xB4
#define | MFR_EE_UNLOCK 0xBD
#define | MFR_EE_ERASE 0xBE
#define | MFR_EE_DATA 0xBF
#define | MFR_CONFIG_LTC2974 0xD0
#define | MFR_CONFIG_ALL 0xD1
#define | MFR_WATCHDOG_T_FIRST 0xE2
#define | MFR_WATCHDOG_T 0xE3
#define | MFR_PADS 0xE5
#define | MFR_ADDRESS 0xE6
#define | MFR_SPECIAL_ID 0xE7
#define | MFR_FAULT_LOG_STORE 0xEA
#define | MFR_FAULT_LOG_RESTORE 0xEB
#define | MFR_FAULT_LOG_CLEAR 0xEC
#define | MFR_READ_IIN 0xED
#define | MFR_FAULT_LOG_STATUS 0xED
#define | MFR_FAULT_LOG 0xEE
#define | MFR_COMMON 0xEF
#define | MFR_SPARE_0 0xF7
#define | MFR_SPARE_1 0xF8
#define | MFR_SPARE_2 0xF9
#define | MFR_SPARE_3 0xFA
#define | MFR_TEMP_1_GAIN 0xF8
#define | MFR_TEMP_1_OFFSET 0xF9
#define | MFR_EEPROM_STATUS 0xF1
#define | MFR_RAIL_ADDRESS 0xFA
#define | MFR_RESET 0xFD
#define | LTC3880_SW_NONE 0x0001
#define | LTC3880_SW_CML 0x0002
#define | LTC3880_SW_TEMP 0x0004
#define | LTC3880_SW_IOUT_OC 0x0010
#define | LTC3880_SW_VOUT_OV 0x0020
#define | LTC3880_SW_OFF 0x0040
#define | LTC3880_SW_BUSY 0x0080
#define | LTC3880_SW_PGOODB 0x0800
#define | LTC3880_SW_MFR 0x1000
#define | LTC3880_SW_INPUT 0x2000
#define | LTC3880_SW_IOUT_POUT 0x4000
#define | LTC3880_SW_VOUT 0x8000
#define | CFGALL_EFL 0x0080
#define | LTC3880_CFGALL_RUN_CLR 0x0001
#define | LTC3880_CFGALL_CLK_STR 0x0002
#define | LTC3880_CFGALL_MASK_PLL_FLT 0x0004
#define | LTC3880_CFGALL_IGNORE_RCFG 0x0040
#define | LTC3880_CFGALL_EFL 0x0080
#define | LTC3880_SMFR_EXT_GPIO 0x0001
#define | LTC3880_SMFR_VDD_UV_OV 0x0004
#define | LTC3880_SMFR_FAULT_LOG 0x0008
#define | LTC3880_SMFR_PLL_UNLOCK 0x0010
#define | LTC3880_SMFR_NVM_CRC 0x0020
#define | LTC3880_SMFR_TEMP_WARN 0x0040
#define | LTC3880_SMFR_TEMP_FAULT 0x0080
#define | LTC3882_CFGALL_RUN_CLR_RISE 0x0001
#define | LTC3882_CFGALL_CLK_STR 0x0002
#define | LTC3882_CFGALL_PEC 0x0004
#define | LTC3882_CFGALL_255MS_TMO 0x0008
#define | LTC3882_CFGALL_DISABLE_SYNC 0x0010
#define | LTC3882_CFGALL_IGNORE_RCFG 0x0040
#define | LTC3882_CFGALL_EFL 0x0080
#define | LTC3882_SMFR_EXT_GPIO 0x0001
#define | LTC3882_SMFR_SHORT_CYCLE 0x0002
#define | LTC3882_SMFR_FAULT_LOG 0x0008
#define | LTC3882_SMFR_PLL_UNLOCK 0x0010
#define | LTC3882_SMFR_NVM_CRC 0x0020
#define | LTC3882_SMFR_TEMP_WARN 0x0040
#define | LTC3882_SMFR_TEMP_FAULT 0x0080
#define | LTC3883_CFGALL_CLK_STR 0x0002
#define | LTC3883_CFGALL_PEC 0x0004
#define | LTC3883_CFGALL_MASK_PLL_ULOCK 0x0008
#define | LTC3883_CFGALL_IGNORE_RCFG 0x0040
#define | LTC3883_CFGALL_EFL 0x0080
#define | LTC3887_CFGALL_RUN_CLR_RISE 0x0001
#define | LTC3887_CFGALL_CLK_STR 0x0002
#define | LTC3887_CFGALL_PEC 0x0004
#define | LTC3887_CFGALL_255MS_TMO 0x0008
#define | LTC3887_CFGALL_DISABLE_SYNC 0x0010
#define | LTC3887_CFGALL_IGNORE_RCFG 0x0040
#define | LTC3887_CFGALL_EFL 0x0080
#define | LTC3887_SMFR_EXT_GPIO 0x0001
#define | LTC3887_SMFR_SHORT_CYCLE 0x0002
#define | LTC3887_SMFR_FAULT_LOG 0x0008
#define | LTC3887_SMFR_PLL_UNLOCK 0x0010
#define | LTC3887_SMFR_NVM_CRC 0x0020
#define | LTC3887_SMFR_TEMP_WARN 0x0040
#define | LTC3887_SMFR_TEMP_FAULT 0x0080
#define | LTC3883_SMFR_EXT_GPIO 0x0001
#define | LTC3883_SMFR_VDD_UV_OV 0x0004
#define | LTC3883_SMFR_FAULT_LOG 0x0008
#define | LTC3883_SMFR_PLL_UNLOCK 0x0010
#define | LTC3883_SMFR_NVM_CRC 0x0020
#define | LTC3883_SMFR_TEMP_WARN 0x0040
#define | LTC3883_SMFR_TEMP_FAULT 0x0080
#define | LTC2972_SFL_EEPROM 0x0001
#define | LTC2974_SW_HIGH_BYTE 0x0001
#define | LTC2974_SW_CML 0x0002
#define | LTC2974_SW_TEMP 0x0004
#define | LTC2974_SW_VIN_UV 0x0008
#define | LTC2974_SW_IOUT_OC 0x0010
#define | LTC2974_SW_VOUT_OV 0x0020
#define | LTC2974_SW_OFF 0x0040
#define | LTC2974_SW_BUSY 0x0080
#define | LTC2974_SW_FANS 0x0400
#define | LTC2974_SW_PGOODB 0x0800
#define | LTC2974_SW_MFR 0x1000
#define | LTC2974_SW_INPUT 0x2000
#define | LTC2974_SW_IOUT 0x4000
#define | LTC2974_SW_VOUT 0x8000
#define | LTC2974_CFGALL_AUX_FB_WPU 0x0001
#define | LTC2974_CFGALL_PMBUS_TIMO 0x0002
#define | LTC2974_CFGALL_PEC 0x0004
#define | LTC2974_CFGALL_VIN_SHARE 0x0008
#define | LTC2974_CFGALL_CRTL0_POL 0x0010
#define | LTC2974_CFGALL_CTRL1_POL 0x0020
#define | LTC2974_CFGALL_VIN_ON_CLR_FLT 0x0040
#define | LTC2974_CFGALL_EFL 0x0080
#define | LTC2974_CFGALL_CNTL2_POL 0x0100
#define | LTC2974_CFGALL_CNTL3_POL 0x0200
#define | LTC2974_CFGALL_FAST_FLAG 0x0400
#define | LTC2974_CFGALL_PGOOD_OFF_UV 0x0800
#define | LTC2974_CFG_DAC_POL 0x0001
#define | LTC2974_CFG_DAC_GAIN 0x0002
#define | LTC2974_CFG_VO_EN_WPD 0x0004
#define | LTC2974_CFG_VO_EN_WPU 0x0008
#define | LTC2974_CFG_SRVO_ON_WARN 0x0040
#define | LTC2974_CFG_SVRO_CONT 0x0080
#define | LTC2974_CFG_SUP_RES 0x0400
#define | LTC2974_CFG_FAST_SERVO 0x0800
#define | LTC2974_CFG_CASCADE_ON 0x4000
#define | LTC2974_SMFR_WATCH_DOG 0x0001
#define | LTC2974_SMFR_AUX_FAULT 0x0002
#define | LTC2974_CFG_ALL_DAC_MODE 0x0030
#define | LTC2974_SMFR_DAC_SAT 0x0004
#define | LTC2974_SMFR_DAC_CON 0x0008
#define | LTC2974_SMFR_SERVO_TGT 0x0010
#define | LTC2974_SMFR_FAULT0_IN 0x0020
#define | LTC2974_SMFR_FAULT1_IN 0x0040
#define | LTC2974_SMFR_DISCHARGE 0x0080
#define | LTC2974_SFL_EEPROM 0x0001
#define | LTC2974_SFL_RAM 0x0002
#define | LTC2975_SFL_EEPROM 0x0001
#define | LTC2977_SFL_EEPROM 0x0001
#define | LTC2977_SFL_RAM 0x0002
#define | LTC2978_SW_HIGH_BYTE 0x0001
#define | LTC2978_SW_CML 0x0002
#define | LTC2978_SW_TEMP 0x0004
#define | LTC2978_SW_VIN_UV 0x0008
#define | LTC2978_SW_IOUT_OC 0x0010
#define | LTC2978_SW_VOUT_OV 0x0020
#define | LTC2978_SW_OFF 0x0040
#define | LTC2978_SW_BUSY 0x0080
#define | LTC2978_SW_FANS 0x0400
#define | LTC2978_SW_PGOODB 0x0800
#define | LTC2978_SW_MFR 0x1000
#define | LTC2978_SW_INPUT 0x2000
#define | LTC2978_SW_IOUT 0x4000
#define | LTC2978_SW_VOUT 0x8000
#define | LTC2978_CFGALL_AUX_FB_WPU 0x0001
#define | LTC2978_CFGALL_PMBUS_TIMO 0x0002
#define | LTC2978_CFGALL_PEC 0x0004
#define | LTC2978_CFGALL_VIN_SHARE 0x0008
#define | LTC2978_CFGALL_CRTL0_POL 0x0010
#define | LTC2978_CFGALL_CTRL1_POL 0x0020
#define | LTC2978_CFGALL_VIN_ON_CLR_FLT 0x0040
#define | LTC2978_CFGALL_EFL 0x0080
#define | LTC2978_CFGALL_FAST_FLAG 0x0400
#define | LTC2978_CFGALL_PGOOD_OFF_UV 0x0800
#define | LTC2978_CFGALL_SHORT_CYC_FAULT 0x1000
#define | LTC2978_CFG_DAC_POL 0x0001
#define | LTC2978_CFG_DAC_GAIN 0x0002
#define | LTC2978_CFG_VO_EN_WPD 0x0004
#define | LTC2978_CFG_VO_EN_WPU 0x0008
#define | LTC2978_CFG_DAC_MODE 0x0030
#define | LTC2978_CFG_SRVO_ON_WARN 0x0040
#define | LTC2978_CFG_SVRO_CONT 0x0080
#define | LTC2978_CFG_CNTL_IN_SEL 0x0100
#define | LTC2978_CFG_ADC_RES 0x0200
#define | LTC2978_CFG_SUP_RES 0x0400
#define | LTC2978_CFG_FAST_SERVO 0x0800
#define | LTC2978_CFG_CHAN_MODE 0xC000
#define | LTC2978_SMFR_WATCH_DOG 0x0001
#define | LTC2978_SMFR_VIN_EN 0x0002
#define | LTC2978_SMFR_DAC_SAT 0x0004
#define | LTC2978_SMFR_DAC_CON 0x0008
#define | LTC2978_SMFR_SERVO_TGT 0x0010
#define | LTC2978_SMFR_FAULT0_IN 0x0020
#define | LTC2978_SMFR_FAULT1_IN 0x0040
#define | LTC2978_SMFR_DISCHARGE 0x0080
#define | LTC2978_SFL_EEPROM 0x0001
#define | LTC2978_SFL_RAM 0x0002
#define | STATUS_CML_CMD_FAULT 0x80
#define | STATUS_CML_DATA_FAULT 0x40
#define | STATUS_CML_PEC_FAULT 0x20
#define | STATUS_CML_MEM_FAULT 0x10
#define | STATUS_CML_PROC_FAULT 0x04
#define | STATUS_CML_PMBUS_FAULT 0x02
#define | STATUS_CML_UNKNOWN_FAULT 0x01

## Enumerations
enum | PsmDeviceType { LTC3880, LTC3882, LTC3882_1, LTC3883, LTC3884, LTC3886, LTC3887, LTM4675, LTM4676, LTM4676A, LTM4677, LTC2974, LTC2975, LTC2977, LTC2978, LTC2980, LTM2987, LTCUnknown }

## Macro Definition Documentation

## ◆ CFGALL_EFL

#define CFGALL_EFL 0x0080

Definition at line 165 of file LT_PMBus.h.

## ◆ CLEAR_FAULTS

#define CLEAR_FAULTS 0x03

Definition at line 68 of file LT_PMBus.h.

## ◆ FAILURE

#define FAILURE 0

Definition at line 63 of file LT_PMBus.h.

## ◆ IIN_OC_WARN_LIMIT

#define IIN_OC_WARN_LIMIT 0x5D

Definition at line 104 of file LT_PMBus.h.

## ◆ IOUT_OC_FAULT_LIMIT

#define IOUT_OC_FAULT_LIMIT 0x46

Definition at line 87 of file LT_PMBus.h.

## ◆ IOUT_OC_WARN_LIMIT

#define IOUT_OC_WARN_LIMIT 0x4A

Definition at line 88 of file LT_PMBus.h.

## ◆ LTC2972_SFL_EEPROM

#define LTC2972_SFL_EEPROM 0x0001

Definition at line 227 of file LT_PMBus.h.

## ◆ LTC2974_CFG_ALL_DAC_MODE

#define LTC2974_CFG_ALL_DAC_MODE 0x0030

Definition at line 269 of file LT_PMBus.h.

## ◆ LTC2974_CFG_CASCADE_ON

#define LTC2974_CFG_CASCADE_ON 0x4000

Definition at line 265 of file LT_PMBus.h.

## ◆ LTC2974_CFG_DAC_GAIN

#define LTC2974_CFG_DAC_GAIN 0x0002

Definition at line 258 of file LT_PMBus.h.

## ◆ LTC2974_CFG_DAC_POL

#define LTC2974_CFG_DAC_POL 0x0001

Definition at line 257 of file LT_PMBus.h.

## ◆ LTC2974_CFG_FAST_SERVO

#define LTC2974_CFG_FAST_SERVO 0x0800

Definition at line 264 of file LT_PMBus.h.

## ◆ LTC2974_CFG_SRVO_ON_WARN

#define LTC2974_CFG_SRVO_ON_WARN 0x0040

Definition at line 261 of file LT_PMBus.h.

## ◆ LTC2974_CFG_SUP_RES

#define LTC2974_CFG_SUP_RES 0x0400

Definition at line 263 of file LT_PMBus.h.

## ◆ LTC2974_CFG_SVRO_CONT

#define LTC2974_CFG_SVRO_CONT 0x0080

Definition at line 262 of file LT_PMBus.h.

## ◆ LTC2974_CFG_VO_EN_WPD

#define LTC2974_CFG_VO_EN_WPD 0x0004

Definition at line 259 of file LT_PMBus.h.

## ◆ LTC2974_CFG_VO_EN_WPU

#define LTC2974_CFG_VO_EN_WPU 0x0008

Definition at line 260 of file LT_PMBus.h.

## ◆ LTC2974_CFGALL_AUX_FB_WPU

#define LTC2974_CFGALL_AUX_FB_WPU 0x0001

Definition at line 244 of file LT_PMBus.h.

## ◆ LTC2974_CFGALL_CNTL2_POL

#define LTC2974_CFGALL_CNTL2_POL 0x0100

Definition at line 252 of file LT_PMBus.h.

## ◆ LTC2974_CFGALL_CNTL3_POL

#define LTC2974_CFGALL_CNTL3_POL 0x0200

Definition at line 253 of file LT_PMBus.h.

## ◆ LTC2974_CFGALL_CRTL0_POL

#define LTC2974_CFGALL_CRTL0_POL 0x0010

Definition at line 248 of file LT_PMBus.h.

## ◆ LTC2974_CFGALL_CTRL1_POL

#define LTC2974_CFGALL_CTRL1_POL 0x0020

Definition at line 249 of file LT_PMBus.h.

## ◆ LTC2974_CFGALL_EFL

#define LTC2974_CFGALL_EFL 0x0080

Definition at line 251 of file LT_PMBus.h.

## ◆ LTC2974_CFGALL_FAST_FLAG

#define LTC2974_CFGALL_FAST_FLAG 0x0400

Definition at line 254 of file LT_PMBus.h.

## ◆ LTC2974_CFGALL_PEC

#define LTC2974_CFGALL_PEC 0x0004

Definition at line 246 of file LT_PMBus.h.

## ◆ LTC2974_CFGALL_PGOOD_OFF_UV

#define LTC2974_CFGALL_PGOOD_OFF_UV 0x0800

Definition at line 255 of file LT_PMBus.h.

## ◆ LTC2974_CFGALL_PMBUS_TIMO

#define LTC2974_CFGALL_PMBUS_TIMO 0x0002

Definition at line 245 of file LT_PMBus.h.

## ◆ LTC2974_CFGALL_VIN_ON_CLR_FLT

#define LTC2974_CFGALL_VIN_ON_CLR_FLT 0x0040

Definition at line 250 of file LT_PMBus.h.

## ◆ LTC2974_CFGALL_VIN_SHARE

#define LTC2974_CFGALL_VIN_SHARE 0x0008

Definition at line 247 of file LT_PMBus.h.

## ◆ LTC2974_SFL_EEPROM

#define LTC2974_SFL_EEPROM 0x0001

Definition at line 277 of file LT_PMBus.h.

## ◆ LTC2974_SFL_RAM

#define LTC2974_SFL_RAM 0x0002

Definition at line 278 of file LT_PMBus.h.

## ◆ LTC2974_SMFR_AUX_FAULT

#define LTC2974_SMFR_AUX_FAULT 0x0002

Definition at line 268 of file LT_PMBus.h.

## ◆ LTC2974_SMFR_DAC_CON

#define LTC2974_SMFR_DAC_CON 0x0008

Definition at line 271 of file LT_PMBus.h.

## ◆ LTC2974_SMFR_DAC_SAT

#define LTC2974_SMFR_DAC_SAT 0x0004

Definition at line 270 of file LT_PMBus.h.

## ◆ LTC2974_SMFR_DISCHARGE

#define LTC2974_SMFR_DISCHARGE 0x0080

Definition at line 275 of file LT_PMBus.h.

## ◆ LTC2974_SMFR_FAULT0_IN

#define LTC2974_SMFR_FAULT0_IN 0x0020

Definition at line 273 of file LT_PMBus.h.

## ◆ LTC2974_SMFR_FAULT1_IN

#define LTC2974_SMFR_FAULT1_IN 0x0040

Definition at line 274 of file LT_PMBus.h.

## ◆ LTC2974_SMFR_SERVO_TGT

#define LTC2974_SMFR_SERVO_TGT 0x0010

Definition at line 272 of file LT_PMBus.h.

## ◆ LTC2974_SMFR_WATCH_DOG

#define LTC2974_SMFR_WATCH_DOG 0x0001

Definition at line 267 of file LT_PMBus.h.

## ◆ LTC2974_SW_BUSY

#define LTC2974_SW_BUSY 0x0080

Definition at line 236 of file LT_PMBus.h.

## ◆ LTC2974_SW_CML

#define LTC2974_SW_CML 0x0002

Definition at line 230 of file LT_PMBus.h.

## ◆ LTC2974_SW_FANS

#define LTC2974_SW_FANS 0x0400

Definition at line 237 of file LT_PMBus.h.

## ◆ LTC2974_SW_HIGH_BYTE

#define LTC2974_SW_HIGH_BYTE 0x0001

Definition at line 229 of file LT_PMBus.h.

## ◆ LTC2974_SW_INPUT

#define LTC2974_SW_INPUT 0x2000

Definition at line 240 of file LT_PMBus.h.

## ◆ LTC2974_SW_IOUT

#define LTC2974_SW_IOUT 0x4000

Definition at line 241 of file LT_PMBus.h.

## ◆ LTC2974_SW_IOUT_OC

#define LTC2974_SW_IOUT_OC 0x0010

Definition at line 233 of file LT_PMBus.h.

## ◆ LTC2974_SW_MFR

#define LTC2974_SW_MFR 0x1000

Definition at line 239 of file LT_PMBus.h.

## ◆ LTC2974_SW_OFF

#define LTC2974_SW_OFF 0x0040

Definition at line 235 of file LT_PMBus.h.

## ◆ LTC2974_SW_PGOODB

#define LTC2974_SW_PGOODB 0x0800

Definition at line 238 of file LT_PMBus.h.

## ◆ LTC2974_SW_TEMP

#define LTC2974_SW_TEMP 0x0004

Definition at line 231 of file LT_PMBus.h.

## ◆ LTC2974_SW_VIN_UV

#define LTC2974_SW_VIN_UV 0x0008

Definition at line 232 of file LT_PMBus.h.

## ◆ LTC2974_SW_VOUT

#define LTC2974_SW_VOUT 0x8000

Definition at line 242 of file LT_PMBus.h.

## ◆ LTC2974_SW_VOUT_OV

#define LTC2974_SW_VOUT_OV 0x0020

Definition at line 234 of file LT_PMBus.h.

## ◆ LTC2975_SFL_EEPROM

#define LTC2975_SFL_EEPROM 0x0001

Definition at line 280 of file LT_PMBus.h.

## ◆ LTC2977_SFL_EEPROM

#define LTC2977_SFL_EEPROM 0x0001

Definition at line 282 of file LT_PMBus.h.

## ◆ LTC2977_SFL_RAM

#define LTC2977_SFL_RAM 0x0002

Definition at line 283 of file LT_PMBus.h.

## ◆ LTC2978_CFG_ADC_RES

#define LTC2978_CFG_ADC_RES 0x0200

Definition at line 320 of file LT_PMBus.h.

## ◆ LTC2978_CFG_CHAN_MODE

#define LTC2978_CFG_CHAN_MODE 0xC000

Definition at line 323 of file LT_PMBus.h.

## ◆ LTC2978_CFG_CNTL_IN_SEL

#define LTC2978_CFG_CNTL_IN_SEL 0x0100

Definition at line 319 of file LT_PMBus.h.

## ◆ LTC2978_CFG_DAC_GAIN

#define LTC2978_CFG_DAC_GAIN 0x0002

Definition at line 313 of file LT_PMBus.h.

## ◆ LTC2978_CFG_DAC_MODE

#define LTC2978_CFG_DAC_MODE 0x0030

Definition at line 316 of file LT_PMBus.h.

## ◆ LTC2978_CFG_DAC_POL

#define LTC2978_CFG_DAC_POL 0x0001

Definition at line 312 of file LT_PMBus.h.

## ◆ LTC2978_CFG_FAST_SERVO

#define LTC2978_CFG_FAST_SERVO 0x0800

Definition at line 322 of file LT_PMBus.h.

## ◆ LTC2978_CFG_SRVO_ON_WARN

#define LTC2978_CFG_SRVO_ON_WARN 0x0040

Definition at line 317 of file LT_PMBus.h.

## ◆ LTC2978_CFG_SUP_RES

#define LTC2978_CFG_SUP_RES 0x0400

Definition at line 321 of file LT_PMBus.h.

## ◆ LTC2978_CFG_SVRO_CONT

#define LTC2978_CFG_SVRO_CONT 0x0080

Definition at line 318 of file LT_PMBus.h.

## ◆ LTC2978_CFG_VO_EN_WPD

#define LTC2978_CFG_VO_EN_WPD 0x0004

Definition at line 314 of file LT_PMBus.h.

## ◆ LTC2978_CFG_VO_EN_WPU

#define LTC2978_CFG_VO_EN_WPU 0x0008

Definition at line 315 of file LT_PMBus.h.

## ◆ LTC2978_CFGALL_AUX_FB_WPU

#define LTC2978_CFGALL_AUX_FB_WPU 0x0001

Definition at line 300 of file LT_PMBus.h.

## ◆ LTC2978_CFGALL_CRTL0_POL

#define LTC2978_CFGALL_CRTL0_POL 0x0010

Definition at line 304 of file LT_PMBus.h.

## ◆ LTC2978_CFGALL_CTRL1_POL

#define LTC2978_CFGALL_CTRL1_POL 0x0020

Definition at line 305 of file LT_PMBus.h.

## ◆ LTC2978_CFGALL_EFL

#define LTC2978_CFGALL_EFL 0x0080

Definition at line 307 of file LT_PMBus.h.

## ◆ LTC2978_CFGALL_FAST_FLAG

#define LTC2978_CFGALL_FAST_FLAG 0x0400

Definition at line 308 of file LT_PMBus.h.

## ◆ LTC2978_CFGALL_PEC

#define LTC2978_CFGALL_PEC 0x0004

Definition at line 302 of file LT_PMBus.h.

## ◆ LTC2978_CFGALL_PGOOD_OFF_UV

#define LTC2978_CFGALL_PGOOD_OFF_UV 0x0800

Definition at line 309 of file LT_PMBus.h.

## ◆ LTC2978_CFGALL_PMBUS_TIMO

#define LTC2978_CFGALL_PMBUS_TIMO 0x0002

Definition at line 301 of file LT_PMBus.h.

## ◆ LTC2978_CFGALL_SHORT_CYC_FAULT

#define LTC2978_CFGALL_SHORT_CYC_FAULT 0x1000

Definition at line 310 of file LT_PMBus.h.

## ◆ LTC2978_CFGALL_VIN_ON_CLR_FLT

#define LTC2978_CFGALL_VIN_ON_CLR_FLT 0x0040

Definition at line 306 of file LT_PMBus.h.

## ◆ LTC2978_CFGALL_VIN_SHARE

#define LTC2978_CFGALL_VIN_SHARE 0x0008

Definition at line 303 of file LT_PMBus.h.

## ◆ LTC2978_SFL_EEPROM

#define LTC2978_SFL_EEPROM 0x0001

Definition at line 334 of file LT_PMBus.h.

## ◆ LTC2978_SFL_RAM

#define LTC2978_SFL_RAM 0x0002

Definition at line 335 of file LT_PMBus.h.

## ◆ LTC2978_SMFR_DAC_CON

#define LTC2978_SMFR_DAC_CON 0x0008

Definition at line 328 of file LT_PMBus.h.

## ◆ LTC2978_SMFR_DAC_SAT

#define LTC2978_SMFR_DAC_SAT 0x0004

Definition at line 327 of file LT_PMBus.h.

## ◆ LTC2978_SMFR_DISCHARGE

#define LTC2978_SMFR_DISCHARGE 0x0080

Definition at line 332 of file LT_PMBus.h.

## ◆ LTC2978_SMFR_FAULT0_IN

#define LTC2978_SMFR_FAULT0_IN 0x0020

Definition at line 330 of file LT_PMBus.h.

## ◆ LTC2978_SMFR_FAULT1_IN

#define LTC2978_SMFR_FAULT1_IN 0x0040

Definition at line 331 of file LT_PMBus.h.

## ◆ LTC2978_SMFR_SERVO_TGT

#define LTC2978_SMFR_SERVO_TGT 0x0010

Definition at line 329 of file LT_PMBus.h.

## ◆ LTC2978_SMFR_VIN_EN

#define LTC2978_SMFR_VIN_EN 0x0002

Definition at line 326 of file LT_PMBus.h.

## ◆ LTC2978_SMFR_WATCH_DOG

#define LTC2978_SMFR_WATCH_DOG 0x0001

Definition at line 325 of file LT_PMBus.h.

## ◆ LTC2978_SW_BUSY

#define LTC2978_SW_BUSY 0x0080

Definition at line 292 of file LT_PMBus.h.

## ◆ LTC2978_SW_CML

#define LTC2978_SW_CML 0x0002

Definition at line 286 of file LT_PMBus.h.

## ◆ LTC2978_SW_FANS

#define LTC2978_SW_FANS 0x0400

Definition at line 293 of file LT_PMBus.h.

## ◆ LTC2978_SW_HIGH_BYTE

#define LTC2978_SW_HIGH_BYTE 0x0001

Definition at line 285 of file LT_PMBus.h.

## ◆ LTC2978_SW_INPUT

#define LTC2978_SW_INPUT 0x2000

Definition at line 296 of file LT_PMBus.h.

## ◆ LTC2978_SW_IOUT

#define LTC2978_SW_IOUT 0x4000

Definition at line 297 of file LT_PMBus.h.

## ◆ LTC2978_SW_IOUT_OC

#define LTC2978_SW_IOUT_OC 0x0010

Definition at line 289 of file LT_PMBus.h.

## ◆ LTC2978_SW_MFR

#define LTC2978_SW_MFR 0x1000

Definition at line 295 of file LT_PMBus.h.

## ◆ LTC2978_SW_OFF

#define LTC2978_SW_OFF 0x0040

Definition at line 291 of file LT_PMBus.h.

## ◆ LTC2978_SW_PGOODB

#define LTC2978_SW_PGOODB 0x0800

Definition at line 294 of file LT_PMBus.h.

## ◆ LTC2978_SW_TEMP

#define LTC2978_SW_TEMP 0x0004

Definition at line 287 of file LT_PMBus.h.

## ◆ LTC2978_SW_VIN_UV

#define LTC2978_SW_VIN_UV 0x0008

Definition at line 288 of file LT_PMBus.h.

## ◆ LTC2978_SW_VOUT

#define LTC2978_SW_VOUT 0x8000

Definition at line 298 of file LT_PMBus.h.

## ◆ LTC2978_SW_VOUT_OV

#define LTC2978_SW_VOUT_OV 0x0020

Definition at line 290 of file LT_PMBus.h.

## ◆ LTC3880_CFGALL_CLK_STR

#define LTC3880_CFGALL_CLK_STR 0x0002

Definition at line 168 of file LT_PMBus.h.

## ◆ LTC3880_CFGALL_EFL

#define LTC3880_CFGALL_EFL 0x0080

Definition at line 171 of file LT_PMBus.h.

## ◆ LTC3880_CFGALL_IGNORE_RCFG

#define LTC3880_CFGALL_IGNORE_RCFG 0x0040

Definition at line 170 of file LT_PMBus.h.

## ◆ LTC3880_CFGALL_MASK_PLL_FLT

#define LTC3880_CFGALL_MASK_PLL_FLT 0x0004

Definition at line 169 of file LT_PMBus.h.

## ◆ LTC3880_CFGALL_RUN_CLR

#define LTC3880_CFGALL_RUN_CLR 0x0001

Definition at line 167 of file LT_PMBus.h.

## ◆ LTC3880_SMFR_EXT_GPIO

#define LTC3880_SMFR_EXT_GPIO 0x0001

Definition at line 173 of file LT_PMBus.h.

## ◆ LTC3880_SMFR_FAULT_LOG

#define LTC3880_SMFR_FAULT_LOG 0x0008

Definition at line 175 of file LT_PMBus.h.

## ◆ LTC3880_SMFR_NVM_CRC

#define LTC3880_SMFR_NVM_CRC 0x0020

Definition at line 177 of file LT_PMBus.h.

## ◆ LTC3880_SMFR_PLL_UNLOCK

#define LTC3880_SMFR_PLL_UNLOCK 0x0010

Definition at line 176 of file LT_PMBus.h.

## ◆ LTC3880_SMFR_TEMP_FAULT

#define LTC3880_SMFR_TEMP_FAULT 0x0080

Definition at line 179 of file LT_PMBus.h.

## ◆ LTC3880_SMFR_TEMP_WARN

#define LTC3880_SMFR_TEMP_WARN 0x0040

Definition at line 178 of file LT_PMBus.h.

## ◆ LTC3880_SMFR_VDD_UV_OV

#define LTC3880_SMFR_VDD_UV_OV 0x0004

Definition at line 174 of file LT_PMBus.h.

## ◆ LTC3880_SW_BUSY

#define LTC3880_SW_BUSY 0x0080

Definition at line 158 of file LT_PMBus.h.

## ◆ LTC3880_SW_CML

#define LTC3880_SW_CML 0x0002

Definition at line 153 of file LT_PMBus.h.

## ◆ LTC3880_SW_INPUT

#define LTC3880_SW_INPUT 0x2000

Definition at line 161 of file LT_PMBus.h.

## ◆ LTC3880_SW_IOUT_OC

#define LTC3880_SW_IOUT_OC 0x0010

Definition at line 155 of file LT_PMBus.h.

## ◆ LTC3880_SW_IOUT_POUT

#define LTC3880_SW_IOUT_POUT 0x4000

Definition at line 162 of file LT_PMBus.h.

## ◆ LTC3880_SW_MFR

#define LTC3880_SW_MFR 0x1000

Definition at line 160 of file LT_PMBus.h.

## ◆ LTC3880_SW_NONE

#define LTC3880_SW_NONE 0x0001

Definition at line 152 of file LT_PMBus.h.

## ◆ LTC3880_SW_OFF

#define LTC3880_SW_OFF 0x0040

Definition at line 157 of file LT_PMBus.h.

## ◆ LTC3880_SW_PGOODB

#define LTC3880_SW_PGOODB 0x0800

Definition at line 159 of file LT_PMBus.h.

## ◆ LTC3880_SW_TEMP

#define LTC3880_SW_TEMP 0x0004

Definition at line 154 of file LT_PMBus.h.

## ◆ LTC3880_SW_VOUT

#define LTC3880_SW_VOUT 0x8000

Definition at line 163 of file LT_PMBus.h.

## ◆ LTC3880_SW_VOUT_OV

#define LTC3880_SW_VOUT_OV 0x0020

Definition at line 156 of file LT_PMBus.h.

## ◆ LTC3882_CFGALL_255MS_TMO

#define LTC3882_CFGALL_255MS_TMO 0x0008

Definition at line 184 of file LT_PMBus.h.

## ◆ LTC3882_CFGALL_CLK_STR

#define LTC3882_CFGALL_CLK_STR 0x0002

Definition at line 182 of file LT_PMBus.h.

## ◆ LTC3882_CFGALL_DISABLE_SYNC

#define LTC3882_CFGALL_DISABLE_SYNC 0x0010

Definition at line 185 of file LT_PMBus.h.

## ◆ LTC3882_CFGALL_EFL

#define LTC3882_CFGALL_EFL 0x0080

Definition at line 187 of file LT_PMBus.h.

## ◆ LTC3882_CFGALL_IGNORE_RCFG

#define LTC3882_CFGALL_IGNORE_RCFG 0x0040

Definition at line 186 of file LT_PMBus.h.

## ◆ LTC3882_CFGALL_PEC

#define LTC3882_CFGALL_PEC 0x0004

Definition at line 183 of file LT_PMBus.h.

## ◆ LTC3882_CFGALL_RUN_CLR_RISE

#define LTC3882_CFGALL_RUN_CLR_RISE 0x0001

Definition at line 181 of file LT_PMBus.h.

## ◆ LTC3882_SMFR_EXT_GPIO

#define LTC3882_SMFR_EXT_GPIO 0x0001

Definition at line 189 of file LT_PMBus.h.

## ◆ LTC3882_SMFR_FAULT_LOG

#define LTC3882_SMFR_FAULT_LOG 0x0008

Definition at line 191 of file LT_PMBus.h.

## ◆ LTC3882_SMFR_NVM_CRC

#define LTC3882_SMFR_NVM_CRC 0x0020

Definition at line 193 of file LT_PMBus.h.

## ◆ LTC3882_SMFR_PLL_UNLOCK

#define LTC3882_SMFR_PLL_UNLOCK 0x0010

Definition at line 192 of file LT_PMBus.h.

## ◆ LTC3882_SMFR_SHORT_CYCLE

#define LTC3882_SMFR_SHORT_CYCLE 0x0002

Definition at line 190 of file LT_PMBus.h.

## ◆ LTC3882_SMFR_TEMP_FAULT

#define LTC3882_SMFR_TEMP_FAULT 0x0080

Definition at line 195 of file LT_PMBus.h.

## ◆ LTC3882_SMFR_TEMP_WARN

#define LTC3882_SMFR_TEMP_WARN 0x0040

Definition at line 194 of file LT_PMBus.h.

## ◆ LTC3883_CFGALL_CLK_STR

#define LTC3883_CFGALL_CLK_STR 0x0002

Definition at line 197 of file LT_PMBus.h.

## ◆ LTC3883_CFGALL_EFL

#define LTC3883_CFGALL_EFL 0x0080

Definition at line 201 of file LT_PMBus.h.

## ◆ LTC3883_CFGALL_IGNORE_RCFG

#define LTC3883_CFGALL_IGNORE_RCFG 0x0040

Definition at line 200 of file LT_PMBus.h.

## ◆ LTC3883_CFGALL_MASK_PLL_ULOCK

#define LTC3883_CFGALL_MASK_PLL_ULOCK 0x0008

Definition at line 199 of file LT_PMBus.h.

## ◆ LTC3883_CFGALL_PEC

#define LTC3883_CFGALL_PEC 0x0004

Definition at line 198 of file LT_PMBus.h.

## ◆ LTC3883_SMFR_EXT_GPIO

#define LTC3883_SMFR_EXT_GPIO 0x0001

Definition at line 219 of file LT_PMBus.h.

## ◆ LTC3883_SMFR_FAULT_LOG

#define LTC3883_SMFR_FAULT_LOG 0x0008

Definition at line 221 of file LT_PMBus.h.

## ◆ LTC3883_SMFR_NVM_CRC

#define LTC3883_SMFR_NVM_CRC 0x0020

Definition at line 223 of file LT_PMBus.h.

## ◆ LTC3883_SMFR_PLL_UNLOCK

#define LTC3883_SMFR_PLL_UNLOCK 0x0010

Definition at line 222 of file LT_PMBus.h.

## ◆ LTC3883_SMFR_TEMP_FAULT

#define LTC3883_SMFR_TEMP_FAULT 0x0080

Definition at line 225 of file LT_PMBus.h.

## ◆ LTC3883_SMFR_TEMP_WARN

#define LTC3883_SMFR_TEMP_WARN 0x0040

Definition at line 224 of file LT_PMBus.h.

## ◆ LTC3883_SMFR_VDD_UV_OV

#define LTC3883_SMFR_VDD_UV_OV 0x0004

Definition at line 220 of file LT_PMBus.h.

## ◆ LTC3887_CFGALL_255MS_TMO

#define LTC3887_CFGALL_255MS_TMO 0x0008

Definition at line 206 of file LT_PMBus.h.

## ◆ LTC3887_CFGALL_CLK_STR

#define LTC3887_CFGALL_CLK_STR 0x0002

Definition at line 204 of file LT_PMBus.h.

## ◆ LTC3887_CFGALL_DISABLE_SYNC

#define LTC3887_CFGALL_DISABLE_SYNC 0x0010

Definition at line 207 of file LT_PMBus.h.

## ◆ LTC3887_CFGALL_EFL

#define LTC3887_CFGALL_EFL 0x0080

Definition at line 209 of file LT_PMBus.h.

## ◆ LTC3887_CFGALL_IGNORE_RCFG

#define LTC3887_CFGALL_IGNORE_RCFG 0x0040

Definition at line 208 of file LT_PMBus.h.

## ◆ LTC3887_CFGALL_PEC

#define LTC3887_CFGALL_PEC 0x0004

Definition at line 205 of file LT_PMBus.h.

## ◆ LTC3887_CFGALL_RUN_CLR_RISE

#define LTC3887_CFGALL_RUN_CLR_RISE 0x0001

Definition at line 203 of file LT_PMBus.h.

## ◆ LTC3887_SMFR_EXT_GPIO

#define LTC3887_SMFR_EXT_GPIO 0x0001

Definition at line 211 of file LT_PMBus.h.

## ◆ LTC3887_SMFR_FAULT_LOG

#define LTC3887_SMFR_FAULT_LOG 0x0008

Definition at line 213 of file LT_PMBus.h.

## ◆ LTC3887_SMFR_NVM_CRC

#define LTC3887_SMFR_NVM_CRC 0x0020

Definition at line 215 of file LT_PMBus.h.

## ◆ LTC3887_SMFR_PLL_UNLOCK

#define LTC3887_SMFR_PLL_UNLOCK 0x0010

Definition at line 214 of file LT_PMBus.h.

## ◆ LTC3887_SMFR_SHORT_CYCLE

#define LTC3887_SMFR_SHORT_CYCLE 0x0002

Definition at line 212 of file LT_PMBus.h.

## ◆ LTC3887_SMFR_TEMP_FAULT

#define LTC3887_SMFR_TEMP_FAULT 0x0080

Definition at line 217 of file LT_PMBus.h.

## ◆ LTC3887_SMFR_TEMP_WARN

#define LTC3887_SMFR_TEMP_WARN 0x0040

Definition at line 216 of file LT_PMBus.h.

## ◆ MFR_ADDRESS

#define MFR_ADDRESS 0xE6

Definition at line 133 of file LT_PMBus.h.

## ◆ MFR_COMMON

#define MFR_COMMON 0xEF

Definition at line 141 of file LT_PMBus.h.

## ◆ MFR_COMPARE_USER_ALL

#define MFR_COMPARE_USER_ALL 0xF0

Definition at line 74 of file LT_PMBus.h.

## ◆ MFR_CONFIG_ALL

#define MFR_CONFIG_ALL 0xD1

Definition at line 129 of file LT_PMBus.h.

## ◆ MFR_CONFIG_LTC2974

#define MFR_CONFIG_LTC2974 0xD0

Definition at line 128 of file LT_PMBus.h.

## ◆ MFR_EE_DATA

#define MFR_EE_DATA 0xBF

Definition at line 127 of file LT_PMBus.h.

## ◆ MFR_EE_ERASE

#define MFR_EE_ERASE 0xBE

Definition at line 126 of file LT_PMBus.h.

## ◆ MFR_EE_UNLOCK

#define MFR_EE_UNLOCK 0xBD

Definition at line 125 of file LT_PMBus.h.

## ◆ MFR_EEPROM_STATUS

#define MFR_EEPROM_STATUS 0xF1

Definition at line 148 of file LT_PMBus.h.

## ◆ MFR_FAULT_LOG

#define MFR_FAULT_LOG 0xEE

Definition at line 140 of file LT_PMBus.h.

## ◆ MFR_FAULT_LOG_CLEAR

#define MFR_FAULT_LOG_CLEAR 0xEC

Definition at line 137 of file LT_PMBus.h.

## ◆ MFR_FAULT_LOG_RESTORE

#define MFR_FAULT_LOG_RESTORE 0xEB

Definition at line 136 of file LT_PMBus.h.

## ◆ MFR_FAULT_LOG_STATUS

#define MFR_FAULT_LOG_STATUS 0xED

Definition at line 139 of file LT_PMBus.h.

## ◆ MFR_FAULT_LOG_STORE

#define MFR_FAULT_LOG_STORE 0xEA

Definition at line 135 of file LT_PMBus.h.

## ◆ MFR_MODEL

#define MFR_MODEL 0x9A

Definition at line 122 of file LT_PMBus.h.

## ◆ MFR_PADS

#define MFR_PADS 0xE5

Definition at line 132 of file LT_PMBus.h.

## ◆ MFR_RAIL_ADDRESS

#define MFR_RAIL_ADDRESS 0xFA

Definition at line 149 of file LT_PMBus.h.

## ◆ MFR_READ_IIN

#define MFR_READ_IIN 0xED

Definition at line 138 of file LT_PMBus.h.

## ◆ MFR_RESET

#define MFR_RESET 0xFD

Definition at line 150 of file LT_PMBus.h.

## ◆ MFR_SPARE_0

#define MFR_SPARE_0 0xF7

Definition at line 142 of file LT_PMBus.h.

## ◆ MFR_SPARE_1

#define MFR_SPARE_1 0xF8

Definition at line 143 of file LT_PMBus.h.

## ◆ MFR_SPARE_2

#define MFR_SPARE_2 0xF9

Definition at line 144 of file LT_PMBus.h.

## ◆ MFR_SPARE_3

#define MFR_SPARE_3 0xFA

Definition at line 145 of file LT_PMBus.h.

## ◆ MFR_SPECIAL_ID

#define MFR_SPECIAL_ID 0xE7

Definition at line 134 of file LT_PMBus.h.

## ◆ MFR_TEMP_1_GAIN

#define MFR_TEMP_1_GAIN 0xF8

Definition at line 146 of file LT_PMBus.h.

## ◆ MFR_TEMP_1_OFFSET

#define MFR_TEMP_1_OFFSET 0xF9

Definition at line 147 of file LT_PMBus.h.

## ◆ MFR_WATCHDOG_T

#define MFR_WATCHDOG_T 0xE3

Definition at line 131 of file LT_PMBus.h.

## ◆ MFR_WATCHDOG_T_FIRST

#define MFR_WATCHDOG_T_FIRST 0xE2

Definition at line 130 of file LT_PMBus.h.

## ◆ ON_OFF_CONFIG

#define ON_OFF_CONFIG 0x02

Definition at line 67 of file LT_PMBus.h.

## ◆ OPERATION

#define OPERATION 0x01

Definition at line 66 of file LT_PMBus.h.

## ◆ OT_FAULT_LIMIT

#define OT_FAULT_LIMIT 0x4F

Definition at line 89 of file LT_PMBus.h.

## ◆ OT_WARN_LIMIT

#define OT_WARN_LIMIT 0x51

Definition at line 90 of file LT_PMBus.h.

## ◆ PAGE

#define PAGE 0x00

Definition at line 65 of file LT_PMBus.h.

## ◆ PAGE_PLUS_READ

#define PAGE_PLUS_READ 0x06

Definition at line 70 of file LT_PMBus.h.

## ◆ PAGE_PLUS_WRITE

#define PAGE_PLUS_WRITE 0x05

Definition at line 69 of file LT_PMBus.h.

## ◆ READ_DUTY_CYCLE

#define READ_DUTY_CYCLE 0x94

Definition at line 119 of file LT_PMBus.h.

## ◆ READ_IIN

#define READ_IIN 0x89

Definition at line 114 of file LT_PMBus.h.

## ◆ READ_IOUT

#define READ_IOUT 0x8C

Definition at line 116 of file LT_PMBus.h.

## ◆ READ_ITEMP

#define READ_ITEMP 0x8E

Definition at line 118 of file LT_PMBus.h.

## ◆ READ_OTEMP

#define READ_OTEMP 0x8D

Definition at line 117 of file LT_PMBus.h.

## ◆ READ_PIN

#define READ_PIN 0x97

Definition at line 121 of file LT_PMBus.h.

## ◆ READ_POUT

#define READ_POUT 0x96

Definition at line 120 of file LT_PMBus.h.

## ◆ READ_VIN

#define READ_VIN 0x88

Definition at line 113 of file LT_PMBus.h.

## ◆ READ_VOUT

#define READ_VOUT 0x8B

Definition at line 115 of file LT_PMBus.h.

## ◆ RESTORE_USER_ALL

#define RESTORE_USER_ALL 0x16

Definition at line 73 of file LT_PMBus.h.

## ◆ SMBALERT_MASK

#define SMBALERT_MASK 0x1B

Definition at line 75 of file LT_PMBus.h.

## ◆ STATUS_BYTE

#define STATUS_BYTE 0x78

Definition at line 105 of file LT_PMBus.h.

## ◆ STATUS_CML

#define STATUS_CML 0x7E

Definition at line 111 of file LT_PMBus.h.

## ◆ STATUS_CML_CMD_FAULT

#define STATUS_CML_CMD_FAULT 0x80

Definition at line 337 of file LT_PMBus.h.

## ◆ STATUS_CML_DATA_FAULT

#define STATUS_CML_DATA_FAULT 0x40

Definition at line 338 of file LT_PMBus.h.

## ◆ STATUS_CML_MEM_FAULT

#define STATUS_CML_MEM_FAULT 0x10

Definition at line 340 of file LT_PMBus.h.

## ◆ STATUS_CML_PEC_FAULT

#define STATUS_CML_PEC_FAULT 0x20

Definition at line 339 of file LT_PMBus.h.

## ◆ STATUS_CML_PMBUS_FAULT

#define STATUS_CML_PMBUS_FAULT 0x02

Definition at line 342 of file LT_PMBus.h.

## ◆ STATUS_CML_PROC_FAULT

#define STATUS_CML_PROC_FAULT 0x04

Definition at line 341 of file LT_PMBus.h.

## ◆ STATUS_CML_UNKNOWN_FAULT

#define STATUS_CML_UNKNOWN_FAULT 0x01

Definition at line 343 of file LT_PMBus.h.

## ◆ STATUS_INPUT

#define STATUS_INPUT 0x7C

Definition at line 109 of file LT_PMBus.h.

## ◆ STATUS_IOUT

#define STATUS_IOUT 0x7B

Definition at line 108 of file LT_PMBus.h.

## ◆ STATUS_MFR_SPECIFIC

#define STATUS_MFR_SPECIFIC 0x80

Definition at line 112 of file LT_PMBus.h.

## ◆ STATUS_TEMP

#define STATUS_TEMP 0X7D

Definition at line 110 of file LT_PMBus.h.

## ◆ STATUS_VOUT

#define STATUS_VOUT 0x7A

Definition at line 107 of file LT_PMBus.h.

## ◆ STATUS_WORD

#define STATUS_WORD 0x79

Definition at line 106 of file LT_PMBus.h.

## ◆ STORE_USER_ALL

#define STORE_USER_ALL 0x15

Definition at line 72 of file LT_PMBus.h.

## ◆ SUCCESS

#define SUCCESS 1

Definition at line 62 of file LT_PMBus.h.

## ◆ TOFF_DELAY

#define TOFF_DELAY 0x64

Definition at line 101 of file LT_PMBus.h.

## ◆ TOFF_FALL

#define TOFF_FALL 0x65

Definition at line 102 of file LT_PMBus.h.

## ◆ TOFF_MAX_WARN_LIMIT

#define TOFF_MAX_WARN_LIMIT 0x66

Definition at line 103 of file LT_PMBus.h.

## ◆ TON_DELAY

#define TON_DELAY 0x60

Definition at line 97 of file LT_PMBus.h.

## ◆ TON_MAX_FAULT_LIMIT

#define TON_MAX_FAULT_LIMIT 0x62

Definition at line 99 of file LT_PMBus.h.

## ◆ TON_MAX_FAULT_RESPONSE

#define TON_MAX_FAULT_RESPONSE 0x63

Definition at line 100 of file LT_PMBus.h.

## ◆ TON_RISE

#define TON_RISE 0x61

Definition at line 98 of file LT_PMBus.h.

## ◆ USER_DATA_03

#define USER_DATA_03 0xB3

Definition at line 123 of file LT_PMBus.h.

## ◆ USER_DATA_04

#define USER_DATA_04 0xB4

Definition at line 124 of file LT_PMBus.h.

## ◆ UT_FAULT_LIMIT

#define UT_FAULT_LIMIT 0x53

Definition at line 91 of file LT_PMBus.h.

## ◆ UT_WARN_LIMIT

#define UT_WARN_LIMIT 0x52

Definition at line 92 of file LT_PMBus.h.

## ◆ VIN_OV_FAULT_LIMIT

#define VIN_OV_FAULT_LIMIT 0x55

Definition at line 93 of file LT_PMBus.h.

## ◆ VIN_OV_WARN_LIMIT

#define VIN_OV_WARN_LIMIT 0x57

Definition at line 94 of file LT_PMBus.h.

## ◆ VIN_UV_FAULT_LIMIT

#define VIN_UV_FAULT_LIMIT 0x59

Definition at line 96 of file LT_PMBus.h.

## ◆ VIN_UV_WARN_LIMIT

#define VIN_UV_WARN_LIMIT 0x58

Definition at line 95 of file LT_PMBus.h.

## ◆ VOUT_COMMAND

#define VOUT_COMMAND 0x21

Definition at line 77 of file LT_PMBus.h.

## ◆ VOUT_MARGIN_HIGH

#define VOUT_MARGIN_HIGH 0x25

Definition at line 79 of file LT_PMBus.h.

## ◆ VOUT_MARGIN_LOW

#define VOUT_MARGIN_LOW 0x26

Definition at line 80 of file LT_PMBus.h.

## ◆ VOUT_MAX

#define VOUT_MAX 0x24

Definition at line 78 of file LT_PMBus.h.

## ◆ VOUT_MODE

#define VOUT_MODE 0x20

Definition at line 76 of file LT_PMBus.h.

## ◆ VOUT_OV_FAULT_LIMIT

#define VOUT_OV_FAULT_LIMIT 0x40

Definition at line 81 of file LT_PMBus.h.

## ◆ VOUT_OV_FAULT_RESPONSE

#define VOUT_OV_FAULT_RESPONSE 0x41

Definition at line 82 of file LT_PMBus.h.

## ◆ VOUT_OV_WARN_LIMIT

#define VOUT_OV_WARN_LIMIT 0x42

Definition at line 83 of file LT_PMBus.h.

## ◆ VOUT_UV_FAULT_LIMIT

#define VOUT_UV_FAULT_LIMIT 0x44

Definition at line 85 of file LT_PMBus.h.

## ◆ VOUT_UV_FAULT_RESPONSE

#define VOUT_UV_FAULT_RESPONSE 0x45

Definition at line 86 of file LT_PMBus.h.

## ◆ VOUT_UV_WARN_LIMIT

#define VOUT_UV_WARN_LIMIT 0x43

Definition at line 84 of file LT_PMBus.h.

## ◆ WRITE_PROTECT

#define WRITE_PROTECT 0x10

Definition at line 71 of file LT_PMBus.h.

## Enumeration Type Documentation

## ◆ PsmDeviceType

enum PsmDeviceType

Enumerator
LTC3880 |
LTC3882 |
LTC3882_1 |
LTC3883 |
LTC3884 |
LTC3886 |
LTC3887 |
LTM4675 |
LTM4676 |
LTM4676A |
LTM4677 |
LTC2974 |
LTC2975 |
LTC2977 |
LTC2978 |
LTC2980 |
LTM2987 |
LTCUnknown |

Definition at line 345 of file LT_PMBus.h.