| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Data Fields
t_RECORD_PMBUS_READ_BYTE_LOOP_MASK Struct Reference

## Detailed Description

Definition at line 248 of file record_type_definitions.h.

## Data Fields
tRecordHeaderLengthAndType | baseRecordHeader
tRecordHeaderAddressAndCommandWithOptionalPEC | detailedRecordHeader
uint8_t | byteMask
uint8_t | expectedDataByte

## Field Documentation

## ◆ baseRecordHeader

tRecordHeaderLengthAndType t_RECORD_PMBUS_READ_BYTE_LOOP_MASK::baseRecordHeader

Definition at line 250 of file record_type_definitions.h.

## ◆ byteMask

uint8_t t_RECORD_PMBUS_READ_BYTE_LOOP_MASK::byteMask

Definition at line 252 of file record_type_definitions.h.

## ◆ detailedRecordHeader

tRecordHeaderAddressAndCommandWithOptionalPEC t_RECORD_PMBUS_READ_BYTE_LOOP_MASK::detailedRecordHeader

Definition at line 251 of file record_type_definitions.h.

## ◆ expectedDataByte

uint8_t t_RECORD_PMBUS_READ_BYTE_LOOP_MASK::expectedDataByte

Definition at line 253 of file record_type_definitions.h.

The documentation for this struct was generated from the following file:

- record_type_definitions.h