Functions | Context

The following lists the presently defined 3 character peripheral abbreviations.

Adc | Analog to Digital converter
--- | ---
Bga | Bandgap reference
Dac | Digital to Analog converter
Cmp | Comparator
Com | UART communication
Fee | Flash Eprom
Fio | Fast interrupt requests
Gio | GPIO ports
I2c | I2C
Irq | Interrupt requests
Pla | Programmable logic array
Pll | Phase locked loop
Psm | Power supply monitor
Pwm | Pulse width monitor
Spi | Serial peripheral interface
Spm | Serial port multiplexer
Swi | Software interrupt
Tcn | Timer/counter n.
Xme | External memory

For function names the leading character must be capital and the other characters lower case. File names should use the same cases although Windows messes this up. MMR names use all 3 characters upper case.