For compatibility with operating systems earlier than Windows 10, manually update the demo board driver so that it uses the DC2985A.inf file in this directory.

To do so, open Device Manager, right-click the board under Ports (COM & LPT) and select Properties. Under the Driver tab, select Update Driver and then manually browse your computer to point to the DC2985A.inf file.

A restart may be required.