Date:					2020-11-10
Name:					TMC2300-IOT-REF v4.0
Layers:					4
PCB Width:				25,4mm
PCB Height:				50,8mm
PCB Thickness:			1,6mm

Outer Layer Copper:		35µm (end)
Inner Layer Copper:		35µm

Silk Screen Top:		required (black)
Silk Screen Bottom:		required (black)
Solder Mask Top:		white
Solder Mask Bottom:		white
UL logo:				required (not for protos / pool services)