Date:				2020-09-02
Name:				TMC4671-LEV-REF-B_V10

Base:				FR4
Layers:				6
PCB Width:			51mm
PCB Height:			33mm
PCB Thickness:			1.6mm

Outer Layer Copper:		35µm (end)
Inner Layer Copper:		35µm

Silk Screen Top:		required (black)
Silk Screen Bottom:		required (black)
Solder Mask Top:		white
Solder Mask Bottom:		white
UL logo:			required (not for protos / pool services)