Date:				2020-09-02
Name:				TMC4671-LEV-REF-B_V10

Base:				Aluminium
Layers:				1
PCB Width:			80mm
PCB Height:			35mm
PCB Thickness:			1.6mm

Outer Layer Copper:		70µm (end)
Inner Layer Copper:		-

Silk Screen Top:		required (black)
Silk Screen Bottom:		none
Solder Mask Top:		white
Solder Mask Bottom:		none
UL logo:			required (not for protos / pool services)