Date:				2020-01-24
Name:				TMC2226-Eval v1.2
Layers:				4
PCB Width:			55mm
PCB Height:			85mm
PCB Thickness:		1,6mm

Outer Layer Copper:	35µm (end)
Inner Layer Copper:	35µm

Silk Screen Top:	required (black)
Silk Screen Bottom:	required (black)
Solder Mask Top:	white
Solder Mask Bottom:	white
UL logo:			required (not for protos / pool services)