Date:				2019-09-27
Name:				TMC4671+TMC6100-BOB_V10
Layers:				4
PCB Width:			50.8mm
PCB Height:			38.1mm
PCB Thickness:			1.55mm

Outer Layer Copper:		35µm (end)
Inner Layer Copper:		35µm

Silk Screen Top:		required (black)
Silk Screen Bottom:		required (black)
Solder Mask Top:		white
Solder Mask Bottom:		white
UL logo:			required (not for protos / pool services)