Date:					2019-09-11
Name:					TMC6100-EVAL v1.2
Layers:					4
PCB Width:				55mm
PCB Height:				85mm
PCB Thickness:			1,6mm

Outer Layer Copper:		35µm (end)
Inner Layer Copper:		35µm

Silk Screen Top:		required (black)
Silk Screen Bottom:		required (black)
Solder Mask Top:		white
Solder Mask Bottom:		white
UL logo:				required (not for protos / pool services)