Date:					2020-06-05
Name:					TMC6140-EVAL v1.1
Layers:					4
PCB Width:				79mm
PCB Height:				85mm
PCB Thickness:			1,6mm

Outer Layer Copper:		35µm
Inner Layer Copper:		70µm

Silk Screen Top:		required (black)
Silk Screen Bottom:		required (black)
Solder Mask Top:		white
Solder Mask Bottom:		white
UL logo:				required (not for protos / pool services)