Date:				2019-01-03
Name:				TMCM-0013-6A v1.0
Layers:				2
PCB Width:			55mm
PCB Height:			85mm
PCB Thickness:		1,6mm

Outer Layer Copper:		35µm (end)
Inner Layer Copper:		35µm

Silk Screen Top:		required (black)
Silk Screen Bottom:		required (black)
Solder Mask Top:		white
Solder Mask Bottom:		white
UL logo:			required (not for protos / pool services)