Board dimensions: 22.000 x 16.000 mm

Gerber Import Information
Units: Metric (mm)
Digit format: 4.3
Integer: 4
Decimal: 3
Mode: Absolute, Reference to relative origin
Zero suppression: Leading

Top Silk Screen:	DS9481P-300 - RevA.GTO
Top Solder Mask:	DS9481P-300 - RevA.GTS
Top Metal:		DS9481P-300 - RevA.GTL
Top Paste Mask: 	DS9481P-300 - RevA.GTP

Bottom Silk Screen:	DS9481P-300 - RevA.GBO
Bottom Metal:		DS9481P-300 - RevA.GBL
Bottom Solder Mask:	DS9481P-300 - RevA.GBS
Bottom Paste Mask:	DS9481P-300 - RevA.GBP

Board Outline:		DS9481P-300 - RevA.GKO
Mechanical Info:	DS9481P-300 - RevA.GM31
Top Assembly:		DS9481P-300 - RevA.GM15
Bottom Assembly:	DS9481P-300 - RevA.GM16

Drill Import Information
Units: Metric (mm)
Digit format: 4.3
Integer: 4
Decimal: 3
Mode: Absolute, Reference to relative origin
Zero suppression: None

ASCII drill file (Round Holes):	DS9481P-300 - RevA - RoundHoles.TXT
ASCII drill file (Slot Holes):	DS9481P-300 - RevA - SlotHoles.TXT

Drill Position file:	DS9481P-300 - RevA.GG1
Drill Symbol file:	DS9481P-300 - RevA.GD1

IPC-D-356 Netlist file:	DS9481P-300 - RevA.net
