Date:				2023-03-14
Name:				Landungsbrücke_V30
Layers:				4
PCB Width:			55mm
PCB Height:			85mm
PCB Thickness:			1.6mm

Outer Layer Copper:		35µm (end)
Inner Layer Copper:		35µm

Silk Screen Top:		required (black)
Silk Screen Bottom:		required (black)
Solder Mask Top:		white
Solder Mask Bottom:		white
UL logo:			required (not for protos / pool services)