Design Name:max14690_evkit_a

1) VIA_CHECK
-------------
<font color="66CC00">No_Error</font>

2) NPTH_HOLE_TO_COPPER
-----------------------
NPTH Hole to Copper: <font color="66CC00">No_Error</font> , no NPTH hole present in this design.

3) HOLE TOLERANCE CHECK
------------------------
DFM minimum allowed Tolerance for
NPTH hole : is +/-1mil or +2/-0 mils or +0/-2mil.
PTH hole : is +/-2mil or +4/-0 mils or +0/-4mil.

<font color="66CC00">No_Error</font> 

4) DRILL_CHART CHECK
---------------------
<font color="66CC00">No_Error</font> 

5) DUPLICATE_DRILL CHECK
-------------------------
<font color="66CC00">No_Error</font> 

6) DIRECT_ATTACH_PLATING CHECK
-------------------------------
Feinmetall DUT needs a special type of plating called 'Direct Attach Plating'
Refer to the latest Fab notes template for this instruction.

<font color="66CC00">No_Error</font> : No Feinmetall parts present in Design.

7) STACKUP_FILM CHECK
----------------------
<font color="66CC00">No_Error</font> 

8) COUNTER SINK CHECK
----------------------
<font color="66CC00">No_Error</font> 

9) TOPHAT ETCH VIOLATION CHECK
-------------------------------
 <font color="66CC00">Design is not TOPHAT</font>

10) SHAPE_NO_NET_REPORT
-----------------------
<font color="66CC00">No_Error</font> 

11) SHAPE_ISLAND_REPORT
-----------------------
<font color="66CC00">No_Error</font> 

12) UNCONNECTED_NET_REPORT
--------------------------
<font color="66CC00">No_Error</font> 

13) UNPLACED_SYMBOL_REPORT
--------------------------
<font color="66CC00">No_Error</font> 

14) MISCELLANEOUS_CHECK
-----------------------
<font color="66CC00">No_Error</font> 

15) ARTWORK_CHECK
-----------------

16) INTENTIONAL_SHORT
---------------------
Design doesn't use Intentional short footprints. If design has manual intentional short, Please ensure you supply short report information with FAB Package.


 *** END OF REPORT*** 	Total FAB Check count :16.
