 
 ---------------------------------------------------------------------------------------
 Confidential Note:  THE INFORMATION CONTAINED IN THIS DOCUMENT IS PROPRIETARY TO ANALOG DEVICES.
 THE INFORMATION IN THIS DOCUMENT IS NOT TO BE SHOWN/REPRODUCED OR 
 DISCLOSED TO ANYONE OUTSIDE OF ADI WITHOUT PRIOR WRITTEN PERMISSION FROM ANALOG DEVICES.
 ***************************************************************************************
 Design Name	:	08_100019a
 Date		:	08/29/2025
 Layout Designer	:	MSELVAM
 Program version	:	2.0
 ***************************************************************************************
 NOTE:If "$NONE" present in NET_NAME; then the short at this location is intentional(Dummy pin in intentional short symbol).
 CAM_NET_SHORT_COUNT column indicates the CAM tool shorting count (for reference only).
 The * on the CAM_NET_SHORT_COUNT value indicates the net is shorted in two or more REFDES locations.

NOTE:Below Shorts are done physically without using dedicated short symbols.

SHORT_DESCRIPTION,CAM_NET_SHORT_COUNT
Nets ("PGND" "SGND") shorted at locations ((2365.07 1539.8) (2385.07 1539.8)) on layers ("L2_GND"),"2*"
Nets ("VIN" "_N135") shorted at locations ((1041.07 1352.0) (1041.0 1352.0)) on layers ("BOTTOM"),"1*"


Total Intentional Short locations reported(0+4):4
Total CAM net Short count reported:2

END OF FILE