
**Intentional Short Report**

1. PGND(top copper) short to AGND(inner layer2) by shorting Vias in Inner Layer2.



1. Short(PC Trace) on Top Layer at FB1 pins.

