
**Assembly Instructions for MAX32010 EVKIt**



1. Attach the fan to heatsink using longest screws provided with heatsink. These screws will not reach holes on PCB. Those holes are for different heatsink.

1. Remove the blue sticker and glue the heatsink on top of MAX32010 IC.



1. Fan in the BOM has male wires (blue circle). Connect a female header to this fan (orange circle). Something like below:

1. Connect female wires to J5. Connect red wire from fan to J5.2 Connect black wire from fan to J5.3 (marked in orange).

