|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ITEM** | **QTY** | **REFERENCE** | **PART DESCRIPTION** | **MANUFACTURER** | **PART NUMBER** |
| 1 | 1 | PCB | PCB | ANALOG DEVICES | 08\_051166b |
| 2 | 1 | C3 | CAP 10nF 50V CER X7R 0402 | MURATA | GCM155R71H103KA55D |
| 3 | 1 | C4 | CAP 4.7UF 50V CER X7R 1206 | SAMSUNG | CL31B475KBHNNNE |
| 4 | 1 | C5 | CAP 10UF 50V CER X5R 1206 | SAMSUNG | CL31A106MBHNNNE |
| 5 | 1 | INPUT | CONN MALE 3POS 2.54MM PITCH R/A | SULLINS | PBC03SBAN |
| 6 | 1 | OUTPUT | CONN FEMALE 3POS 2.54MM PITCH R/A | SULLINS | PPPC031LGBN-RC |
| 7 | 1 | P1 | CONN-PCB 3POS HEADER WIRE TO BRD WAFER ASSY STRAIGHT 2MM PITCH (Note ) | MOLEX | 53253-0370 |
| 8 | 2 | R1,R7 | RES TBD THICK FILM 0805 (Note ) | TBD0805 | TBD0805 |
| 9 | 1 | R2 | RES 100K 1% THICK FILM 0805 | PANASONIC | ERJ-6ENF1003V |
| 10 | 1 | R4 | RES 249K 1% THICK FILM 0805 | VISHAY | CRCW0805249KFKECC |
| 11 | 1 | R6 | RES 768K 1% THICK FILM 0805 | PANASONIC | ERJ-6ENF7683V |
| 12 | 1 | U1 | IC LOW NOISE LDO NEGATIVE MICPROWER REGULATOR | ANALOG DEVICES | LT1964EDD#PBF |