Date:					2024-06-20
Name:					TMCM-1690-COE-EVAL v1.0
Layers:					4
PCB Width:				130mm
PCB Height:				85mm
PCB Thickness:				1,6mm

Outer Layer Copper:		35µm (end)
Inner Layer Copper:		35µm

Silk Screen Top:		required (black)
Silk Screen Bottom:		none
Solder Mask Top:		white
Solder Mask Bottom:		white
UL logo:			required (not for protos / pool services)