Date:				2019-11-14
Name:				TMCM-1617-BB_V10
Layers:				4
PCB Width:			130mm
PCB Height:			85mm
PCB Thickness:			1.6mm

Outer Layer Copper:		35µm (end)
Inner Layer Copper:		35µm

Silk Screen Top:		required (black)
Silk Screen Bottom:		none
Solder Mask Top:		white
Solder Mask Bottom:		white
UL logo:			required (not for protos / pool services)