! Device:      HMC1019ALP4E								
! Description: 0.5 dB LSB GaAs MMIC 5-Bit Digital Attenuator								
! Frequency:   0.1 -  30 GHz								
! Ports:       								
! 	RF1	= Port 1						
!	RF2	= Port 2						
!								
! Vdd:          5 Volt
! Vee:          -5 Volt								
! Control:      0/+5 Volt control voltage																
!								
! Data:    Data was collected using a calibrated network analyzer with AFR software.								
!          Fixtures were calculated using AFR and fixturing was applied to collect 								
!          this Deembedded  S Parameter data of HMC1019ALP4E.								
!								
! Note:    Analog Devices supplies this data as a sample of measured data at the package pin								
!          for this product.  Your particular data for this product may vary.								
!          Data was taken at 25 degrees C.								
!          Analog Devices reserves the right to change this data at anytime.