
Testing combination 1
EMDMA Stream no = 0
Internal memory type = 0x0
External memory type = 0x0
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 1 passed

Cycles = 45746, Throughput = 358.151520


Testing combination 2
EMDMA Stream no = 0
Internal memory type = 0x1
External memory type = 0x1
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 2 passed

Cycles = 26037, Throughput = 629.258362


Testing combination 3
EMDMA Stream no = 0
Internal memory type = 0x0
External memory type = 0x1
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 3 passed

Cycles = 45718, Throughput = 358.370880


Testing combination 4
EMDMA Stream no = 0
Internal memory type = 0x1
External memory type = 0x0
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 4 passed

Cycles = 28500, Throughput = 574.877197


Testing combination 5
EMDMA Stream no = 0
Internal memory type = 0x2
External memory type = 0x2
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 5 passed

Cycles = 33602, Throughput = 487.590027


Testing combination 6
EMDMA Stream no = 0
Internal memory type = 0x0
External memory type = 0x2
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 6 passed

Cycles = 45727, Throughput = 358.300354


Testing combination 7
EMDMA Stream no = 0
Internal memory type = 0x2
External memory type = 0x0
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 7 passed

Cycles = 32873, Throughput = 498.402954


Testing combination 8
EMDMA Stream no = 0
Internal memory type = 0x1
External memory type = 0x2
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 8 passed

Cycles = 30958, Throughput = 529.233154


Testing combination 9
EMDMA Stream no = 0
Internal memory type = 0x2
External memory type = 0x1
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 9 passed

Cycles = 32768, Throughput = 500.000000


Testing combination 10
EMDMA Stream no = 0
Internal memory type = 0x0
External memory type = 0x0
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 10 passed

Cycles = 45717, Throughput = 358.378723


Testing combination 11
EMDMA Stream no = 0
Internal memory type = 0x1
External memory type = 0x1
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 11 passed

Cycles = 26036, Throughput = 629.282532


Testing combination 12
EMDMA Stream no = 0
Internal memory type = 0x0
External memory type = 0x1
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 12 passed

Cycles = 28499, Throughput = 574.897339


Testing combination 13
EMDMA Stream no = 0
Internal memory type = 0x1
External memory type = 0x0
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 13 passed

Cycles = 45710, Throughput = 358.433594


Testing combination 14
EMDMA Stream no = 0
Internal memory type = 0x2
External memory type = 0x2
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 14 passed

Cycles = 33609, Throughput = 487.488464


Testing combination 15
EMDMA Stream no = 0
Internal memory type = 0x0
External memory type = 0x2
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 15 passed

Cycles = 32781, Throughput = 499.801727


Testing combination 16
EMDMA Stream no = 0
Internal memory type = 0x2
External memory type = 0x0
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 16 passed

Cycles = 45726, Throughput = 358.308197


Testing combination 17
EMDMA Stream no = 0
Internal memory type = 0x1
External memory type = 0x2
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 17 passed

Cycles = 32917, Throughput = 497.736725


Testing combination 18
EMDMA Stream no = 0
Internal memory type = 0x2
External memory type = 0x1
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 18 passed

Cycles = 30965, Throughput = 529.113525


Testing combination 19
EMDMA Stream no = 1
Internal memory type = 0x0
External memory type = 0x0
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 19 passed

Cycles = 45721, Throughput = 358.347382


Testing combination 20
EMDMA Stream no = 1
Internal memory type = 0x1
External memory type = 0x1
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 20 passed

Cycles = 26034, Throughput = 629.330872


Testing combination 21
EMDMA Stream no = 1
Internal memory type = 0x0
External memory type = 0x1
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 21 passed

Cycles = 45709, Throughput = 358.441437


Testing combination 22
EMDMA Stream no = 1
Internal memory type = 0x1
External memory type = 0x0
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 22 passed

Cycles = 28496, Throughput = 574.957886


Testing combination 23
EMDMA Stream no = 1
Internal memory type = 0x2
External memory type = 0x2
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 23 passed

Cycles = 33910, Throughput = 483.161316


Testing combination 24
EMDMA Stream no = 1
Internal memory type = 0x0
External memory type = 0x2
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 24 passed

Cycles = 45716, Throughput = 358.386566


Testing combination 25
EMDMA Stream no = 1
Internal memory type = 0x2
External memory type = 0x0
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 25 passed

Cycles = 32598, Throughput = 502.607513


Testing combination 26
EMDMA Stream no = 1
Internal memory type = 0x1
External memory type = 0x2
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 26 passed

Cycles = 30954, Throughput = 529.301575


Testing combination 27
EMDMA Stream no = 1
Internal memory type = 0x2
External memory type = 0x1
Mode = 0
Buffer count = 4096
DMA copy started
Test combination 27 passed

Cycles = 32854, Throughput = 498.691193


Testing combination 28
EMDMA Stream no = 1
Internal memory type = 0x0
External memory type = 0x0
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 28 passed

Cycles = 45712, Throughput = 358.417908


Testing combination 29
EMDMA Stream no = 1
Internal memory type = 0x1
External memory type = 0x1
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 29 passed

Cycles = 26040, Throughput = 629.185852


Testing combination 30
EMDMA Stream no = 1
Internal memory type = 0x0
External memory type = 0x1
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 30 passed

Cycles = 28494, Throughput = 574.998230


Testing combination 31
EMDMA Stream no = 1
Internal memory type = 0x1
External memory type = 0x0
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 31 passed

Cycles = 45714, Throughput = 358.402252


Testing combination 32
EMDMA Stream no = 1
Internal memory type = 0x2
External memory type = 0x2
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 32 passed

Cycles = 33666, Throughput = 486.663116


Testing combination 33
EMDMA Stream no = 1
Internal memory type = 0x0
External memory type = 0x2
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 33 passed

Cycles = 32715, Throughput = 500.810028


Testing combination 34
EMDMA Stream no = 1
Internal memory type = 0x2
External memory type = 0x0
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 34 passed

Cycles = 45719, Throughput = 358.363037


Testing combination 35
EMDMA Stream no = 1
Internal memory type = 0x1
External memory type = 0x2
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 35 passed

Cycles = 32683, Throughput = 501.300385


Testing combination 36
EMDMA Stream no = 1
Internal memory type = 0x2
External memory type = 0x1
Mode = 1
Buffer count = 4096
DMA copy started
Test combination 36 passed

Cycles = 30956, Throughput = 529.267334

All done
