
Testing combination 1
MDMA Stream no = 0
Source memory type = 0x0
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1973.025024 MHz

Test combination 1 passed


Testing combination 2
MDMA Stream no = 0
Source memory type = 0x1
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1975.403904 MHz

Test combination 2 passed


Testing combination 3
MDMA Stream no = 0
Source memory type = 0x0
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1973.975936 MHz

Test combination 3 passed


Testing combination 4
MDMA Stream no = 0
Source memory type = 0x1
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1974.451712 MHz

Test combination 4 passed


Testing combination 5
MDMA Stream no = 0
Source memory type = 0x2
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1216.693888, Destination throughput=1209.151232 MHz

Test combination 5 passed


Testing combination 6
MDMA Stream no = 0
Source memory type = 0x0
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1968.284416 MHz

Test combination 6 passed


Testing combination 7
MDMA Stream no = 0
Source memory type = 0x2
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1815.602816, Destination throughput=1799.648512 MHz

Test combination 7 passed


Testing combination 8
MDMA Stream no = 0
Source memory type = 0x1
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1969.704192 MHz

Test combination 8 passed


Testing combination 9
MDMA Stream no = 0
Source memory type = 0x2
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1807.590528, Destination throughput=1792.560128 MHz

Test combination 9 passed


Testing combination 10
MDMA Stream no = 1
Source memory type = 0x0
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1973.025024 MHz

Test combination 10 passed


Testing combination 11
MDMA Stream no = 1
Source memory type = 0x1
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1975.403904 MHz

Test combination 11 passed


Testing combination 12
MDMA Stream no = 1
Source memory type = 0x0
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1973.975936 MHz

Test combination 12 passed


Testing combination 13
MDMA Stream no = 1
Source memory type = 0x1
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1974.451712 MHz

Test combination 13 passed


Testing combination 14
MDMA Stream no = 1
Source memory type = 0x2
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1235.409408, Destination throughput=1227.633792 MHz

Test combination 14 passed


Testing combination 15
MDMA Stream no = 1
Source memory type = 0x0
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1968.284416 MHz

Test combination 15 passed


Testing combination 16
MDMA Stream no = 1
Source memory type = 0x2
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1787.865600, Destination throughput=1772.392960 MHz

Test combination 16 passed


Testing combination 17
MDMA Stream no = 1
Source memory type = 0x1
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1969.704192 MHz

Test combination 17 passed


Testing combination 18
MDMA Stream no = 1
Source memory type = 0x2
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1794.916736, Destination throughput=1780.095616 MHz

Test combination 18 passed


Testing combination 19
MDMA Stream no = 2
Source memory type = 0x0
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1973.025024 MHz

Test combination 19 passed


Testing combination 20
MDMA Stream no = 2
Source memory type = 0x1
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1975.403904 MHz

Test combination 20 passed


Testing combination 21
MDMA Stream no = 2
Source memory type = 0x0
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1973.975936 MHz

Test combination 21 passed


Testing combination 22
MDMA Stream no = 2
Source memory type = 0x1
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1974.451712 MHz

Test combination 22 passed


Testing combination 23
MDMA Stream no = 2
Source memory type = 0x2
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1213.629568, Destination throughput=1206.124800 MHz

Test combination 23 passed


Testing combination 24
MDMA Stream no = 2
Source memory type = 0x0
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1968.284416 MHz

Test combination 24 passed


Testing combination 25
MDMA Stream no = 2
Source memory type = 0x2
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1790.992512, Destination throughput=1775.465984 MHz

Test combination 25 passed


Testing combination 26
MDMA Stream no = 2
Source memory type = 0x1
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1969.704192 MHz

Test combination 26 passed


Testing combination 27
MDMA Stream no = 2
Source memory type = 0x2
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1814.396416, Destination throughput=1799.253248 MHz

Test combination 27 passed


Testing combination 28
MDMA Stream no = 3
Source memory type = 0x0
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=3221.392128, Destination throughput=3177.657088 MHz

Test combination 28 passed


Testing combination 29
MDMA Stream no = 3
Source memory type = 0x1
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=3978.630400, Destination throughput=3919.617280 MHz

Test combination 29 passed


Testing combination 30
MDMA Stream no = 3
Source memory type = 0x0
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=3466.779392, Destination throughput=3421.888000 MHz

Test combination 30 passed


Testing combination 31
MDMA Stream no = 3
Source memory type = 0x1
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=3978.630400, Destination throughput=3912.129792 MHz

Test combination 31 passed


Testing combination 32
MDMA Stream no = 3
Source memory type = 0x2
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1587.289344, Destination throughput=1574.173696 MHz

Test combination 32 passed


Testing combination 33
MDMA Stream no = 3
Source memory type = 0x0
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=3468.247296, Destination throughput=3413.333248 MHz

Test combination 33 passed


Testing combination 34
MDMA Stream no = 3
Source memory type = 0x2
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=2782.608640, Destination throughput=2749.916160 MHz

Test combination 34 passed


Testing combination 35
MDMA Stream no = 3
Source memory type = 0x1
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=3965.149952, Destination throughput=3887.992320 MHz

Test combination 35 passed


Testing combination 36
MDMA Stream no = 3
Source memory type = 0x2
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=2915.302400, Destination throughput=2883.491840 MHz

Test combination 36 passed


Testing combination 37
MDMA Stream no = 4
Source memory type = 0x0
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1973.025024 MHz

Test combination 37 passed


Testing combination 38
MDMA Stream no = 4
Source memory type = 0x1
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1975.403904 MHz

Test combination 38 passed


Testing combination 39
MDMA Stream no = 4
Source memory type = 0x0
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1973.975936 MHz

Test combination 39 passed


Testing combination 40
MDMA Stream no = 4
Source memory type = 0x1
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1974.451712 MHz

Test combination 40 passed


Testing combination 41
MDMA Stream no = 4
Source memory type = 0x2
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1260.695552, Destination throughput=1252.599424 MHz

Test combination 41 passed


Testing combination 42
MDMA Stream no = 4
Source memory type = 0x0
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1968.284416 MHz

Test combination 42 passed


Testing combination 43
MDMA Stream no = 4
Source memory type = 0x2
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1805.200512, Destination throughput=1789.427712 MHz

Test combination 43 passed


Testing combination 44
MDMA Stream no = 4
Source memory type = 0x1
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1969.704192 MHz

Test combination 44 passed


Testing combination 45
MDMA Stream no = 4
Source memory type = 0x2
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1811.187328, Destination throughput=1796.097408 MHz

Test combination 45 passed


Testing combination 46
MDMA Stream no = 5
Source memory type = 0x0
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1973.025024 MHz

Test combination 46 passed


Testing combination 47
MDMA Stream no = 5
Source memory type = 0x1
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1975.403904 MHz

Test combination 47 passed


Testing combination 48
MDMA Stream no = 5
Source memory type = 0x0
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1973.975936 MHz

Test combination 48 passed


Testing combination 49
MDMA Stream no = 5
Source memory type = 0x1
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1974.451712 MHz

Test combination 49 passed


Testing combination 50
MDMA Stream no = 5
Source memory type = 0x2
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1227.817728, Destination throughput=1220.137088 MHz

Test combination 50 passed


Testing combination 51
MDMA Stream no = 5
Source memory type = 0x0
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1972.075136 MHz

Test combination 51 passed


Testing combination 52
MDMA Stream no = 5
Source memory type = 0x2
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1797.673856, Destination throughput=1782.031744 MHz

Test combination 52 passed


Testing combination 53
MDMA Stream no = 5
Source memory type = 0x1
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1973.500416 MHz

Test combination 53 passed


Testing combination 54
MDMA Stream no = 5
Source memory type = 0x2
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1801.231360, Destination throughput=1786.306176 MHz

Test combination 54 passed


Testing combination 55
MDMA Stream no = 6
Source memory type = 0x0
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1973.025024 MHz

Test combination 55 passed


Testing combination 56
MDMA Stream no = 6
Source memory type = 0x1
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1975.403904 MHz

Test combination 56 passed


Testing combination 57
MDMA Stream no = 6
Source memory type = 0x0
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1973.975936 MHz

Test combination 57 passed


Testing combination 58
MDMA Stream no = 6
Source memory type = 0x1
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1993.672448, Destination throughput=1974.451712 MHz

Test combination 58 passed


Testing combination 59
MDMA Stream no = 6
Source memory type = 0x2
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1230.769280, Destination throughput=1223.051648 MHz

Test combination 59 passed


Testing combination 60
MDMA Stream no = 6
Source memory type = 0x0
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1992.217856, Destination throughput=1968.284416 MHz

Test combination 60 passed


Testing combination 61
MDMA Stream no = 6
Source memory type = 0x2
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1796.491264, Destination throughput=1780.869504 MHz

Test combination 61 passed


Testing combination 62
MDMA Stream no = 6
Source memory type = 0x1
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1990.765440, Destination throughput=1967.811712 MHz

Test combination 62 passed


Testing combination 63
MDMA Stream no = 6
Source memory type = 0x2
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1809.586944, Destination throughput=1794.523520 MHz

Test combination 63 passed


Testing combination 64
MDMA Stream no = 7
Source memory type = 0x0
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=3268.954624, Destination throughput=3223.927552 MHz

Test combination 64 passed


Testing combination 65
MDMA Stream no = 7
Source memory type = 0x1
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=3978.630400, Destination throughput=3919.617280 MHz

Test combination 65 passed


Testing combination 66
MDMA Stream no = 7
Source memory type = 0x0
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=3466.779392, Destination throughput=3421.888000 MHz

Test combination 66 passed


Testing combination 67
MDMA Stream no = 7
Source memory type = 0x1
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=3978.630400, Destination throughput=3912.129792 MHz

Test combination 67 passed


Testing combination 68
MDMA Stream no = 7
Source memory type = 0x2
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=1630.248704, Destination throughput=1616.416768 MHz

Test combination 68 passed


Testing combination 69
MDMA Stream no = 7
Source memory type = 0x0
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=3468.247296, Destination throughput=3413.333248 MHz

Test combination 69 passed


Testing combination 70
MDMA Stream no = 7
Source memory type = 0x2
Destination memory type = 0x0
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=2917.378816, Destination throughput=2881.463296 MHz

Test combination 70 passed


Testing combination 71
MDMA Stream no = 7
Source memory type = 0x1
Destination memory type = 0x2
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=3965.149952, Destination throughput=3887.992320 MHz

Test combination 71 passed


Testing combination 72
MDMA Stream no = 7
Source memory type = 0x2
Destination memory type = 0x1
Buffer count = 512
MSIZE value = 32
DMA copy started


Source throughput=2904.964608, Destination throughput=2873.377792 MHz

Test combination 72 passed

All done
