DC718 Rev C2

Contact Information:

Board Designer:
  Eric Trelewicz
  email:  etrelewicz@gmail.com

COPY ALL CORRESPONDENCE TO the following person(s):
Mark Thoren
mthoren@linear.com 

Created with: EagleCad 4.16
Photo plots: gerber274x
drill file: Excellon

File Descriptions

DC718C2.sch	EagleCad Schematic
DC718C2.brd	EagleCad Board file

THe following files are all gerber274x format:
(DC718C2.gpi	photo plot information file)
{
   Coordinate Format : 2.4
   Coordinate Units  : Inch
   Data Mode         : Absolute
   Zero Suppression  : None
   End Of Block      : *
}

DC718C2.l1	Top copper, layer 1
DC718C2.l2	layer 2 copper, possitive
DC718C2.l3	layer 3 copper, possitive
DC718C2.l4	back, solder layer, layer4 copper

DC718C2.smt	soldermask top
DC718C2.smb	soldermask back

DC718C2.sst	silk screen top
DC718C2.ssb	silk screen back

DC718C2.spt	solder paste top
DC718C2.spb	solder paste back

DC718C2.ast	assembly top
DC718C2.asb	assembly back


DC718C2.FAB	Fabrication drawing (stackup information here!)

Additional log and drill files

DC718C2.dri	drill information file
DC718C2.drl	Tool code hole sizes
DC718C2.tap	drill file

Additional files in pdf/xls

0718C2.xls	   bill of material
DC718C2_AssyDwg.pdf
DC718C2_FabDwg.pdf
DC718C2_gerber1x.pdf
DC718C2_gerber2x.pdf
DC718C2_Schematic.pdf



