**QUALIFICATION RESULT FOR PCN 15\_0224   
REDUCTION OF BURN-IN FROM 160 TO 48 HOURS FOR OP200AZ/883 (5962-8859301MPA)**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| TEST | Reference Specification | Sample ID | Pre Burn-in Test Result | Post Burn-in Test Result (PDA) | | | Completion Date |
| 48 Hours | 96 Hours | 160 Hours |  |
| Burn-in | MIL-STD-883, TM1015 | 3 Lots |  |  |  |  |  |
| End Point Electrical | Readpoints:  0 hrs, 48 hrs,  96 hrs, 160 hrs | Lot 1 | 195/200 | 0% | 0% | 0% | 16-Apr-2015 |
| Lot 2 | 190/200 | 0% | 0% | 0% | 16-Apr-2015 |
| Lot 3 | 1489/1516 | 0% | 0% | 0% | 25-Nov-2014 |

X