(

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "ic_adi" )
( -FromCell "ADSP21565" )
( -FromVer "*" )
( -FromProp "WW_PN" "E033866" )
( -ToLib "ic_adi" )
( -ToCell "ADSP21565" )
( -ToVer "*" )
( -ToProp "VALUE" "ADSP-21565" )
( -ToProp "WW_PN" "E033866" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "LQFP120_14X14_PAD5_4X5_4" )
( -ToProp "HLM_STATUS" "RWC" )
( -ToProp "DESCRIPTION" "IC-ADI SHARC DSP, PRELIM" )
( -ToProp "MFG" "ANALOG DEVICES" )
( -ToProp "MFG_PN" "ADSP-21565" )
( -ToProp "AVE_COST" "N/A" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "N/A" )
( -ToProp "CASE" "QFP" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "121" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "www.analog.com" )
( -ToProp "TOL" "N/A" )
( -ToProp "PPM" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "N/A" )
( -ToProp "ALT_PN1" "E" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/899087" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "resistors" )
( -FromCell "RES" )
( -FromVer "*" )
( -FromProp "WW_PN" "E034570" )
( -ToLib "resistors" )
( -ToCell "RES" )
( -ToVer "*" )
( -ToProp "VALUE" "0" )
( -ToProp "WW_PN" "E034570" )
( -ToProp "WATTAGE" "1/20W" )
( -ToProp "TOL" "JUMPER" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "R0201" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "RES SMD 0 Ohm JUMPER 1/20W 0201" )
( -ToProp "MFG" "VISHAY" )
( -ToProp "MFG_PN" "CRCW02010000Z0ED" )
( -ToProp "AVE_COST" "USD 0.0043" )
( -ToProp "MFG_LEAD_TIME" "20 WEEKS" )
( -ToProp "EOL" "8.4 YEARS" )
( -ToProp "CASE" "0201" )
( -ToProp "JEDEC_REV" "A-01" )
( -ToProp "ALT_SYMBOLS" "(R0201NC)" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "www.vishay.com" )
( -ToProp "PPM" "JUMPER" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +155C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/369521" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "resistors" )
( -FromCell "RES" )
( -FromVer "*" )
( -FromProp "WW_PN" "E032279" )
( -ToLib "resistors" )
( -ToCell "RES" )
( -ToVer "*" )
( -ToProp "VALUE" "10K" )
( -ToProp "WW_PN" "E032279" )
( -ToProp "WATTAGE" "1/20W" )
( -ToProp "TOL" "5" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "R0201" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "RES SMD 10K Ohm 5% 1/20W 0201" )
( -ToProp "MFG" "PANASONIC" )
( -ToProp "MFG_PN" "ERJ-1GNJ103C" )
( -ToProp "AVE_COST" "USD 0.0043" )
( -ToProp "MFG_LEAD_TIME" "18 WEEKS" )
( -ToProp "EOL" "6.9 YEARS" )
( -ToProp "CASE" "0201" )
( -ToProp "JEDEC_REV" "A-01" )
( -ToProp "ALT_SYMBOLS" "(R0201NC)" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "industrial.panasonic.com/ww" )
( -ToProp "PPM" "+/- 200PPM" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/770239" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "resistors" )
( -FromCell "RES" )
( -FromVer "*" )
( -FromProp "WW_PN" "E021894" )
( -ToLib "resistors" )
( -ToCell "RES" )
( -ToVer "*" )
( -ToProp "VALUE" "330" )
( -ToProp "WW_PN" "E021894" )
( -ToProp "WATTAGE" "1/16W" )
( -ToProp "TOL" "1" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "R0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "RES SMD 330 Ohm 1% 1/16W 0402 AEC-Q200" )
( -ToProp "MFG" "VISHAY" )
( -ToProp "MFG_PN" "CRCW0402330RFKED" )
( -ToProp "AVE_COST" "N/A" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "N/A" )
( -ToProp "CASE" "0402" )
( -ToProp "JEDEC_REV" "B-00" )
( -ToProp "ALT_SYMBOLS" "(R0402L,R0402L_ALT)" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "www.vishayfoilresistors.com" )
( -ToProp "PPM" "+/- 100PPM" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +155C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/190915" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "resistors" )
( -FromCell "RES" )
( -FromVer "*" )
( -FromProp "WW_PN" "E003751" )
( -ToLib "resistors" )
( -ToCell "RES" )
( -ToVer "*" )
( -ToProp "VALUE" "10K" )
( -ToProp "WW_PN" "E003751" )
( -ToProp "WATTAGE" "1/10W" )
( -ToProp "TOL" "1" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "R0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "RES SMD 10K Ohm 1% 1/10W 0402 AEC-Q200" )
( -ToProp "MFG" "PANASONIC" )
( -ToProp "MFG_PN" "ERJ-2RKF1002X" )
( -ToProp "AVE_COST" "N/A" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "N/A" )
( -ToProp "CASE" "0402" )
( -ToProp "JEDEC_REV" "B-00" )
( -ToProp "ALT_SYMBOLS" "(R0402L,R0402L_ALT)" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "industrial.panasonic.com/ww" )
( -ToProp "PPM" "+/- 100PPM" )
( -ToProp "STOCKROOM_WL" "A003-0035-004" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "41816DG719" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "7000582" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +155C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/431273" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "diodes" )
( -FromCell "DIOLED" )
( -FromVer "*" )
( -FromProp "WW_PN" "E040428" )
( -ToLib "diodes" )
( -ToCell "DIOLED" )
( -ToVer "*" )
( -ToProp "VALUE" "SML-D14U2WT86C" )
( -ToProp "VOLTAGE" "2V" )
( -ToProp "TOL" "N/A" )
( -ToProp "WW_PN" "E040428" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "LED0603_A" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "LED RED 615NM AUTOMOTIVE" )
( -ToProp "MFG" "ROHM" )
( -ToProp "MFG_PN" "SML-D14U2WT86C" )
( -ToProp "AVE_COST" "USD 0.2496" )
( -ToProp "MFG_LEAD_TIME" "10 WEEKS" )
( -ToProp "EOL" "8.5 YEARS" )
( -ToProp "CASE" "0603" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "URL" "www.rohm.com" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-40C TO +100C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmbe-hlm.ad.analog.com/apps/hlm/attachments/1271369/download" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "capacitors" )
( -FromCell "CAP" )
( -FromVer "*" )
( -FromProp "WW_PN" "E033351" )
( -ToLib "capacitors" )
( -ToCell "CAP" )
( -ToVer "*" )
( -ToProp "VALUE" "10uF" )
( -ToProp "VOLTAGE" "10V" )
( -ToProp "TOL" "20" )
( -ToProp "WW_PN" "E033351" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "C0603" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "CAP CER 10uF 10V 20% X5R 0603 AEC-Q200" )
( -ToProp "MFG" "TAIYO YUDEN" )
( -ToProp "MFG_PN" "LMK107BBJ106MAHT" )
( -ToProp "AVE_COST" "N/A" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "7.5 YEARS" )
( -ToProp "CASE" "0603" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "URL" "www.taiyo-yuden.com" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +85C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/828645" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "capacitors" )
( -FromCell "CAP" )
( -FromVer "*" )
( -FromProp "WW_PN" "E028141" )
( -ToLib "capacitors" )
( -ToCell "CAP" )
( -ToVer "*" )
( -ToProp "VALUE" "0.1uF" )
( -ToProp "VOLTAGE" "16V" )
( -ToProp "TOL" "10" )
( -ToProp "WW_PN" "E028141" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "C0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "CAP CER 0.1uF 16V 10% X7R 0402 AEC-Q200" )
( -ToProp "MFG" "MURATA" )
( -ToProp "MFG_PN" "GCM155R71C104KA55D" )
( -ToProp "AVE_COST" "USD 0.0053" )
( -ToProp "MFG_LEAD_TIME" "16 WEEKS" )
( -ToProp "EOL" "6.4 YEARS" )
( -ToProp "CASE" "0402" )
( -ToProp "JEDEC_REV" "B-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "URL" "www.murata.com" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/437208" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "filters" )
( -FromCell "FLTR3P" )
( -FromVer "*" )
( -FromProp "WW_PN" "E011145" )
( -ToLib "filters" )
( -ToCell "FLTR3P" )
( -ToVer "*" )
( -ToProp "VALUE" "4700pF" )
( -ToProp "WW_PN" "E011145" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "F2606" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "FLTR EMI (LC COMBINED TYPE) 2606" )
( -ToProp "MFG" "MURATA MANUFACTURING" )
( -ToProp "MFG_PN" "NFE61PT472C1H9L" )
( -ToProp "AVE_COST" "USD 0.5247" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "5.1 YEARS" )
( -ToProp "CASE" "2606" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "3" )
( -ToProp "VOLTAGE" "50V" )
( -ToProp "URL" "www.murata.com" )
( -ToProp "TOL" "-4" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "40602DG050" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-40C TO +85C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/18503" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "resistors" )
( -FromCell "RES" )
( -FromVer "*" )
( -FromProp "WW_PN" "E030866" )
( -ToLib "resistors" )
( -ToCell "RES" )
( -ToVer "*" )
( -ToProp "VALUE" "0" )
( -ToProp "WW_PN" "E030866" )
( -ToProp "WATTAGE" "1/5W" )
( -ToProp "TOL" "JUMPER" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "R0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "RES SMD 0 Ohm JUMPER 1/5W 0402 AEC-Q200" )
( -ToProp "MFG" "VISHAY" )
( -ToProp "MFG_PN" "CRCW04020000Z0EDHP" )
( -ToProp "AVE_COST" "USD 0.0297" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "7.3 YEARS" )
( -ToProp "CASE" "0402" )
( -ToProp "JEDEC_REV" "B-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "www.vishay.com" )
( -ToProp "PPM" "JUMPER" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +155C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/190915" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "resistors" )
( -FromCell "RES" )
( -FromVer "*" )
( -FromProp "WW_PN" "E004011" )
( -ToLib "resistors" )
( -ToCell "RES" )
( -ToVer "*" )
( -ToProp "VALUE" "10K" )
( -ToProp "WW_PN" "E004011" )
( -ToProp "WATTAGE" "1/20W" )
( -ToProp "TOL" "1" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "R0201" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "RES SMD 10K Ohm 1% 1/20W 0201" )
( -ToProp "MFG" "PANASONIC" )
( -ToProp "MFG_PN" "ERJ-1GNF1002C" )
( -ToProp "AVE_COST" "N/A" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "N/A" )
( -ToProp "CASE" "0201" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "industrial.panasonic.com/ww" )
( -ToProp "PPM" "+/- 200PPM" )
( -ToProp "STOCKROOM_WL" "A003-0081-004" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "7005859" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/431273" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "switches" )
( -FromCell "SWBCDROTARY6P" )
( -FromVer "*" )
( -FromProp "WW_PN" "E040089" )
( -ToLib "switches" )
( -ToCell "SWBCDROTARY6P" )
( -ToVer "*" )
( -ToProp "VALUE" "RDTAR10S1R" )
( -ToProp "WW_PN" "E040089" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "SWSMSQ394H268" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "SWITCH ROTARY DIP BCD 0.15A" )
( -ToProp "MFG" "E-SWITCH, INC." )
( -ToProp "MFG_PN" "RDTAR10S1R" )
( -ToProp "AVE_COST" "USD 3.9822" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "6.8 YEARS" )
( -ToProp "CASE" "N/A" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "6" )
( -ToProp "VOLTAGE" "42V" )
( -ToProp "URL" "www.e-switch.com" )
( -ToProp "TOL" "N/A" )
( -ToProp "PPM" "+/-N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "N/A" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmbe-hlm.ad.analog.com/apps/hlm/attachments/1260473/download" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "8" )
( -Save true )
( -HardProp true )
( -FromLib "conn_pcb" )
( -FromCell "CN10P" )
( -FromVer "*" )
( -FromProp "WW_PN" "E027236" )
( -ToLib "conn_pcb" )
( -ToCell "CN10P" )
( -ToVer "*" )
( -ToProp "VALUE" "SHF-105-01-L-D-TH-TR" )
( -ToProp "WW_PN" "E027236" )
( -ToProp "PACK_TYPE" "TH" )
( -ToProp "JEDEC_TYPE" "CNTHMHDR2X5L500W200H215" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "CONN-PCB SHROUDED AND EJECTOR IDC HDR VERT 1.27MM PITCH" )
( -ToProp "MFG" "SAMTEC INC." )
( -ToProp "MFG_PN" "SHF-105-01-L-D-TH-TR" )
( -ToProp "AVE_COST" "USD 1.383" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "7.2 YEARS" )
( -ToProp "CASE" "N/A" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "10" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "www.samtec.com" )
( -ToProp "TOL" "N/A" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "6003603" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/340160" )
)

( _globalModify
( -Scope "7" )
( -Save true )
( -HardProp true )
( -FromLib "capacitors" )
( -FromCell "CAP" )
( -FromVer "*" )
( -FromProp "WW_PN" "E035949" )
( -ToLib "capacitors" )
( -ToCell "CAP" )
( -ToVer "*" )
( -ToProp "VALUE" "10uF" )
( -ToProp "VOLTAGE" "25V" )
( -ToProp "TOL" "20" )
( -ToProp "WW_PN" "E035949" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "C0603" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "CAP CER 10uF 25V 20% X5R 0603 AEC-Q200" )
( -ToProp "MFG" "MURATA" )
( -ToProp "MFG_PN" "GRT188R61E106ME13D" )
( -ToProp "AVE_COST" "USD 0.1072" )
( -ToProp "MFG_LEAD_TIME" "38 WEEKS" )
( -ToProp "EOL" "11.7 YEARS" )
( -ToProp "CASE" "0603" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "URL" "www.murata.com" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +85C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmbe-hlm.ad.analog.com/apps/hlm2/Attachment/View/945130" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "7" )
( -Save true )
( -HardProp true )
( -FromLib "capacitors" )
( -FromCell "CAP" )
( -FromVer "*" )
( -FromProp "WW_PN" "E028142" )
( -ToLib "capacitors" )
( -ToCell "CAP" )
( -ToVer "*" )
( -ToProp "VALUE" "1000pF" )
( -ToProp "VOLTAGE" "25V" )
( -ToProp "TOL" "10" )
( -ToProp "WW_PN" "E028142" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "C0201" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "CAP CER 1000pF 25V 10% X7R 0201 AEC-Q200" )
( -ToProp "MFG" "MURATA" )
( -ToProp "MFG_PN" "GCM033R71E102KA03D" )
( -ToProp "AVE_COST" "USD 0.0054" )
( -ToProp "MFG_LEAD_TIME" "18 WEEKS" )
( -ToProp "EOL" "6.4 YEARS" )
( -ToProp "CASE" "0201" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "URL" "www.murata.com" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/437208" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "7" )
( -Save true )
( -HardProp true )
( -FromLib "capacitors" )
( -FromCell "CAP" )
( -FromVer "*" )
( -FromProp "WW_PN" "E039013" )
( -ToLib "capacitors" )
( -ToCell "CAP" )
( -ToVer "*" )
( -ToProp "VALUE" "0.47uF" )
( -ToProp "VOLTAGE" "25V" )
( -ToProp "TOL" "10" )
( -ToProp "WW_PN" "E039013" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "C0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "CAP CER 0.47uF 25V 10% X5R 0402" )
( -ToProp "MFG" "SAMSUNG" )
( -ToProp "MFG_PN" "CL05A474KA5NNNC" )
( -ToProp "AVE_COST" "USD 0.0654" )
( -ToProp "MFG_LEAD_TIME" "20 WEEKS" )
( -ToProp "EOL" "6.4 YEARS" )
( -ToProp "CASE" "0402" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "URL" "www.samsung.com" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +85C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmbe-hlm.ad.analog.com/apps/hlm/attachments/841422/download" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "7" )
( -Save true )
( -HardProp true )
( -FromLib "capacitors" )
( -FromCell "CAP" )
( -FromVer "*" )
( -FromProp "WW_PN" "E033317" )
( -ToLib "capacitors" )
( -ToCell "CAP" )
( -ToVer "*" )
( -ToProp "VALUE" "0.1uF" )
( -ToProp "VOLTAGE" "16V" )
( -ToProp "TOL" "5" )
( -ToProp "WW_PN" "E033317" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "C0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "CAP CER 0.1uF 16V 5% X7R 0402" )
( -ToProp "MFG" "KEMET" )
( -ToProp "MFG_PN" "C0402C104J4RACTU" )
( -ToProp "AVE_COST" "USD 0.0255" )
( -ToProp "MFG_LEAD_TIME" "37 WEEKS" )
( -ToProp "EOL" "7.5 YEARS" )
( -ToProp "CASE" "0402" )
( -ToProp "JEDEC_REV" "B-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "URL" "www.kemet.com" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/454643" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "7" )
( -Save true )
( -HardProp true )
( -FromLib "capacitors" )
( -FromCell "CAP" )
( -FromVer "*" )
( -FromProp "WW_PN" "E035952" )
( -ToLib "capacitors" )
( -ToCell "CAP" )
( -ToVer "*" )
( -ToProp "VALUE" "1uF" )
( -ToProp "VOLTAGE" "10V" )
( -ToProp "TOL" "10" )
( -ToProp "WW_PN" "E035952" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "C0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "CAP CER 1uF 10V 10% X7S 0402 AEC-Q200" )
( -ToProp "MFG" "MURATA" )
( -ToProp "MFG_PN" "GCM155C71A105KE38D" )
( -ToProp "AVE_COST" "USD 0.0205" )
( -ToProp "MFG_LEAD_TIME" "38 WEEKS" )
( -ToProp "EOL" "6.4 YEARS" )
( -ToProp "CASE" "0402" )
( -ToProp "JEDEC_REV" "B-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "URL" "www.murata.com" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmbe-hlm.ad.analog.com/apps/hlm2/Attachment/View/437208" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "7" )
( -Save true )
( -HardProp true )
( -FromLib "capacitors" )
( -FromCell "CAP" )
( -FromVer "*" )
( -FromProp "WW_PN" "E041210" )
( -ToLib "capacitors" )
( -ToCell "CAP" )
( -ToVer "*" )
( -ToProp "VALUE" "0.22uF" )
( -ToProp "VOLTAGE" "25V" )
( -ToProp "TOL" "10" )
( -ToProp "WW_PN" "E041210" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "C0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "CAP CER 0.22uF 25V 10% X7R 0402 AEC-Q200 LOW ESR" )
( -ToProp "MFG" "TDK" )
( -ToProp "MFG_PN" "CGA2B3X7R1E224K050BB" )
( -ToProp "AVE_COST" "USD 0.0801" )
( -ToProp "MFG_LEAD_TIME" "20 WEEKS" )
( -ToProp "EOL" "16.1 YEARS" )
( -ToProp "CASE" "0402" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "URL" "www.global.tdk.com" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmbe-hlm.ad.analog.com/apps/hlm/attachments/1308986/download" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "capacitors" )
( -FromCell "CAP" )
( -FromVer "*" )
( -FromProp "WW_PN" "E022721" )
( -ToLib "capacitors" )
( -ToCell "CAP" )
( -ToVer "*" )
( -ToProp "VALUE" "0.1uF" )
( -ToProp "VOLTAGE" "25V" )
( -ToProp "TOL" "10" )
( -ToProp "WW_PN" "E022721" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "C0201" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "CAP CER 0.1uF 25V 10% X5R 0201" )
( -ToProp "MFG" "MURATA" )
( -ToProp "MFG_PN" "GRM033R61E104KE14D" )
( -ToProp "AVE_COST" "USD 0.007" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "7.5 YEARS" )
( -ToProp "CASE" "0201" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "URL" "www.murata.com" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +85C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/463003" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "ic_other" )
( -FromCell "ICSI5356X" )
( -FromVer "*" )
( -FromProp "WW_PN" "E041435" )
( -ToLib "ic_other" )
( -ToCell "ICSI5356X" )
( -ToVer "*" )
( -ToProp "VALUE" "SI5356A-B03215-GM" )
( -ToProp "WW_PN" "E041435" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "QFN24_4X4_PAD2_5X2_5" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "IC I2C PROGRAMMABLE, ANY-FREQ 1-200MHZ, QUAD FREQ 8-OUTPUT CLK GEN" )
( -ToProp "MFG" "SILICON LABS" )
( -ToProp "MFG_PN" "SI5356A-B03215-GM" )
( -ToProp "AVE_COST" "USD 8.392" )
( -ToProp "MFG_LEAD_TIME" "6 WEEKS" )
( -ToProp "EOL" "6 YEARS" )
( -ToProp "CASE" "24QFN" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "25" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "www.silabs.com" )
( -ToProp "TOL" "N/A" )
( -ToProp "PPM" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-40C TO +85C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmbe-hlm.ad.analog.com/apps/hlm/attachments/1322666/download" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "crystals" )
( -FromCell "XTAL" )
( -FromVer "*" )
( -FromProp "WW_PN" "E040906" )
( -ToLib "crystals" )
( -ToCell "XTAL" )
( -ToVer "*" )
( -ToProp "VALUE" "25MEGHZ" )
( -ToProp "WW_PN" "E040906" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "YSML236W138H55" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "IC CRYSTAL MICRO MINIATURE, 18PF" )
( -ToProp "MFG" "ABRACON CORP." )
( -ToProp "MFG_PN" "ABM7-25.000MHZ-D2Y-T" )
( -ToProp "AVE_COST" "USD 0.5623" )
( -ToProp "MFG_LEAD_TIME" "23 WEEKS" )
( -ToProp "EOL" "5.1 YEARS" )
( -ToProp "CASE" "N/A" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "www.abracon.com" )
( -ToProp "TOL" "20PPM" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-40C TO +85C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmbe-hlm.ad.analog.com/apps/hlm/attachments/1295153/download" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "resistors" )
( -FromCell "RES" )
( -FromVer "*" )
( -FromProp "WW_PN" "E029449" )
( -ToLib "resistors" )
( -ToCell "RES" )
( -ToVer "*" )
( -ToProp "VALUE" "1.5K" )
( -ToProp "WW_PN" "E029449" )
( -ToProp "WATTAGE" "1/20W" )
( -ToProp "TOL" "0.1" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "R0201" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "RES SMD 1.5K Ohm 0.1% 1/20W 0201 AEC-Q200 HIGH RELIABILITY" )
( -ToProp "MFG" "PANASONIC" )
( -ToProp "MFG_PN" "ERA-1AEB152C" )
( -ToProp "AVE_COST" "USD 0.1233" )
( -ToProp "MFG_LEAD_TIME" "18 WEEKS" )
( -ToProp "EOL" "8 YEARS" )
( -ToProp "CASE" "0201" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "industrial.panasonic.com/ww" )
( -ToProp "PPM" "+/- 25PPM" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +155C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/445472" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "resistors" )
( -FromCell "RES" )
( -FromVer "*" )
( -FromProp "WW_PN" "E007239" )
( -ToLib "resistors" )
( -ToCell "RES" )
( -ToVer "*" )
( -ToProp "VALUE" "100" )
( -ToProp "WW_PN" "E007239" )
( -ToProp "WATTAGE" "1/20W" )
( -ToProp "TOL" "1" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "R0201" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "RES SMD 100 Ohm 1% 1/20W 0201" )
( -ToProp "MFG" "PANASONIC" )
( -ToProp "MFG_PN" "ERJ-1GNF1000C" )
( -ToProp "AVE_COST" "USD 0.0068" )
( -ToProp "MFG_LEAD_TIME" "8 WEEKS" )
( -ToProp "EOL" "8.1 YEARS" )
( -ToProp "CASE" "0201" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "(R0201NC)" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "industrial.panasonic.com/ww" )
( -ToProp "PPM" "+/- 200PPM" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/431273" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "resistors" )
( -FromCell "RES" )
( -FromVer "*" )
( -FromProp "WW_PN" "E007920" )
( -ToLib "resistors" )
( -ToCell "RES" )
( -ToVer "*" )
( -ToProp "VALUE" "2.2K" )
( -ToProp "WW_PN" "E007920" )
( -ToProp "WATTAGE" "1/20W" )
( -ToProp "TOL" "1" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "R0201" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "RES SMD 2.2K Ohm 1% 1/20W 0201" )
( -ToProp "MFG" "PANASONIC" )
( -ToProp "MFG_PN" "ERJ-1GNF2201C" )
( -ToProp "AVE_COST" "USD 0.0072" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "8.3 YEARS" )
( -ToProp "CASE" "0201" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "industrial.panasonic.com/ww" )
( -ToProp "PPM" "+/- 200PPM" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "41816JH1376" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "7006540" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/431273" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "resistors" )
( -FromCell "RES" )
( -FromVer "*" )
( -FromProp "WW_PN" "E003751" )
( -ToLib "resistors" )
( -ToCell "RES" )
( -ToVer "*" )
( -ToProp "VALUE" "10K" )
( -ToProp "WW_PN" "E003751" )
( -ToProp "WATTAGE" "1/10W" )
( -ToProp "TOL" "1" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "R0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "RES SMD 10K Ohm 1% 1/10W 0402 AEC-Q200" )
( -ToProp "MFG" "PANASONIC" )
( -ToProp "MFG_PN" "ERJ-2RKF1002X" )
( -ToProp "AVE_COST" "N/A" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "N/A" )
( -ToProp "CASE" "0402" )
( -ToProp "JEDEC_REV" "B-00" )
( -ToProp "ALT_SYMBOLS" "(R0402L,R0402L_ALT)" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "industrial.panasonic.com/ww" )
( -ToProp "PPM" "+/- 100PPM" )
( -ToProp "STOCKROOM_WL" "A003-0035-004" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "41816DG719" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "7000582" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +155C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/431273" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "resistors" )
( -FromCell "RES" )
( -FromVer "*" )
( -FromProp "WW_PN" "E027299" )
( -ToLib "resistors" )
( -ToCell "RES" )
( -ToVer "*" )
( -ToProp "VALUE" "3.01K" )
( -ToProp "WW_PN" "E027299" )
( -ToProp "WATTAGE" "1/10W" )
( -ToProp "TOL" "1" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "R0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "RES SMD 3.01K Ohm 1% 1/10W 0402 AEC-Q200" )
( -ToProp "MFG" "PANASONIC" )
( -ToProp "MFG_PN" "ERJ-2RKF3011X" )
( -ToProp "AVE_COST" "USD 0.0024" )
( -ToProp "MFG_LEAD_TIME" "10 WEEKS" )
( -ToProp "EOL" "6.9 YEARS" )
( -ToProp "CASE" "0402" )
( -ToProp "JEDEC_REV" "B-00" )
( -ToProp "ALT_SYMBOLS" "(R0402L)" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "industrial.panasonic.com/ww" )
( -ToProp "PPM" "+/- 100PPM" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +155C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/534404" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "resistors" )
( -FromCell "RES" )
( -FromVer "*" )
( -FromProp "WW_PN" "E003452" )
( -ToLib "resistors" )
( -ToCell "RES" )
( -ToVer "*" )
( -ToProp "VALUE" "33" )
( -ToProp "WW_PN" "E003452" )
( -ToProp "WATTAGE" "1/10W" )
( -ToProp "TOL" "5" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "R0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "RES SMD 33 Ohm 5% 1/10W 0402 AEC-Q200" )
( -ToProp "MFG" "PANASONIC" )
( -ToProp "MFG_PN" "ERJ-2GEJ330X" )
( -ToProp "AVE_COST" "N/A" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "N/A" )
( -ToProp "CASE" "0402" )
( -ToProp "JEDEC_REV" "B-00" )
( -ToProp "ALT_SYMBOLS" "(R0402L)" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "industrial.panasonic.com/ww" )
( -ToProp "PPM" "+/- 200PPM" )
( -ToProp "STOCKROOM_WL" "A003-0021-016" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "41816DG861" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +155C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/454650" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "ic_other" )
( -FromCell "ICIS25LP512" )
( -FromVer "*" )
( -FromProp "WW_PN" "E040080" )
( -ToLib "ic_other" )
( -ToCell "ICIS25LP512" )
( -ToVer "*" )
( -ToProp "VALUE" "IS25LP512M-RMLA3" )
( -ToProp "WW_PN" "E040080" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "SO16WB" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "IC 512MB SERIAL FLASH MEMORY 133MHZ MULTI I/O SPI & QUAD I/O QPI DTR INTERFACE" )
( -ToProp "MFG" "ISSI" )
( -ToProp "MFG_PN" "IS25LP512M-RMLA3" )
( -ToProp "AVE_COST" "N/A" )
( -ToProp "MFG_LEAD_TIME" "N/A" )
( -ToProp "EOL" "N/A" )
( -ToProp "CASE" "SOIC" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "16" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "www.issi.com" )
( -ToProp "TOL" "N/A" )
( -ToProp "PPM" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-40C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmbe-hlm.ad.analog.com/apps/hlm/pcb/lprs/LPR-055077?taskId=48992#" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "capacitors" )
( -FromCell "CAP" )
( -FromVer "*" )
( -FromProp "WW_PN" "E030894" )
( -ToLib "capacitors" )
( -ToCell "CAP" )
( -ToVer "*" )
( -ToProp "VALUE" "0.01uF" )
( -ToProp "VOLTAGE" "25V" )
( -ToProp "TOL" "10" )
( -ToProp "WW_PN" "E030894" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "C0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "CAP CER 0.01uF 25V 10% X7R 0402 AEC-Q200" )
( -ToProp "MFG" "MURATA" )
( -ToProp "MFG_PN" "GCM155R71E103KA37D" )
( -ToProp "AVE_COST" "USD 0.0164" )
( -ToProp "MFG_LEAD_TIME" "38 WEEKS" )
( -ToProp "EOL" "6.4 YEARS" )
( -ToProp "CASE" "0402" )
( -ToProp "JEDEC_REV" "B-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "2" )
( -ToProp "URL" "www.murata.com" )
( -ToProp "PPM" "N/A" )
( -ToProp "WATTAGE" "N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-55C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmfg.analog.com/wwmfg/apps/Hlm/Attachment/View/475631" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "ic_ttl" )
( -FromCell "741G125" )
( -FromVer "*" )
( -FromProp "WW_PN" "E040081" )
( -ToLib "ic_ttl" )
( -ToCell "741G125" )
( -ToVer "*" )
( -ToProp "VALUE" "74CBTLV1G125DBVRQ1" )
( -ToProp "WW_PN" "E040081" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "SOT23-5L-2" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "IC-TTL LOW VOLT SINGLE FET BUS SWITCH" )
( -ToProp "MFG" "TEXAS INSTRUMENTS" )
( -ToProp "MFG_PN" "74CBTLV1G125DBVRQ1" )
( -ToProp "AVE_COST" "USD 0.581" )
( -ToProp "MFG_LEAD_TIME" "6 WEEKS" )
( -ToProp "EOL" "10 YEARS" )
( -ToProp "CASE" "SOT23-5" )
( -ToProp "JEDEC_REV" "A-00" )
( -ToProp "ALT_SYMBOLS" "()" )
( -ToProp "PIN_COUNT" "5" )
( -ToProp "VOLTAGE" "N/A" )
( -ToProp "URL" "www.ti.com" )
( -ToProp "TOL" "N/A" )
( -ToProp "PPM" "+/-N/A" )
( -ToProp "STOCKROOM_WL" "N/A" )
( -ToProp "STOCKROOM_LK" "N/A" )
( -ToProp "STOCKROOM_GT" "N/A" )
( -ToProp "STOCKROOM_SJ" "N/A" )
( -ToProp "STOCKROOM_GBO" "N/A" )
( -ToProp "STOCKROOM_NSH" "N/A" )
( -ToProp "ROHS" "Y" )
( -ToProp "OTR" "-40C TO +125C" )
( -ToProp "ALT_PN1" "N/A" )
( -ToProp "ALT_PN2" "N/A" )
( -ToProp "SCD" "http://wwmbe-hlm.ad.analog.com/apps/hlm/attachments/1260251/download" )
( -ToProp "IMPLEMENTATION" "N/A" )
)

( _globalModify
( -Scope "3" )
( -Save true )
( -HardProp true )
( -FromLib "capacitors" )
( -FromCell "CAP" )
( -FromVer "*" )
( -FromProp "WW_PN" "E033384" )
( -ToLib "capacitors" )
( -ToCell "CAP" )
( -ToVer "*" )
( -ToProp "VALUE" "27pF" )
( -ToProp "VOLTAGE" "50V" )
( -ToProp "TOL" "5" )
( -ToProp "WW_PN" "E033384" )
( -ToProp "PACK_TYPE" "SM" )
( -ToProp "JEDEC_TYPE" "C0402" )
( -ToProp "HLM_STATUS" "REL" )
( -ToProp "DESCRIPTION" "CAP CER 27pF 50V 5% C0G 0402 AEC-Q200" )
( -ToProp "