5BWIN.EXE
Rev 1.00
January 1996
Barry Long

The 5B Custom program (SW-5B) assists users of 5B Series of signal 
conditioners in selecting Custom-ranged 5B modules. The user enters 
the desired module's input and output ranges and the program will 
verify whether or not the custom ranges are valid.
The program also lists general 5B module information, ranges, 
application notes, etc...
Requires Windows 3.1 or later.

TO INSTALL 5B CUSTOM:

1) Create a temporary directory on your hard disk. For example:
        
        md c:\5btemp

2) Copy 5BCUSTOM.ZIP into the temporary directory

3) Using PKUNZIP, unzip 5BCUSTOM.ZIP into the new 
   directory. For example:

        pkunzip 5BCUSTOM.ZIP

4) Go into Windows, select the File/Run menu, and run SETUP:

        c:\5btemp\setup.exe

   Setup will properly install 5BCUSTOM as a Windows application,
   into the directory of your choice. After this has been done you 
   may delete the temporary directory and its contents.
