| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Files
LTC6950: 1.4GHz Low Phase Noise, Low Jitter PLL with Clock Distribution
RF, Silicon Oscillators, PLL Synthesizers, and VCOs

LTC6950: 1.4GHz Low Phase Noise, Low Jitter PLL with Clock Distribution. More...

## Files
file | LTC6950.cpp
| Library for LTC6950: 1.4GHz Low Phase Noise, Low Jitter PLL with Clock Distribution.
file | LTC6950.h
| LTC6950: 1.4GHz Low Phase Noise, Low Jitter PLL with Clock Distribution.
file | DC1795A.ino
| DC1795A LTC6950: 1.4GHz Low Phase Noise, Low Jitter PLL with Clock Distribution.

## Detailed Description

LTC6950: 1.4GHz Low Phase Noise, Low Jitter PLL with Clock Distribution.

    The LTC®6950 is a low phase noise integer-N frequency
    synthesizer core with clock distribution. The LTC6950
    delivers the low phase noise clock signals demanded in
    high frequency, high resolution data acquisition systems.

    The frequency synthesizer contains a full low noise PLL core
    with a programmable reference divider (R), a programmable
    feedback divider (N), a phase/frequency detector (PFD)
    and a low noise charge pump (CP). The clock distribution
    section of the LTC6950 delivers up to five outputs based on
    the VCO input. Each output is individually programmed to
    divide the VCO input frequency by any integer from 1 to 63
    and to delay the output by 0 to 63 VCO clock cycles. Four
    of the outputs feature very low noise, low skew LVPECL
    logic signals capable of operation up to 1.4GHz. The fifth
    output is selectable as either an LVDS (800MHz) or CMOS
    (250MHz) logic type. This output is also programmed to
    produce an output signal based on either the VCO input
    or the reference divider output.

http://www.linear.com/product/LTC6950

http://www.linear.com/product/LTC6950#demoboards

Copyright 2018(c) Analog Devices, Inc.

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

- Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.
- Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.
- Neither the name of Analog Devices, Inc. nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.
- The use of this software may or may not infringe the patent rights of one or more patent holders. This license does not release you from the requirement that you obtain separate licenses from these patent holders to use this software.
- Use of the software either in source or binary form, must be run on or directly connected to an Analog Devices Inc. component.

THIS SOFTWARE IS PROVIDED BY ANALOG DEVICES "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, NON-INFRINGEMENT, MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL ANALOG DEVICES BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, INTELLECTUAL PROPERTY RIGHTS, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.